Data/hora: 13/06/2024 05:29:43

Provedor de dados: | 5
País: | France
Título: | Ultra Wide Swath Sea interferometric multibeam echo sounder with sea bottom imaging system.
Autores: | Hammerstad, E; Pohner, F.
Data: | 1990-12
Ano: | 1990
Palavras-chave: | Ocean floor; Multibeam sonar; Bathymetry; Signal processing; Sonar imagery; Imaging techniques; Side scan sonar; Echosounding; Echosounders.
Resumo: | The SIMRAD EM12 is a new full ocean depth multibeam echo sounder, operating at 13 kHz. By use of interferometric signal processing techniques it will achieve an ultra wide swath geometry of 150 degrees, corresponding to 7.5 times the depth of water. The system will in addition to the bathymetry produce a fully corrected sidescan sonar image of the seafloor, on to the depth soundings, the EM12 has the capability to generate a sidescan image of the seabed.
Tipo: | Text
Idioma: | Inglês
Identificador: | http://archimer.ifremer.fr/doc/1990/acte-1141.pdf
Editor: | Actes de colloques. Ifremer. Brest [ACTES COLLOQ. IFREMER.]. 1991
Relação: | http://archimer.ifremer.fr/doc/00000/1141/
Formato: | application/pdf