Data/hora: 12/06/2024 12:20:35

Provedor de dados: 	5	
País: 	France	
Título: 	Improving gear selectivity of whiting ( Merlangius merlangus ) on board French demersal trawlers in the English Channel and North Sea	
Autores: 	Vogel, Camille; Kopp, Dorothee; Morandeau, Fabien; Morfin, Marie; Mehault, Sonia.	
Data: 	2017-09	
Ano: 	2017	
Palavras-chave: 	Square mesh; Sorting grids; Fishing gear technology; Merlangius merlangus; Catch comparison; GLMM.	
Resumo: 	In the English Channel and Southern Bight, French demersal trawlers target a mix of demersal species including whiting (Merlangius merlangus). The discard ban to be implemented in January 2016 motivated fishermen to look for technical measures to reduce unwanted catches of undersized individuals (&lt;27 cm). From 2008–2014, 18 different gear configurations were tested for bycatch reduction on board fleets of vessels of 16–20 m and 20–24 m. Selective devices tested included grids, square mesh panels (SMP), square mesh cylinders (SMC), various combinations of these devices and large mesh trawls. Using the catch comparison method, our results focus on six devices that proved efficient to reduce catches of undersized whiting, equally divided between the two vessel size groups. Large mesh trawls are not adequate to improve whiting size selectivity with losses of commercial size fish. The mandatory 80-mm SMP was efficient at letting undersized whiting escape from the trawl for both vessel length classes. Its efficiency was enhanced when it was positioned 6–9 m ahead of the codline compared with that placed at 12–15 m. The most appropriate bar spacing for whiting size-selectivity was found in a flexigrid with 23 mm bar spacing, but this required a large portion of square mesh netting to be installed ahead of it (SMP and SMC) to limit catches of undersized individuals. The most promising device tested was an 80 mm SMC, either 2 m long and used alone or 1 m long and used in association with the mandatory SMP; these setups allowed significant escapes of fish up to 25 cm in length. For both SMP and SMC, a mesh size equal to or larger than 100 mm led to losses of commercial size whiting.	
Tipo: 	Text	
Idioma: 	Inglês	
Identificador: 	http://archimer.ifremer.fr/doc/00384/49553/50079.pdf

DOI:10.1016/j.fishres.2017.04.013

http://archimer.ifremer.fr/doc/00384/49553/	
Editor: 	Elsevier Science Bv	
Formato: 	application/pdf	
Fonte: 	Fisheries Research (0165-7836) (Elsevier Science Bv), 2017-09 , Vol. 193 , P. 207-216	
Fonte: 	2017 Elsevier B.V. All rights reserved.

info:eu-repo/semantics/openAccess

restricted use