Data/hora: 03/06/2024 02:19:12

Provedor de dados: 	58	
País: 	Brazil	
Título: 	Nickel biosorption by Acinetobacter baumannii and Pseudomonas aeruginosa isolated from industrial wastewater	
Autores: 	Rodríguez,Carlos E.; Quesada,Adolfo.	
Data: 	2006-12-01	
Ano: 	2006	
Palavras-chave: 	Biosorption; Nickel; Acinetobacter baumannii; Pseudomonas aeruginosa; Wastewater treatment.	
Resumo: 	Nickel biosorption ability was evaluated in two bacterial strains: Acinetobacter baumannii UCR-2971 and Pseudomonas aeruginosa UCR-2957, resulting in greatest adsorption at pH 4.5 and a residence time of 100 minutes. Biosorption isotherms showed that the process follows the Langmuir model. The maximum adsorption rates (Nmax) were 8.8 and 5.7 mg·g-1 for A. baumannii and P. aeruginosa, respectively; however, affinity constants suggest that P. aeruginosa (K=1.28) has higher affinity for nickel than A. baumannii (K=0.68). It is suggested that both strains could be used for wastewater treatment, as long as the concentration of Ni2+ is within the range of mg·L-1.	
Tipo: 	Info:eu-repo/semantics/article	
Idioma: 	Inglês	
Identificador: 	http://www.scielo.br/scielo.php?script=sci_arttext&pid=S1517-83822006000400012	
Editor: 	Sociedade Brasileira de Microbiologia	
Relação: 	10.1590/S1517-83822006000400012	
Formato: 	text/html	
Fonte: 	Brazilian Journal of Microbiology  v.37 n.4 2006	
Fonte: 	info:eu-repo/semantics/openAccess