Data/hora: 10/06/2024 12:59:13

Provedor de dados: | 63
País: | Brazil
Título: | Topography and spatial variability of soil physical properties
Autores: | Ceddia,Marcos Bacis; Vieira,Sidney Rosa; Villela,André Luis Oliveira; Mota,Lenilson dos Santos; Anjos,Lúcia Helena Cunha dos; Carvalho,Daniel Fonseca de.
Data: | 2009-06-01
Ano: | 2009
Palavras-chave: | Terrain elevation; Geostatistics; Soil physics; Cross semivariance.
Resumo: | Among the soil formation factors, relief is one of the most used in soil mapping, because of its strong correlation with the spatial variability of soil attributes over a landscape. In this study the relationship between topography and the spatial variability of some soil physical properties was evaluated. The study site, a pasture with 2.84 ha, is located near Seropédica, Rio de Janeiro State, Brazil, where a regular square grid with 20 m spacing was laid out and georreferenced. In each sampling point, altitude was measured and undisturbed soil samples were collected, at 0.0-0.1, 0.1-0.2, and 0.2-0.3 m depths. Organic carbon content, soil texture, bulk density, particle density, and soil water retention at 10 (Field Capacity), 80 (limit of tensiometer reading) and 1500 kPa (Permanent Wilting Point) were determined. Descriptive statistics was used to evaluate central tendency and dispersion parameters of the data. Semivariograms and cross semivariograms were calculated to evaluate the spatial variability of elevation and soil physical attributes, as well as, the relation between elevation and soil physical attributes. Except for silt fraction content (at the three depths), bulk density (at 0.2-0.3 m) and particle density (at 0.0-0.1 m depth), all soil attributes showed a strong spatial dependence. Areas with higher elevation presented higher values of clay content, as well as soil water retention at 10, 80 and 1500 kPa. The correlation between altitude and soil physical attributes decreased as soil depth increased. The cross semivariograms demonstrated the viability in using altitude as an auxiliary variable to improve the interpolation of sand and clay contents at the depth of 0.0-0.3 m, and of water retention at 10, 80 and 1500 kPa at the depth of 0.0-0.2 m.
Tipo: | Info:eu-repo/semantics/article
Idioma: | Inglês
Identificador: | http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0103-90162009000300009
Editor: | São Paulo - Escola Superior de Agricultura "Luiz de Queiroz"
Relação: | 10.1590/S0103-90162009000300009
Formato: | text/html
Fonte: | Scientia Agricola  v.66 n.3 2009
Fonte: | info:eu-repo/semantics/openAccess