Data/hora: 10/06/2024 13:48:28

Provedor de dados: 	90	
País: 	Brazil	
Título: 	RECOVERY OF AN OXISOL DEGRADED BY THE CONSTRUCTION OF A HYDROELECTRIC POWER PLANT	
Autores: 	Carvalho,Joseane Carina Borges de; Espindola,Carlos Roberto; Alves,Marlene Cristina; Figueiredo,Getulio Coutinho; Dechen,Sonia Carmela Falci.	
Data: 	2015-12-01	
Ano: 	2015	
Palavras-chave: 	Aggregate stability; Soil compaction; Stripped soil; Soil quality.	
Resumo: 	ABSTRACT The removal of thick layers of soil under native scrubland (Cerrado) on the right bank of the Paraná River in Selvíria (State of Mato Grosso do Sul, Brazil) for construction of the Ilha Solteira Hydroelectric Power Plant caused environmental damage, affecting the revegetation process of the stripped soil. Over the years, various kinds of land use and management systems have been tried, and the aim of this study was to assess the effects of these attempts to restore the structural quality of the soil. The experiment was conducted considering five treatments and thirty replications. The following treatments were applied: stripped soil without anthropic intervention and total absence of plant cover; stripped soil treated with sewage sludge and planted to eucalyptus and grass a year ago; stripped soil developing natural secondary vegetation (capoeira) since 1969; pastureland since 1978, replacing the native vegetation; and soil under native vegetation (Cerrado). In the 0.00-0.20 m layer, the soil was chemically characterized for each experimental treatment. A 30-point sampling grid was used to assess soil porosity and bulk density, and to assess aggregate stability in terms of mean weight diameter (MWD) and geometric mean diameter (GMD). Aggregate stability was also determined using simulated rainfall. The results show that using sewage sludge incorporated with a rotary hoe improved the chemical fertility of the soil and produced more uniform soil pore size distribution. Leaving the land to develop secondary vegetation or turning it over to pastureland produced an intermediate level of structural soil quality, and these two treatments produced similar results. Stripped soil without anthropic intervention was of the lowest quality, with the lowest values for cation exchange capacity (CEC) and macroporosity, as well as the highest values of soil bulk density and percentage of aggregates with diameter size &lt;0.50 mm, corroborated by its lower organic matter content. However, the percentage of larger aggregates was higher in the native vegetation treatment, which boosted MWD and GMD values. Therefore, assessment of some land use and management systems show that even decades after their implementation to mitigate the degenerative effects resulting from the installation of the Hydroelectric Plant, more efficient approaches are still required to recover the structural quality of the soil.	
Tipo: 	Info:eu-repo/semantics/article	
Idioma: 	Inglês	
Identificador: 	http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-06832015000601776	
Editor: 	Sociedade Brasileira de Ciência do Solo	
Relação: 	10.1590/01000683rbcs20140641	
Formato: 	text/html	
Fonte: 	Revista Brasileira de Ciência do Solo  v.39 n.6 2015	
Fonte: 	info:eu-repo/semantics/openAccess