Data/hora: 11/06/2024 14:14:05

Provedor de dados: 	90	
País: 	Brazil	
Título: 	Aggregate stability by the "high energy moisture characteristic" method in an oxisol under differentiated management	
Autores: 	Silva,Érika Andressa da; Oliveira,Geraldo César de; Silva,Bruno Montoani; Carducci,Carla Eloize; Avanzi,Junior Cesar; Serafim,Milson Evaldo.	
Data: 	2014-10-01	
Ano: 	2014	
Palavras-chave: 	Aggregation; Coffee production; Management systems; Method.	
Resumo: 	Studies testing the High Energy Moisture Characteristic (HEMC) technique in tropical soils are still incipient. By this method, the effects of different management systems can be evaluated. This study investigated the aggregation state of an Oxisol under coffee with Brachiaria between crop rows and surface-applied gypsum rates using HEMC. Soil in an experimental area in the Upper São Francisco region, Minas Gerais, was studied at depths of 0.05 and 0.20 m in coffee rows. The treatments consisted of 0, 7, and 28 Mg ha-1 of agricultural gypsum rates distributed on the soil surface of the coffee rows, between which Brachiaria was grown and periodically cut, and compared with a treatment without Brachiaria between coffee rows and no gypsum application. To determine the aggregation state using the HEMC method, soil aggregates were placed in a Büchner funnel (500 mL) and wetted using a peristaltic pump with a volumetric syringe. The wetting was applied increasingly at two pre-set speeds: slow (2 mm h-1) and fast (100 mm h-1). Once saturated, the aggregates were exposed to a gradually increasing tension by the displacement of a water column (varying from 0 to 30 cm) to obtain the moisture retention curve [M = f (Ψ) ], underlying the calculation of the stability parameters: modal suction, volume of drainable pores (VDP), stability index (slow and fast), VDP ratio, and stability ratio. The HEMC method conferred sensitivity in quantifying the aggregate stability parameters, and independent of whether gypsum was used, the soil managed with Brachiaria between the coffee rows, with regular cuts discharged in the crop row direction, exhibited a decreased susceptibility to disaggregation.	
Tipo: 	Info:eu-repo/semantics/article	
Idioma: 	Inglês	
Identificador: 	http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-06832014000500028	
Editor: 	Sociedade Brasileira de Ciência do Solo	
Relação: 	10.1590/S0100-06832014000500028	
Formato: 	text/html	
Fonte: 	Revista Brasileira de Ciência do Solo  v.38 n.5 2014	
Fonte: 	info:eu-repo/semantics/openAccess