Consulta: creatorFacets:"Alwan, salih kadhim"
Registros recuperados: 7
Data/hora: 10/06/2024 17:24:53

Evaluation of innovative cultivation methods, on potato Burren cultivar
Provedor de dados: 111
Autores: Alwan, salih kadhim.
The study aimed to identify the effect of cultivation machine on potato Burren variety, specification under CMBGR  and CMBRO at different distances and ranges of cultivation depths .Two types of potato cultivation  methods (CMBGR and CMBRO) were tested under two cultivation distances(25 and 30 cm) and three levels of cultivation depths (8, 10 and 12 cm). The experiments were conducted in a factorial experiment under a randomized complete block design with three replications ,The CMBGR was significantly better than CMBRO in all studied parameters .For CMBGR the fuel consumption, machine productivity,machine efficiency, germination percentage ,root density and distributed in soil for vegetative growth stage , root density and distributed in soil for tubers...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Potato; Tractor (type New Holland–TD80); Cultivation distances  machine(type Adwhit  ); Mechanical properties; Depth.
Ano: 2021
URL: http://www.cigrjournal.org/index.php/Ejounral/article/view/6415

Effect mechanical on rice husking for test two machines
Provedor de dados: 111
Autores: Alwan, salih kadhim.
The experiment was conducted to evaluated Effect of husking process on the rice productivity for two cultivars Mashkhab (M-33) and Jasmine (JA). Two types of machines (S-KB40 and Y-ST50) were tested at three ranges of clearance between cylinders of 0.5 mm, 0.7mm and 0.9mm for two rice cultivars of JA and M-33. The experiments were carried out in a factorial experiment under complete randomized design with three replications,&amp;nbsp; the study was of the characteristics following machine productivity, power required and husking efficiency, and the qualitative characteristics for two rice JA and M-33 cultivars included, broken rice ratio and head rice . The results showed that S-KB40 machine is better than Y-ST50 machine in all studied conditions for both...
Tipo: Info:eu-repo/semantics/article
Ano: 2024
URL: http://www.cigrjournal.org/index.php/Ejounral/article/view/8755

Effect of grain moisture  and clearance of machine on mechanical damage of processed paddy
Provedor de dados: 111
Autores: Alwan, salih kadhim.
The effect of  clearance in husking machine (Satake BK40 type) on paddy cultivar of Amber 31 (AM31)  were tested during husking at three clearance of 0.5,0.7and 0.9 mm and two grains moisture 9-11% and 11-13%  .The experiments were carried out in a factorial experiment under complete randomized design with three replications. The results showed that the 9-11% grain moisture was significantly better than the 11-13% grain moisture in all studied conditions. The results showed a machine productivity of 1.707 and 1.441 th-1, power consumption of 13.585 and 14.800 kW, husking efficiency of 83.478% and 81.979%, milling recovery of 69.848 and68.794% ,head paddy of 68.086 and 66.221 %, and broken paddy of 6.226 % and 7.471 % , for 9-11% and 11-13%, respectively....
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Mechanical damage; Processed paddy; Clearance; Husking; Grain moisture .
Ano: 2022
URL: http://www.cigrjournal.org/index.php/Ejounral/article/view/6473

The effect of thresher machines ,moisture grain and velocity on maize , Cadiz cultivar
Provedor de dados: 111
Autores: Alwan, salih kadhim.
           The effect of thresher machines on maize , Cadiz cultivar was studied based on some technical indicators. Two types of machines (Maize thresher local M.T.L and Maize thresher MGI.Ty60) were tested at three velocity cylinder threshing  of 200,250 and 300rpm  and three ranges of grain moistures of 15%, 17% and 19%. The experiments were carried out in a factorial experiment under complete randomized design with three replications. The results showed that the Maize thresher local M.T.L machine was significantly better than the Maize thresher MGI.Ty60  machine in all studied conditions. The results showed a production process of 1.196 and 1.147 t\h, power consumption of 11.361 and 12.234 kW, cracked grain percentage of 4.024% and 4.374%, broken maize...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Maize; Moisture content; Thresher velocity; Cadiz cultivar; Thresher .
Ano: 2018
URL: http://www.cigrjournal.org/index.php/Ejounral/article/view/5029

A study  the effect of  two machine types  in some technical indicators
Provedor de dados: 111
Autores: Alwan, salih kadhim.
The experiment has been conducted to evaluate the effect in some technical indicators of  husking and whitening machines for cultivar rice (DM), in the labrotaries of the Tehran University in 2015. This research includes the using of two types of  machines (Satake and Yanmar),),under three clearance between cylinders levels  0.4 , 0.6 and 0.8  mm  and three grain moisture levels  10-12% , 12- 14% and 14-16%. The results showed that the Satake type machine is significantly better than the Yanmar type machine in all studies properties  .While clearance o.8 significant superiorly on two  0.4,0.6 mm levels as well as moisture cotent of grain 10-12%  is superior significantly on two 12-14%,14-16% levels in  all studied properties . The best results have come...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Agriculture engineering Husking; Grain moisture content; Machine; Clearance; Rice; Technical indicators.
Ano: 2016
URL: http://www.cigrjournal.org/index.php/Ejounral/article/view/3840

Effect of local design machine , clearance and grain moisture on corn shelling
Provedor de dados: 111
Autores: Alwan, salih kadhim.
The effect of local thresher machine on maize cultivar Rabie was observed based on some technical indicators, under two clearance of threshing cylinders (0.7 and 0.9mm) and three grain moisture content .The experiments were conducted in a factorial experiment under complete randomized design with three replications. The 0.9mm clearance  was significantly better than 0.7mm clearance  while the moisture content of grain at range of 13-15% was significantly superior to the other ranges of 15-17% and17%-19% in all studied parameters. For local THM the machine productivity, power consumption, threshing efficiency, grains damage ,broken corn, grain cleaning, were 1.251 th-1, 9.358 kW, 88.717; 1.529; 3.272;  and 1.318 percent respectively. The interaction among ...
Tipo: Info:eu-repo/semantics/article
Ano: 2021
URL: http://www.cigrjournal.org/index.php/Ejounral/article/view/6225

Mechanical damage for local design machine on maize cultivars of CA and GO
Provedor de dados: 111
Autores: Alwan, salih kadhim.
The effect of  rotational speed in shelling machine (LMS type) on maize cultivars of Cadiz (CA) and Golden (GO) were tested during shelling at three rotational speed of 300,400 and 500rpm . The experiments were carried out in a factorial experiment under complete randomized design with three replications. The results showed that the CA cultivar was significantly better than the GO in all studied conditions. The results showed a shelling productivity of 1.354 and 1.303 t\h, power consumption of 8.725 and 9.174 kW, shelling efficiency of 84.857% and 82.857%, unshelled grains of 1.260 and1.509% ,loose grains at kernel outlet of 1.444 and 1.612 %, grains damage of 1.546 and 1.805% and grain cleanliness of 90.828 and 90.148 % broken maize  of 3.777 % and 4.335...
Tipo: Info:eu-repo/semantics/article
Ano: 2019
URL: http://www.cigrjournal.org/index.php/Ejounral/article/view/5393