Consulta: subjectFacets:"Acoustic imagery"
Registros recuperados: 1
Data/hora: 13/06/2024 01:09:43

Cartographie sous-marine: Etat de l'art et problemes
Provedor de dados: 5
Autores: Renard, V.
The side looking sonars have been developed for greater swath coverage, digital processing of the signals has improved the quality of the images and interferometric techniques have been used to determine the depth of the bottom features. A review of the systems existing today is presented. Documents such as graphs, block diagrams, images, maps, sections, created from data acquired at sea level suffer from a filtering or smoothing effect that restricts the representativity of the measured parameters and therefore limits their interpretation. The greater the depth of the seafloor, the greater the filtering. It is due not only to the nature of the measured phenomenon but also the characteristics of the sensors, to their operation and to the data processing....
Tipo: Text
Palavras-chave: Bathymetry; Cartography; Sensors; Echosounders; Acoustic imagery; Acoustics; Ocean floor; Seafloor mapping.
Ano: 1990
URL: http://archimer.ifremer.fr/doc/1990/acte-1147.pdf