Consulta: subjectFacets:"Furrow irrigation"
Registros recuperados: 18
Data/hora: 10/06/2024 13:44:42

Espaçamento e densidade para o cultivo do arroz de sequeiro na microrregião Alto Purus-Acre. II. Plantio em sulco.
Provedor de dados: 14
Autores: CAMPOS, I. S.; MEDEIROS, J. A.
A cultura do arroz no Acre, ainda não se reveste da importância econ6mica esperada, apesar de sua condição de cereal de alta produtividade e baixo custo de produção. Com o êxodo da população do meio rural para a cidade e outras regiões que ofereçam melhores condiç6es de trabalho, o agricultor, muitas vezes, vê-se ante o dilema de usar máquinas ou não poder realizar as diversas operações agrícolas, face a indisponibilidade ou deficiência de mão-de-obra. O sistema operacional utilizado pela maioria dos agricultores, é baseado na mão-de-obra familiar, onde considerável parte da produção obtida é consumida pela família, sendo a restante comercializada. Processos inadequados de manejo do solo e da cultura, contribuem para o decréscimo da produtividade. Apesar...
Tipo: Comunicado Técnico (INFOTECA-E)
Palavras-chave: Dry rice; Arroz de secano; Alto Purus; Acre; Amazônia Ocidental; Western Amazon; Oriza sativa; Densidad de plantas; Distancia entre hileras; Riego por surcos; Arroz; Arroz sequeiro; Cultivo de sequeiro; Espaçamento; Densidade de plantio; Plantio; Irrigação por Sulco; Rice; Plant density; Row spacing; Furrow irrigation.
Ano: 1980
URL: http://www.infoteca.cnptia.embrapa.br/infoteca/handle/doc/492303

Irrigacao do feijoeiro.
Provedor de dados: 14
Autores: AZEVEDO, J. A. de; CAIXETA, T. J.
Reune informacoes relativas a pratica da irrigacao no feijoeiro. Mostra a sua influencia na produtividade da cultura e destaca a necessidade de sua utilizacao, diante da deficiencia de agua no solo, originada das incertezas do clima nas epocas tradicionais de plantio. Discute em detalhes as reacoes do feijoeiro a periodo de deficit e de excesso de agua. Indica as fases criticas e as necessidades totais e parciais de agua. Sao descritos os criterios que, pela simplicidade de aplicacao e maior ocorrencia de resultados experimentais, permitem decidir o momento de irrigar e quantificar os volumes de irrigacao. De alguns metodos de irrigacao, entre os com possibilidade de serem usados no cultivo do feijao (irrigacao por sulcos e por aspersao), definem-se...
Tipo: Circular Técnica (INFOTECA-E)
Palavras-chave: Sulco; Cultivo; Bean; Deficit hídrico; Feijoeiro; Irrigation returns; Phaseolus vulgares; Sub-irrigation; Water deficit; Yield.; Deficiência Hídrica; Cerrado; Feijão; Evapotranspiração; Manejo de Água; Irrigação por Sulco; Irrigação; Irrigação por Aspersão; Produtividade; Rentabilidade; Topografia.; Evapotranspiration; Furrow irrigation; Sprinkler irrigation; Water management.
Ano: 1986
URL: http://www.infoteca.cnptia.embrapa.br/infoteca/handle/doc/547470

Tubo janelado para irrigacao por sulcos.
Provedor de dados: 14
Autores: SILVA, E. M. da; AZEVEDO, J. A. de; RESENDE, M.
bitstream/item/99254/1/comtec-24.pdf
Tipo: Comunicado Técnico (INFOTECA-E)
Palavras-chave: Sulco; Tubo janelado; Irrigation equipment; Control; Controle; Erosion; Janelados.; Cerrado; Erosão; Irrigação por Sulco.; Irrigação; Furrow irrigation; Pipes.
Ano: 1981
URL: http://www.infoteca.cnptia.embrapa.br/infoteca/handle/doc/549325

Eficiência de irrigação em sulcos parcialmente fechados no final.
Provedor de dados: 14
Autores: SOARES, J. M.
Trata do sistema de irrigação por sulcos abertos; sistema de irrigação por sulcos parcialmente fechados no final: recessão da água no sulco, vazão de escoamento superficial no final do sulco, perdas de água por escoamento, eficiência de aplicação e custos de implantação dos vertedores.
Tipo: Comunicado Técnico (INFOTECA-E)
Palavras-chave: Sulco; Escoamento superficial; Vazão constante; Recessão de água; Constant flow; Water recession.; Irrigação; Irrigation; Furrow irrigation; Runoff.
Ano: 1989
URL: http://www.infoteca.cnptia.embrapa.br/infoteca/handle/doc/133406

Monitoramento do manejo de agua na cultura da videira ao nivel de campo sob irrigacao por sulcos, utilizando tubos janelados moveis.
Provedor de dados: 14
Autores: SOARES, J. M.; NASCIMENTO, T.; CORDEIRO, G. G.; CASTRO NETO, M. T. de; SILVA, D. D. da.
Descricao do sistema de irrigacao, monitoramento da umidade do solo, mapeamento horizontal do sistema radicular da videira sob irrigacao por sulcos, distribuicao vertical do sistema radicular.
Tipo: Outras publicações técnicas (INFOTECA-E)
Palavras-chave: Tubo janelado novelo; Grape; Management; Gated pipe; Uva; Água; Irrigação por Sulco; Manejo; Grapes; Furrow irrigation; Water.
Ano: 1994
URL: http://www.infoteca.cnptia.embrapa.br/infoteca/handle/doc/133443

Soil phosphorus availability differences between sprinkler and furrow irrigation
Provedor de dados: 18
Autores: Ippolito, J.A.; Bjorneberg, D.L.
Water flowing in irrigation furrows detaches and transports soil particles and subsequently nutrients such as phosphorus.  To reduce the risk of erosion and offsite phosphorus transport, producers in south-central Idaho have been converting from furrow to sprinkler irrigation.  We completed research on soil phosphorus dynamics in furrow versus sprinkler irrigated soils from four paired-fields in the region.  Surface soils (0-2.5 inches) were obtained from fields in September following barley harvest.  Furrow irrigated soils contained 38 parts per million of plant-available phosphorus (i.e. Olsen-extractable), on average, as compared to 20 parts per million under sprinkler irrigation.  These results are important as 20 parts per million extractable...
Tipo: Conference or Workshop Item
Palavras-chave: Furrow irrigation; Sprinkler irrigation; Soil.
Ano: 2013
URL: http://eprints.nwisrl.ars.usda.gov/1573/1/1529.pdf

Estimation of furrow irrigation sediment loss using an artificial neural network
Provedor de dados: 18
Autores: King, B.A.; Bjorneberg, D.L.; Trout, T.J.; Mateos, L; Araujo, D. F.; Costa, R. N.
The area irrigated by furrow irrigation in the U.S. has been steadily decreasing but still represents about 20% of the total irrigated area in the U.S. Furrow irrigation sediment loss is a major water quality issue and a method for estimating sediment loss is needed to quantify the environmental impacts and estimate effectiveness and economic value of conservation practices. Artificial neural network (NN) modeling was applied to furrow irrigation to predict sediment loss as a function of hydraulic and soil conditions.  A data set consisting of 1926 furrow evaluations spanning three continents and a wide range of hydraulic and soil conditions was used to train and test a multilayer perceptron feed forward NN model. The final NN model consisted of 16 inputs,...
Tipo: Article
Palavras-chave: Furrow irrigation; Water quality.
Ano: 2015
URL: http://eprints.nwisrl.ars.usda.gov/1593/1/1551.pdf

Soil phosphorus dynamics under sprinkler and furrow irrigation
Provedor de dados: 18
Autores: Ippolito, J.A.; Bjorneberg, D.L.
Furrow irrigation detaches and transports soil particles and subsequently nutrients such as phosphorus.  To reduce the risk of erosion and offsite phosphorus movement, producers can convert from furrow to sprinkler irrigation.  We completed research on soil phosphorus dynamics in furrow versus sprinkler irrigated soils from four paired fields in south central Idaho.  Surface soils (0-2.5 inches) were obtained from fields in the fall following harvest.  Furrow irrigated soils contained 38 parts per million of plant-available phosphorus (i.e. Olsen-extractable) on average, as compared to 20 parts per million under sprinkler irrigation.  These results are important as 20 parts per million Olsen-extractable phosphorus may be considered the concentration where...
Tipo: Conference or Workshop Item
Palavras-chave: Furrow irrigation; Sprinkler irrigation; Soil.
Ano: 2014
URL: http://eprints.nwisrl.ars.usda.gov/1574/1/1530.pdf

Changes in soil test phosphorus and phosphorus in runoff from calcareous soils receiving manure, compost, and fertilizer application with and without alum
Provedor de dados: 18
Autores: Leytem, A.B.; Bjorneberg, D.L.
Tipo: Article
Palavras-chave: Calcareous soil; Manure; Phosphorous; Furrow irrigation.
Ano: 2009
URL: http://eprints.nwisrl.ars.usda.gov/1355/3/1332.pdf

Conservation practice effectiveness in the irrigated Upper Snake/Rock Creek watershed
Provedor de dados: 18
Autores: Bjorneberg, D.L.; Westermann, D.T.; Nelson, N.O.; Kendrick, J.H.
The Upper Snake River/Rock Creek Conservation Effects Assessment Project was initiated in 2005 to determine the effectiveness of conservation practices in an irrigated watershed. Our objectives were to determine water and salt balances and water quality effects of using sprinkler rather than furrow irrigation in the Twin Falls irrigation tract in southern Idaho. Data from the current study were compared with earlier studies conducted from 1968 to 1971. Irrigation water diverted from the Snake River supplied 73% and 83% of the hydrologic input to this 82,000 ha (202,000 ac) watershed in 2005 and 2006, respectively, with approximately 40% flowing back to the Snake River through furrow irrigation runoff, unused irrigation water, and subsurface drainage. Net...
Tipo: Article
Palavras-chave: Sprinkler irrigation; Furrow irrigation.
Ano: 2008
URL: http://eprints.nwisrl.ars.usda.gov/1324/1/1301.pdf

The Current State of Predicting Furrow Irrigation Erosion
Provedor de dados: 18
Autores: Bjorneberg, D.L.; Strelkoff, T.; Clemmens, A.J.; Lee, J.H.
There continues to be a need to predict furrow irrigation erosion to estimate on- and off-site impacts of irrigation management. The objective of this paper is to review the current state of furrow erosion prediction technology considering four models: SISL, WEPP, WinSRFR and APEX. SISL is an empirical model for predicting annual soil loss from furrow irrigated fields. SISL could potentially be a useful model if a new method was developed to calculate base soil loss for areas other than southern Idaho where it was developed. The WEPP model uses physically-based equations to predict erosion in irrigation furrows, which are assumed to be the same as rills. Primary difficulties with the WEPP model are defining erodibility parameters for furrow irrigation and...
Tipo: Conference or Workshop Item
Palavras-chave: Furrow irrigation; Soil.
Ano: 2010
URL: http://eprints.nwisrl.ars.usda.gov/1570/1/1526.pdf

Worms and water
Provedor de dados: 18
Autores: Kemper, W.D.; Trout, T.J.; Segeren, Antone; Bullock, Murray.
Tipo: Article
Palavras-chave: Practical farm efficiency; Sprinkler irrigation; Furrow irrigation.
Ano: 1987
URL: http://eprints.nwisrl.ars.usda.gov/492/1/644.pdf

Aggregate tensile strength and friability characteristics of furrow and sprinkler irrigated fields in Southern Idaho
Provedor de dados: 18
Autores: Koehn, A.C.; Lehrsch, G.A.; Busscher, W.J.; Evans, D.E.; King, B.A.; Stieneke, D.L.; Sojka, R.E.
Agricultural crops grown in southern Idaho are furrow or sprinkler irrigated. Therefore, the soil experiences several wetting and drying cycles each growing season that can contribute to changes in aggregate tensile strength and friability. The objective of the research was to evaluate the influence of irrigation on soil structural properties. Four furrow irrigated fields were sampled at the top and bottom of the field, in the furrow and on the bed location of the furrow. Five sprinkler irrigated fields were sampled at 0-5 and 5-15 cm depth and at the top and bottom of the field. Results from this study indicate that differences in tensile strength in furrow irrigated fields were only evident soon after irrigation; otherwise, there were few differences in...
Tipo: Article
Palavras-chave: Furrow irrigation; Sprinkler irrigation.
Ano: 2014
URL: http://eprints.nwisrl.ars.usda.gov/1567/1/1523.pdf

Managing Runoff Water Quality From Recently Manured, Furrow Irrigated Fields
Provedor de dados: 18
Autores: Lentz, R.D.; Westermann, D.T.
Nutrient losses in furrow irrigation runoff potentially increase when soils are amended with manure. We evaluated the effect of tillage, water soluble polyacrylamide (WSPAM) and irrigation management on runoff water quality during the first furrow irrigation on a calcareous silt loam soil, which had received 45 Mg/ha (dry wt.) dairy manure applied in the fall. In Exp. 1 the amended soil was rototilled and irrigated that fall; furrow inflows were either treated with 10 mg/L WSPAM injected into furrow inflows only during furrow advance (Fall-WSPAM), or were untreated (Fall-Control). In Exp. 2 the first irrigation on the amended soil was delayed until the following spring and treatments included rototilled WSPAM (Spring-WSPAM) and untreated rototilled...
Tipo: Article
Palavras-chave: Water management; Water quality; Furrow irrigation.
Ano: 2010
URL: http://eprints.nwisrl.ars.usda.gov/1384/1/1359.pdf

Reducing nutrient losses in runoff from furrow irrigation
Provedor de dados: 18
Autores: Lentz, R.D.; Westermann, D.T.; Lehrsch, G.A.
Few studies have comprehensively examined nutrient losses in runoff from furrow-irrigated fields, but the rising cost of fertilizer and finite nature of the resource encourages further research.  A 2-yr experiment measured runoff losses of sediment, particulate P and N, and dissolved NO3-N, NH4-N, K, and reactive P (DRP) from fertilized, manured, or non-amended fields.  Average nutrient losses were substantial, including 15.6 lbs ac/yr dissolved N, P, and K and 73.6 lbs ac/yr particulate N and P. The cost or replacing these nutrients with inorganic fertilizers was not trivial, at $54.69 ac/yr.  Relative to non-amended soil, manure increased dissolved K, NO3-N, and DRP in runoff by 2.1x, 1.5x, and 2.7x, respectively. Other experiments evaluated the...
Tipo: Conference or Workshop Item
Palavras-chave: Furrow irrigation; Runoff losses; Nutrients; Sediment.
Ano: 2013
URL: http://eprints.nwisrl.ars.usda.gov/1518/1/1482.pdf

Isotopic composition of maize as related to N-fertilization and irrigation in the Mediterranean region
Provedor de dados: 63
Autores: Lasa,Berta; Irañeta,Iosu; Muro,Julio; Irigoyen,Ignacio; Aparicio Tejo,Pedro María.
Nitrate leaching as a result of excessive application of N-fertilizers and water use is a major problem of vulnerable regions. The farming of maize requires high N fertilization and water inputs in Spain. Isotopic techniques may provide information on the processes involved in the N and C cycles in farmed areas. The aim of this work was studying the impact of sprinkler and furrow irrigation and N input on maize (Zea mays L.) yields, and whether isotopic composition can be used as indicator of best farming practices. Trials were set up in Tudela (Spain) with three rates of N fertilization (0, 240 and 320 kg urea-N ha-1) and two irrigation systems (furrow and sprinkler). Yield, nitrogen content, irrigation parameters, N fate and C and N isotope composition...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Zea mays L.; Furrow irrigation; Nitrogen; Sprinkler irrigation.
Ano: 2011
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0103-90162011000200008

Water-yield relationships of potato under different irrigation methods and regimens
Provedor de dados: 63
Autores: Erdem,Tolga; Erdem,Yesim; Orta,Halim; Okursoy,Hakan.
Yield response to irrigation of different crops is of major importance in production planning where water resources are limited. This study aims to determine the effect of different irrigation methods and irrigation regimens on potato yield in the Trakya Region, Turkey, during 2003 and 2005. Potato was grown under furrow and drip irrigation methods and three regimens: irrigation applied when 30, 50, or 70% of the available water was consumed. The seasonal potato evapotranspiration ranged on 501 to 683 mm in 2003, and 464 to 647 mm in 2005. The furrow and drip irrigation methods had no significant effect on tuber yield for both years. Irrigation regimens influenced tuber yield (P &lt; 0.05) in 2005, and the highest tuber yield was registered for 30%...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Furrow irrigation; Drip irrigation; Evapotranspiration; Water use efficiency.
Ano: 2006
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0103-90162006000300003

A Dynamic Decision Support System for Farm Water Management in Surface Irrigation: Model Development and Application
Provedor de dados: 117
Autores: Flores,Carlos I.; Holzapfel,Eduardo A.; Lagos,Octavio.
An online dynamic decision support system (DDSS) was developed, to support the farm water management in surface irrigation. The online DDSS was based on the formulation and integration of three components: a dynamic-relational data base, an administrator model, and a graphical user interface. The DDSS allows routines of actualization, edition and addition of online data, providing information in real time. The online DDSS was applied in an orange orchard (Citrus sinensis L. Osbeck) cv. Valencia Late under furrow irrigation. The results pointed out that the time irrigation cutoff was the main significant management factor, to decrease the hazard of leaching, superficial runoff and percolation. Applying the results obtained with the DDSS, furrow irrigation...
Tipo: Journal article
Palavras-chave: Furrow irrigation; On-line irrigation management; Orange orchard.
Ano: 2010
URL: http://www.scielo.cl/scielo.php?script=sci_arttext&pid=S0718-58392010000200011