Consulta: subjectFacets:"Seawater"
Registros recuperados: 64
Data/hora: 12/06/2024 13:28:14

Patterns of trace metal bioaccumulation and trophic transfer in a phytoplankton-zooplankton-small pelagic fish marine food web
Provedor de dados: 5
Autores: Chouvelon, Tiphaine; Strady, Emilie; Harmelin-vivien, Mireille; Radakovitch, Olivier; Brach-papa, Christophe; Crochet, Sylvette; Knoery, Joel; Rozuel, Emmanuelle; Thomas, Bastien; Tronczynski, Jacek; Chiffoleau, Jean-francois.
Trace metal contamination in the European sardine and anchovy food web was investigated in the Gulf of Lions, NW Mediterranean Sea, including seawater and size fractions of plankton. The results highlighted: i) higher and more variable concentrations in the smaller plankton size classes for all metals except cadmium; ii) higher concentrations in anchovy versus sardine for all elements except lead; iii) different patterns of metal bioaccumulation through the food web: cobalt, nickel, copper, silver, lead and zinc displayed continuously decreasing concentrations (with the exception of increased zinc in fish only), while mercury concentrations dropped considerably in larger plankton size classes and rose significantly in fish. Lastly, cadmium concentrations...
Tipo: Text
Palavras-chave: Inorganic elements; Seawater; Size-classed plankton; Sardina pilchardus; Engraulis encrasicolus; Mediterranean Sea.
Ano: 2019
URL: https://archimer.ifremer.fr/doc/00511/62286/67906.pdf

Réaction de réduction de l'oxygène sur les aciers inoxydables en eau de mer naturelle. Influence du biofilm sur les processus de corrosion
Provedor de dados: 5
Autores: Le Bozec, Nathalie.
iofilm development on stainless steels immersed in natural seawater can have prejudicial consequences on the resistance of these materials to corrosion . The goal of the present study was to get more precise information on the corrosion processes, and especially on the oxygen reduction reaction. As the reaction is linked to the stainless steel surface state, the characterisation of the oxides films (composition, structure, thickness...) is essential to understand the mechanisms and the oxygen reduction kinetic. The first aim of the study has been to correlate the oxygen reduction processes with the characteristics of the oxides layer as a function of the alloy surface treatment (mechanical polishing, electrochemical passivation and prereduction, chemical...
Tipo: Text
Palavras-chave: Hydrogen peroxide; Oxides layer; Biofilm; Oxygen reduction; Corrosion; Seawater; Stainless steels; Peroxyde d'hydrogène; Films d'oxydes; Biofilm; Réduction de l'oxygène; Corrosion; Eau de mer; Aciers inoxydables.
Ano: 2000
URL: http://archimer.ifremer.fr/doc/2004/these-223.pdf

Long-term effects of moderate elevation of oxidation–reduction potential on European seabass (Dicentrarchus labrax) in recirculating aquaculture systems
Provedor de dados: 5
Autores: Li, Xian; Przybyla, Cyrille; Triplet, Sebastien; Liu, Ying; Blancheton, Jean-paul.
The long term effects of moderate elevation ORP (oxidation–reduction potential) around 300–320 mV on the growth, hematological parameters and the ability of European seabass (Dicentrarchus labrax) to react against bacterial infection was studied in recirculating aquaculture systems (RASs). Two RASs, one with a moderate ozonation (RAS-O3) and a control (RAS-C) were used in this experiment. After 60 days, seabass reared in the RAS-O3 were more able to react against a Vibrio anguillarum infection. It was in spite of the fact that seabass in the RAS-O3 showed decreased feed intake, feed conversion rate, growth rate and modified hematological parameters compared with the fish in RAS-C. It is obvious that an ORP level of 300–320 mV is too high for seabass to...
Tipo: Text
Palavras-chave: Oxidation–reduction potential; Seawater; European seabass; Welfare; RASs.
Ano: 2015
URL: https://archimer.ifremer.fr/doc/00244/35562/34132.pdf

Detection of ostreid herpesvirus 1 (OsHV-1) DNA in seawater by PCR: influence of water parameters in bioassays
Provedor de dados: 5
Autores: Vigneron, Vassilia; Solliec, Gaelle; Montanie, Hélène; Renault, Tristan.
Since 1991, herpesvirus infections have been reported among larvae and juveniles of various bivalves. Most of the studies focused on detection of viral infections of economically important species. However, the persistence of bivalve herpesviruses; in the marine environment is poorly documented. The present study concerns the role of seawater parameters in Ostreid Herpesvirus I (OsHV-1) detection by polymerase chain reaction (PCR). Viral DNA extracted from purified particles or virions present in infected oyster larvae were detected by PCR after storage in different media at different temperatures. The lowest detection threshold was found using distilled water or Tris EDTA buffer. In seawater, the threshold was higher. The use of sterile media permitted...
Tipo: Text
Palavras-chave: Temperature; PCR; Detection; Seawater; Viral DNA; Oyster herpesvirus 1.
Ano: 2004
URL: http://archimer.ifremer.fr/doc/2004/publication-2909.pdf

Use of rotavirus virus-like particles as surrogates to evaluate virus persistence in shellfish
Provedor de dados: 5
Autores: Loisy, Fabienne; Atmar, R; Le Saux, Jean-claude; Cohen, J; Caprais, Marie-paule; Pommepuy, Monique; Le Guyader, Soizick.
Rotavirus virus-like particles (VLPs) and MS2 bacteriophages were bioaccumulated in bivalve mollusks to evaluate viral persistence in shellfish during depuration and relaying under natural conditions. Using this nonpathogenic surrogate virus, we were able to demonstrate that about 1 log(10) of VLPs was depurated after 1 week in warm seawater (22 degrees C). Phage MS2 was depurated more rapidly (about 2 log(10) in 1 week) than were VLPs, as determined using a single-compartment model and linear regression analysis. After being relayed in the estuary under the influence of the tides, VLPs were detected in oysters for up to 82 days following seeding with high levels of VLPs (concentration range between 10(10) and 10(9) particles per g of pancreatic tissue)...
Tipo: Text
Palavras-chave: Seawater; Viral diseases; Bioaccumulation; Depuration; Contamination; Model; Pancreas; Regression analysis; Shellfish; Phages; Virus.
Ano: 2005
URL: http://archimer.ifremer.fr/doc/2005/publication-1233.pdf

Natural Degradation and Biodegradation of Poly(3-Hydroxybutyrate-co-3-Hydroxyvalerate) in Liquid and Solid Marine Environments
Provedor de dados: 5
Autores: Deroine, Morgan; Cesar, Guy; Le Duigou, Antoine; Davies, Peter; Bruzaud, Stephane.
In this study, natural degradation and biodegradation of poly(3-hydroxybuyrate-co-3-hydroxyvalerate) (PHBV) films were followed in different marine environments. First of all, ageing of PHBV films was investigated in natural seawater for 180 days and degradation was followed by means of weight loss measurements, scanning electron microscopy (SEM), differential scanning calorimetry and steric exclusion chromatography. In a second part, biodegradation tests were performed on PHBV powder, by following carbon dioxide (CO2) release(,) to highlight the PHBV bioassimilation of marine microorganisms. Three different marine environments were considered for biodegradation tests: a solid inoculum with foreshore sand, a solid-liquid inoculum with sand and seawater and...
Tipo: Text
Palavras-chave: PHBV; Natural ageing; Degradation; Biodegradation; Seawater.
Ano: 2015
URL: http://archimer.ifremer.fr/doc/00296/40735/42020.pdf

Iron sources and dissolved-particulate interactions in the seawater of the Western Equatorial Pacific, iron isotope perspectives
Provedor de dados: 5
Autores: Labatut, M.; Lacan, F.; Pradoux, C.; Chmeleff, J.; Radic, A.; Murray, J. W.; Poitrasson, F.; Johansen, A. M.; Thil, F.
This work presents iron isotope data in the western equatorial Pacific. Marine aerosols and top core margin sediments display a slightly heavy Fe isotopic composition (Fe-56) of 0.330.11 (2SD) and 0.140.07, respectively. Samples reflecting the influence of Papua New Guinea runoff (Sepik River and Rabaul volcano water) are characterized by crustal values. In seawater, Fe is mainly supplied in the particulate form and is found with a Fe-56 between -0.49 and 0.34 +/- 0.07 parts per thousand. The particulate Fe seems to be brought mainly by runoff and transported across continental shelves and slopes. Aerosols are suspected to enrich the surface Vitiaz Strait waters, while hydrothermal activity likely enriched New Ireland waters. Dissolved Fe isotopic ratios...
Tipo: Text
Palavras-chave: Iron isotopes; Particles; Equatorial Pacific; Papua New Guinea; Seawater; GEOTRACES.
Ano: 2014
URL: https://archimer.ifremer.fr/doc/00290/40074/39162.pdf

Impact of environmental factors on in situ determination of iron in seawater by flow injection analysis
Provedor de dados: 5
Autores: Laes, Agathe; Vuillemin, Renaud; Leilde, Bernard; Sarthou, Géraldine; Bournot Marec, Claudie; Blain, Stéphane.
A sensitive method for iron determination in seawater has been adapted on a submersible chemical analyser for in situ measurements. The technique is based on flow injection analysis (FIA) coupled with spectrophotometric detection. When direct injection of seawater was used, the detection limit was 1.6 nM, and the precision 7%, for a triplicate injection of a 4 nM standard. At low iron concentrations, on line preconcentration using a column filled with 8-hydroxyquinoline (8HQ) resin was used. The detection limit was 0.15 nM (time of preconcentration = 240 s), and the precision 6%, for a triplicate determination of a I nM standard, allowing the determination of Fe in most of the oceanic regimes, except the most depleted surface waters. The effect of...
Tipo: Text
Palavras-chave: Temperature and pressure effects; Submersible chemical analyser; Seawater; In situ measurements; Iron; Flow injection analysis.
Ano: 2005
URL: http://archimer.ifremer.fr/doc/2005/publication-1209.pdf

Durability of polydicyclopentadiene under high temperature, high pressure and seawater (offshore oil production conditions)
Provedor de dados: 5
Autores: Le Gac, Pierre-yves; Choqueuse, Dominique; Paris, Marc; Recher, G.; Zimmer, Celine; Melot, D.
In the offshore industry polymer coatings are widely used to ensure thermal insulation of steel pipes, and to avoid over-cooling of the hot oil inside. Because of very severe service conditions (i.e. high temperature, high pressure and presence of seawater) and an expected life time of 20 years, durability of these coatings is a major issue for this industry. Polypropylene and polyurethane are often used for this application, nevertheless these polymers have some limitations in terms of processing time for polypropylene and maximum service temperature for polyurethane. Polycyclopentadiene (pDCPD) shows good processing characteristics and low thermal conductivity, so this polymer could be a good alternative coating in the offshore industry, but the...
Tipo: Text
Palavras-chave: Polydicyclopentadiene; Seawater; Accelerated ageing; Oxidation; Offshore; Field joint.
Ano: 2013
URL: http://archimer.ifremer.fr/doc/00114/22534/20233.pdf

Responses of enteric bacteria to environmental stresses in seawater
Provedor de dados: 5
Autores: Troussellier, Marc; Bonnefont, Jean-luc; Courties, Claude; Derrien, Annick; Dupray, Elizabeth; Gauthier, Michel; Gourmelon, Michele; Joux, Fabien; Lebaron, Philippe; Martin, Yvan; Pommepuy, Monique.
The effects of different environmental factors (nutrient deprivation, hyperosmotic shock, exposure to light) on enteric bacteria which have been transferred into the marine environment, have been studied experimentally (microcosms) by considering demographic, physiological and genetic responses in Escherichia coli or Salmonella typhimurium populations. Short-term experiments (less than or equal to 48 h) showed that nutrient deprivation induced limited changes in measured bacteriological variables, but when combined with hyperosmotic shock, it results in an energy charge decrease and inactivation of membrane transport. Light exposure mainly affects the colony-forming capacity of bacterial populations. Combining different stress factors confirmed the rapid...
Tipo: Text
Palavras-chave: Genetics; Cellular states; Physiology; Seawater; Enteric bacteria; Génétique; Etats cellulaires; Physiologie; Eau de mer; Entérobactéries.
Ano: 1998
URL: http://archimer.ifremer.fr/doc/1998/publication-845.pdf

The determination of total dissolved free primary amines in seawater: Critical factors, optimized procedure and artefact correction
Provedor de dados: 5
Autores: Aminot, Alain; Kerouel, Roger.
The paper reviews the methods described in the literature for the determination of total dissolved free primary amines (TDFPA) by fluorescence. A wide set of reaction conditions can be found, but they rely on few experiments for their validation. Among fluorogenic compounds, o-plithaldialdehyde (OPA) is more sensitive than fluorescamine and was thus examined here. However, the use of mercaptoethanol (ME) in the reaction (as ail additional derivatization compound) is able to generate unreliable results, in particular when standardization relies on glycine. We suggest replacing ME with 3-mercaptopropionic acid (MPA) which induces more stable and comparable fluorescence among amine Compounds. A systematic study was therefore undertaken to define reagent...
Tipo: Text
Palavras-chave: Fluorescence; Determination; Seawater; Total dissolved free primary amines.
Ano: 2006
URL: http://archimer.ifremer.fr/doc/2006/publication-2274.pdf

Environmental degradation of composites for marine structures: new materials and new applications
Provedor de dados: 5
Autores: Davies, Peter.
This paper describes the influence of seawater ageing on composites used in a range of marine structures, from boats to tidal turbines. Accounting for environmental degradation is an essential element in the multi-scale modelling of composite materials but it requires reliable test data input. The traditional approach to account for ageing effects, based on testing samples after immersion for different periods, is evolving towards coupled studies involving strong interactions between water diffusion and mechanical loading. These can provide a more realistic estimation of long-term behaviour but still require some form of acceleration if useful data, for 20 year lifetimes or more, are to be obtained in a reasonable time. In order to validate extrapolations...
Tipo: Text
Palavras-chave: Seawater; Immersion; Durability; Damage; Coupling.
Ano: 2016
URL: http://archimer.ifremer.fr/doc/00340/45167/44603.pdf

Pasteurization: A reliable method for preservation of nutrient in seawater samples for inter-laboratory and field applications
Provedor de dados: 5
Autores: Daniel, Anne; Kerouel, Roger; Aminot, Alain.
Following previous work, the production of reference material for nutrients in seawater, using pasteurization as a preservation method, was carried out seven times between 2006 and 2010 in the framework of inter-laboratory exercises. The preparation of samples from natural seawater allowed to become depleted in nutrients then spiked, bottled and pasteurized, is described. Five main nutrients are involved in this study: ammonium, nitrite, nitrate, phosphate and silicate. Bottles are in glass for the ammonium samples and in plastic for the other nutrients. Pasteurization was performed at 80 ± 3 °C for 2 h. Samples were controlled for homogeneity and stability at 3–5 month interval, before and after the period allocated for each exercise and a third time...
Tipo: Text
Palavras-chave: Pasteurization; Nutrients; Seawater; Inter-laboratory exercises.
Ano: 2012
URL: http://archimer.ifremer.fr/doc/00058/16905/15066.pdf

Biofilms en mileu marin
Provedor de dados: 5
Autores: Compere, Chantal.
Introduction: Almost all submerged surfaces in the marine environment are subject to developing an organic film, with the exception of some living organisms, such as sponges, which do not undergo any great colonization, for no currently-known scientific reason. The presence of this biofilm is at the source of many problems in the oceanographic field and for marine business. This article introduces some drawbacks relating to the existence of this fouling and elaborates upon the main studies conducted at IFREMER concerning the most-used methods for combating it. However, the anti-fouling agents that are generally used for protecting facilities are toxic and can have disastrous consequences on the marine environment's fauna and flora. Moreover, the use of...
Tipo: Text
Palavras-chave: Biofilm; Seawater.
Ano: 1999
URL: http://archimer.ifremer.fr/doc/1999/publication-1698.pdf

Etude du phosphore dans les sédiments ostréicoles du bassin des Chasses des Sables d'Olonne
Provedor de dados: 5
Autores: Feuillet, Michèle.
Tipo: Text
Palavras-chave: Biscay bay; Oyster culture zone; Marine sediment; Seawater; Phosphorus.
Ano: 1971
URL: http://archimer.ifremer.fr/doc/1971/publication-2240.pdf

Performances of dead-end ultrafiltration of seawater: from the filtration and backwash efficiencies to the membrane fouling mechanisms
Provedor de dados: 5
Autores: Masse, Anthony; Arab, Oumnia; Sechet, Veronique; Jaouen, Pascal; Pontie, Maxime; Sabiri, Nour-eddine; Plantier, Severine.
The present work investigates the fouling mechanisms of PVDF hollow fibre membrane (0.03 μm) during the dead end ultrafiltration at a fixed permeate flux (outside to inside configuration) of complex synthetic seawater composed by humic acids, alginic acids, inorganic particles and numerous salts at high concentrations. Short term ultrafiltration experiments at 100 L.h-1.m-2 show that the optimal specific filtered volume seems to be equal to 50 L.m-2. A residual fouling resistance equal to 2.1010 m-1 is added after each cycle of filtration during 8h of ultrafiltration at 100 L.h-1.m-2 and 50 L.m-2. Most of the fouling is reversible (80%). Organics are barely (15% of humic acids) retained by the membrane. Backwash efficiency drops during operation which...
Tipo: Text
Palavras-chave: Seawater; Ultrafiltration; Fouling membrane; Alginic acids; Humic acids.
Ano: 2015
URL: http://archimer.ifremer.fr/doc/00286/39716/38172.pdf

An automated photo-oxidation method for the determination of dissolved organic phosphorus in marine and fresh water
Provedor de dados: 5
Autores: Aminot, Alain; Kerouel, Roger.
A segmented flow automated method with on-line photo-oxidation for the determination of dissolved organic phosphorus + soluble reactive phosphorus (DOP + SRP) in seawater and fresh water is described here. A low-power lamp was used for a compact, easy-to-handle and low-ozone-producing manifold. The influence of seawater matrix components was studied in detail using natural seawater and salt solutions spiked with DOP model compounds. Bromide was found to be the most inhibitory species in seawater. The work shows that most salt solutions referred to as artificial seawater are not satisfactory model matrices to test the actual seawater matrix effect. Since DOP recovered in undiluted seawater samples was about half that obtained in fresh water samples, the...
Tipo: Text
Palavras-chave: Measurement; Fresh water; Seawater; Total dissolved phosphorus; Dissolved organic phosphorus.
Ano: 2001
URL: http://archimer.ifremer.fr/doc/2001/publication-1678.pdf

Air-sea CO2 flux variability in frontal regions of the Southern Ocean from CARbon Interface OCean Atmosphere drifters
Provedor de dados: 5
Autores: Boutin, Jacqueline; Merlivat, L.; Henocq, C.; Martin, Nicolas; Sallee, Jean-baptiste.
Nine CARbon Interface OCean Atmosphere (CARIOCA) drifters were deployed in the Southern Ocean (south of the subtropical front, STF) between 2001 and 2006. They recorded 65 months of measurements in all seasons between 57 degrees S and 40 degrees S. Hydrological fronts detected by altimetry indicate that one buoy explored the polar zone (PZ) of the Atlantic Ocean and the western Indian Ocean; the remaining buoys explored the northern and southern parts of the subantarctic zone (SAZ) from the mid-Indian Ocean (73 degrees E) to the eastern Pacific Ocean (112 degrees W). The air-sea CO2 fluxes along the buoy trajectories are primarily driven by the spatial variability of the fugacity of CO2 in seawater, fCO(2): in the SAZ, they vary between -1.1 and -4.2 mol...
Tipo: Text
Palavras-chave: Antarctic circumpolar current; Northwestern mediterranean sea; Atlantic sector; Surface water; Gas exchange; Polar front; Temperature; Seawater; Transport.
Ano: 2008
URL: https://archimer.ifremer.fr/doc/00204/31483/29880.pdf

Multi-Element Determination of Trace Elements in Natural Water Reference Materials by ICP-SFMS after Tm Addition and Iron Co-precipitation
Provedor de dados: 5
Autores: Bayon, Germain; Birot, Dominique; Bollinger, Claire; Barrat, Jean Alix.
We report on an improved method for determining trace element abundances in seawater and other natural waters. The analytical procedure involves co-precipitation on iron hydroxides after addition of a Tm spike, and measurement by inductively coupled plasma-sector field mass spectrometry (ICP-SFMS). The validity of the method was assessed through a series of co-precipitation experiments, using ultra-diluted solutions of a certified rock reference material (BIR-1). Results obtained for four natural water reference materials (NASS-5, CASS-4, SLEW-3, SLRS-4) are in agreement with published working values for rare earth elements, yttrium, vanadium and, when available, for hafnium, zirconium, thorium and scandium. A set of proposed values with uncertainties...
Tipo: Text
Palavras-chave: Seawater; Reference material; ICP-MS; Trace elements; Rare earth elements; Eau de mer; Materiau de reference; ICP-MS; Elements traces; Terres Rares.
Ano: 2011
URL: http://archimer.ifremer.fr/doc/00031/14189/18000.pdf

Impact of granular filtration on ultrafiltration membrane performance as pre-treatment to seawater desalination in presence of algal blooms
Provedor de dados: 5
Autores: Sabiri, Nour-eddine; Sechet, Veronique; Jaouen, Pascal; Pontie, Maxime; Masse, Anthony; Plantier, Severine.
To mitigate fouling of the ultrafiltration (UF) membrane and improve permeate quality, we coupled granular filters (GF) with UF membrane as a pre-treatment for reconstituted seawater in the presence of algal bloom. Mono and bilayer granular filtrations were led at a mean velocity of 10 m h(-1) over a 7-hour period. Both GF gave the same algal cell retention rate (similar to 63%) after 7 hours of filtration. Turbidity reduction rate was 50% for the monolayer filter and 75% for the bilayer filter. Resulting organic matter removal rate was 10% for the monolayer filter and 35% for the bilayer filter. Dissolved organic carbon removal was low (20%) with the bilayer filter and non-existent with the monolayer filter. GF-coupled UF reduced humic acids in the...
Tipo: Text
Palavras-chave: Algal bloom; Fouling; Granular filtration; Pre-treatment; Seawater; Ultrafiltration.
Ano: 2018
URL: http://archimer.ifremer.fr/doc/00442/55315/56845.pdf

Mesure de la demande chimique en oxygène dans l'eau de mer.
Provedor de dados: 5
Autores: Michel, Pierre.
Introduction: Measuring the chemical oxygen demand (COD) is a way of determining the organic matter in water based on its oxidisibility by bichromate. The presence of organic matter in sea water is one of the factors that determines the productivity of the oceans: whether this organic matter will be absorbed directly or must first be transformed into nutritive substances by bacteria. This beneficial action also has its limits. On the one hand, consumption of organic matter remains limited; when it exceeds a certain rate, there is no longer any increase in productivity. On the other hand, the excess organic matter deteriorates by consuming the dissolved oxygen and thus competes with marine life. In extreme cases, this excess can cause the eutrophication of...
Tipo: Text
Palavras-chave: Methodology; Organic matter; Oxygen demand; Seawater.
Ano: 1972
URL: http://archimer.ifremer.fr/doc/1972/publication-2060.pdf

Bilan 1992 de la contamination des côtes françaises par les composés organostanniques
Provedor de dados: 5
Autores: Michel, Pierre; Averty, Bernard.
Au cours du printemps 1992, un échantillonnage systématique a permis d'évaluer le niveau de la contamination des côtes françaises par les composés organostanniques. Le tributyl étain (TBT) a été mesuré dans la phase dissoute avec ses produits de dégradation dibutyl étain (DBT) et monobutyl étain (MBT). Les concentrations mesurées restent importantes dans les zones portuaires et les zones de mélanges. Ces concentrations sont le plus souvent excessives lorsqu'on se réfère au seuil toxique de 1ng.1-1 pour lequel des effets sont connus sur l'huître et certains autres mollusques. Les trois façades maritimes françaises ont été contôlées ; c'est en Méditerranée que l'on peut observer les plus fortes concentrations. En plus du TBT et de ses métabolites, on a aussi...
Tipo: Text
Palavras-chave: Tributyl étain; Dibutyl étain; Monobutyl étain; Triphényl étain; Composés organostanniques; Eau de mer; France.; Tributyltin; Dibutyltin; Monobutyltin; Triphenyltin; Organotin compounds; Seawater; French coasts.
Ano: 1996
URL: http://archimer.ifremer.fr/doc/00104/21530/19111.pdf

A re-examination of matrix effects in the segmented-flow analysis of nutrients in sea and estuarine water
Provedor de dados: 5
Autores: Coverly, Stephen; Kerouel, Roger; Aminot, Alain.
Modern instruments together with the use of standard reference materials have improved the accuracy and long-term reproducibility of the analysis of nutrients (ammonium, nitrate, nitrite, phosphate and silicate) in sea water using segmented-flow analysis, so that errors arising from matrix effects become more significant. Colorimetric detectors with bubble-through flowcells have become widely used for seawater analysis in recent years and their associated matrix effects are described. A re-examination of all categories of matrix effects, whose main origin is salinity, was thus undertaken to assess how much they are liable to alter the data. Interferences were classified into four types, each of which was examined in order to show its influence on the...
Tipo: Text
Palavras-chave: Nutrient; Determination; Seawater; Estuarine water; Segmented-flow analysis; Matrix effects.
Ano: 2012
URL: http://archimer.ifremer.fr/doc/00057/16843/14530.pdf

C18 Sep-Pak extractable dissolved organic copper related to hydrochemistry in the North-West Mediterranean
Provedor de dados: 5
Autores: El Sayed, Mohamed A.; Aminot, Alain.
Extractable organic copper using C18 Sep-Pak cartridges was investigated in seawater after laboratory experiment showed that the (C18 Sep-Pak) cartridges were reliable, in open and coastal waters with normal levels of dissolved organic carbon, for the separation of a specific fraction of organo-copper complexes.Given that the Sep-Pak cartridges retain the hydrophobic fraction of the dissolved organic matter, this extraction technique was applied for studying the characteristics of this particular hydrophobic dissolved organic copper fraction (hDOCu) in the north-western Mediterranean waters. Surface distribution of hDOC is influenced by organic matter input from the river Rhone and its estuary as well as the physical processes affecting the primary...
Tipo: Text
Palavras-chave: Mediterranean sea; Seawater; Dissolved organic matter; Copper compounds.
Ano: 2000
URL: http://archimer.ifremer.fr/doc/2000/publication-1681.pdf

One-Single Extraction Procedure for the Simultaneous Determination of a Wide Range of Polar and Nonpolar Organic Contaminants in Seawater
Provedor de dados: 5
Autores: Fauvelle, Vincent; Castro-jimenez, Javier; Schmidt, Natascha; Carlez, Benoit; Panagiotopoulos, Christos; Sempere, Richard.
A rapid analytical method including one-single solid-phase extraction (SPE) procedure followed by gas and liquid chromatography coupled with high resolution mass spectrometry detection (GC-MS and LC-HRMS respectively) was developed for the quantification of 40 organic compounds (1.6 &lt; log K-ow &lt; 9.5) in seawater including both legacy and emerging contaminants, with a focus on the most common plastic organic additives. This new method allowed for the analyses of nine organophosphate esters (OPEs), seven phthalates (PAEs), six bisphenols (BPs), five perfluorinated compounds (PFCs), and thirteen legacy organochlorinated compounds (OCs, including polychlorobiphenyles and pesticides) with recoveries in the ranges of 57-124% for OPEs, 52-163% for PAEs,...
Tipo: Text
Palavras-chave: Plastic additive; Seawater; Organic contaminants; Legacy contaminants; Phtalates; Bisphenol; Organophosphate esters.
Ano: 2018
URL: https://archimer.ifremer.fr/doc/00645/75716/76697.pdf

Lessons learned from an intercalibration exercise on the quantification and characterisation of microplastic particles in sediment and water samples
Provedor de dados: 5
Autores: Cadiou, Jean-francois; Gerigny, Olivia; Koren, Š.; Zeri, C.; Kaberi, H.; Alomar, C.; Panti, C.; Fossi, M.c.; Adamopoulou, A.; Digka, N.; Deudero, S.; Concato, M.; Carbonell, A.; Baini, M.; Galli, M.; Galgani, Francois.
An intercalibration exercise on the characterisation of microplastics in marine sediment and water samples was carried out among five laboratories involved in the implementation of the Marine Strategy Framework Directive (MSFD) in their country. The samples were prepared by mixing cleaned natural sediment and sea water with microplastics sets made of particles of various polymers, shapes and colours. Overall, the errors on total counts were under 25% in absolute value. The risk of non-detection and loss of particles is greater than the risk of contamination during sample analysis. Significant differences are observed among particle types. It appears difficult to obtain reliable and comparable data on the colour of microplastics. A comparison of the errors...
Tipo: Text
Palavras-chave: Microplastics; Intercalibration; Protocols; Sediment; Seawater.
Ano: 2020
URL: https://archimer.ifremer.fr/doc/00622/73397/72812.pdf

Les microplastiques en milieu marin : supports de contaminants chimiques - Étude bibliographique
Provedor de dados: 5
Autores: Roclin, Lea.
microplastics are ubiquitous in the marine environment, particularly in ocean gyres. this review makes an assessment of the current knowledge about microplastics as support of chemical contaminants in marine environment. 121 papers were included in this report, with 53 on the theme "microplastics, contaminants and marine environment". adsorption and desorption capacities of contaminants on microplastic depend on the contaminant, the microplastic, and external factors (salinity, organic matter and interaction with other contaminants). regardless of the sampled matrix (water and sand) and the geographical area, results have shown the presence of chemical contaminants on microplastics, which are persistent organic pollutants (pops) in the water (pcbs, pahs,...
Tipo: Text
Palavras-chave: Microplastiques; Contaminants chimiques; Polluant organique persistant; Milieu marin; Microplastic; Chemical contaminant; Persistent organic pollutants; Seawater.
Ano: 2015
URL: http://archimer.ifremer.fr/doc/00278/38914/37454.pdf

Development of a mreB-targeted real-time PCR method for the quantitative detection of Vibrio harveyi in seawater and biofilm from aquaculture systems
Provedor de dados: 5
Autores: Mougin, Julia; Roquigny, Roxane; Travers, Marie-agnes; Grard, Thierry; Bonnin-jusserand, Maryse; Le Bris, Cédric.
Vibrio harveyi is a particularly problematic Gram-negative bacterium because it can form biofilms on aquaculture facility surfaces, leading to resistance of bacteria against antibiotics and water sanitizers. A SYBR Green I quantitative real-time PCR method was developed to detect V. harveyi directly from environmental samples, including seawater and biofilm. Specific primers targeting the mreB gene were designed. The exclusivity and inclusivity of the newly designed primers were evaluated using a panel of 85 bacteria: 58 V. harveyi from multiples origins and 27 non-V. harveyi isolates, and compared with two pairs of primers targeting the topA and toxR genes that were designed previously. All sets of primers were able to distinguish V. harveyi from closely...
Tipo: Text
Palavras-chave: Vibrio harveyi; Quantitative detection; MreB gene; Seawater; Biofilm; Aquaculture.
Ano: 2020
URL: https://archimer.ifremer.fr/doc/00622/73365/72542.pdf

Determination of iron-porphyrin-like complexes at nanomolar levels in seawater
Provedor de dados: 5
Autores: Vong, Lilita; Laes, Agathe; Blain, Stéphane.
A new method for the non-specific determination of iron-porphyrin-like complexes in natural waters has been developed. It is based on the chemiluminescent oxidation of the luminol in the presence of dioxygen (O-2) at pH 13. The method has been implemented in a FIA manifold that allowed the direct injection of seawater. The limit of detection is 0.11 nM of equivalent hemin (Fe-protoporphyrin IX). Fe2+, Fe3+, H2O2, siderophore (deferoxamin mesylate), humic acid and phytic acid did not interfere when the), were present at the concentrations expected in seawater. Metal free porphyrin and Mg, Cu, Co porphyrin complexes did not induce a significant chemiluminescent signal. Poisoned unfiltered samples could be stored for several weeks before analyses. The new...
Tipo: Text
Palavras-chave: Chemiluminescence; Complexation; Flow injection; Seawater; Porphyrin; Iron.
Ano: 2007
URL: http://archimer.ifremer.fr/doc/2007/publication-3298.pdf

Distribution of phthalates in Marseille Bay (NW Mediterranean Sea)
Provedor de dados: 5
Autores: Paluselli, Andrea; Fauvelle, Vincent; Schmidt, Natascha; Galgani, Francois; Net, Sopheak; Sempere, Richard.
Phthalic Acid Esters (PAEs) are a group of emerging organic contaminants that have become a serious issue because of their ubiquitous presence and hazardous impact on the marine environment worldwide. Seawater samples were collected monthly from December 2013 to November 2014 in the northwestern Mediterranean Sea (Marseille Bay). The samples were analyzed for dissolved organic carbon (DOC) as well as the molecular distribution of dissolved PAEs by using solid phase extraction followed by gas chromatography and mass spectrometry (GC/MS) analyses. The results demonstrated the occurrence of six PAEs, including dimethyl phthalate (DMP), diethyl phthalate (DEP), di-isobutyl phthalate (DiBP), di-n-butyl phthalate (DnBP), benzylbutyl phthalate (BzBP) and...
Tipo: Text
Palavras-chave: Phthalates; DEHP; DMP; Seawater; Dissolved organic matter; Endocrine disruptors.
Ano: 2018
URL: https://archimer.ifremer.fr/doc/00413/52482/53358.pdf

Adaptative responses of E-coli to marine environmental stresses. a modelling approach based on viability and dormancy concepts
Provedor de dados: 5
Autores: Martin, Y; Troussellier, Marc; Bonnefont, Jl.
In an attempt to synthesize conceptual and experimental information on the behaviour of enteric bacteria in seawater, a mathematical model has been developed. This model is based on changes in intracellular metabolisable components depending an physiological responses of the cell when subjected to nutrient starvation, salinity stress and solar radiation. Following a strategy which takes into account short- and mid-term physiological adaptation and reversal processes, the cells can develop in different states: culturable (B-1), viable and definitively nonculturable (B-2), and reversibly dormant (B-3) cells. Model parameters were deduced either from original microcosm experiments, from literature data or calibration procedures. Validation of the model was...
Tipo: Text
Palavras-chave: Escherichia coli; Eau de mer; Stress; États cellulaires; Modélisation; Escherichia coli; Seawater; Stress; Cellular states; Modelling.
Ano: 1998
URL: http://archimer.ifremer.fr/doc/00325/43646/43224.pdf

Consequences of radioactive releases into the sea resulting from the accident at the Fukushima Dai-ichi nuclear power plant - Evolution of expert investigation according to the data available
Provedor de dados: 5
Autores: Laguionie, Philippe; Bailly-du-bois, Pascal; Boust, D.; Fievet, B.; Garreau, Pierre; Connan, O.; Charmasson, Sabine; Arnaud, M.; Duffa, Celine; Champion, D.
The accident at the Fukushima Dai-ichi Nuclear Power Plant (FDNPP) in March 2011 led to an unprecedented direct input of artificial radioactivity into the marine environment. The Institute for Radioprotection and Nuclear Safety was requested by the French authorities to investigate the radioecological impact of this input, in particular the potential contamination of products of marine origin used for human consumption. This article describes the close link between the responses provided and the availability of the data, as well as their nature and ability to meet the requirements of expert investigation. These responses were needed: (i) to evaluate the inputs of radionuclides into the marine environment, (ii) to understand their dispersion in seawater,...
Tipo: Text
Palavras-chave: Nuclear power plant; Accident analysis; Seawater; Sediment; Biota.
Ano: 2012
URL: http://archimer.ifremer.fr/doc/00096/20690/18353.pdf

Devenir des virus entériques en mer et influence des facteurs environnementaux
Provedor de dados: 5
Autores: Gantzer, Christophe; Dubois, Éric; Crance, Jean-marc; Billaudel, Sylviane; Kopecka, Helena; Schwartzbrod, Louis; Pommepuy, Monique; Le Guyader, Françoise.
To improve the knowledge of the survival of enteric viruses in a marine environment, the influence of physico-chemical parameters (temperature, UV, salinity) on the survival of infectious poliovirus 1 and hepatitis A Virus (HAV) in seawater was first studied, the influence of suspended solids (SS) on poliovirus adsorption and survival in seawater was then evaluated and the detection of rotavirus genome in environmental samples (shellfish, river water, treated wastewater) was finally investigated. The results show that temperature has a major impact on virus survival in seawater as the time necessary to inactivate 90 % of the virus (T-90) is 671 days at 4 degrees C and only 25 days at 25 degrees C. Ultraviolet light (42 mW s cm(-2)) rapidly inactivates...
Tipo: Text
Palavras-chave: Environmental factors; Survival; Seawater; Enteric viruses; Facteurs environnementaux; Survie; Eau de mer; Virus entériques.
Ano: 1998
URL: http://archimer.ifremer.fr/doc/1998/publication-846.pdf

Rotavirus VLP2/6: a new tool for tracking rotavirus in the marine environment
Provedor de dados: 5
Autores: Loisy, Fabienne; Atmar, Robert L.; Cohen, Jean; Bosch, Albert; Le Guyader, Soizick.
The potential of rotavirus 2/6-virus-like-particles (VLP2/6) for use as tracers in the marine environment was investigated. The stability of bovine rotavirus (strain RF) and VLP2/6 in natural seawater at 25degreesC for six days was studied. ELISA and western blot methods were used to quantify the particles. The rates of decline of rotavirus particles and VLP2/6 were similar (approximately 0.5 log 10 per day). Western blot analysis showed that the integrity of capsid proteins VP2 and VP6 was conserved during the incubation time. These results demonstrate that VLP2/6 particles have the same stability in seawater as rotavirus particles. Thus, VLP2/6 can be used as a tracer, which should be of particular value for studying the fate of rotavirus particles in...
Tipo: Text
Palavras-chave: Stability; Tracer; Seawater; Virus like particles; Rotavirus.
Ano: 2004
URL: https://archimer.ifremer.fr/doc/2004/publication-330.pdf

Sulfide determination in hydrothermal seawater samples using a vibrating gold micro-wire electrode in conjunction with stripping chronopotentiometry
Provedor de dados: 5
Autores: Aumond, Virginie; Waeles, Mathieu; Salaun, Pascal; Gibbon-walsh, Kristoff; Van Den Berg, Constant M. G.; Sarradin, Pierre-marie; Riso, Ricardo D.
A rapid electrochemical stripping chronopotentiometric procedure to determined sulfide in unaltered hydrothermal seawater samples is presented. Sulfide is deposited at -0.25 V (vs Ag/AgCl, KCl 3 M) at a vibrating gold microwire and then stripped through the application of a reductive constant current (typically -2 mu A). The hydrodynamic conditions are modulated by vibration allowing a short deposition step, which is shown here to be necessary to minimize H2S volatilization. The limit of detection (LOD) is 30 nM after a deposition step of 7s. This LOD is in the same range as the most sensitive cathodic voltammetric technique using a mercury drop electrode and is well below those reported previously for other electrodes capable of being implemented in situ....
Tipo: Text
Palavras-chave: Sulfide; Stripping chronopotentiometry; Vibrating electrode; Gold; Seawater; Hydrothermal.
Ano: 2012
URL: http://archimer.ifremer.fr/doc/00111/22222/20065.pdf

High-precision measurements of seawater Pb isotope compositions by double spike thermal ionization mass spectrometry
Provedor de dados: 5
Autores: Paul, Maxence; Bridgestock, Luke; Rehkaemper, Mark; Van Deflierdt, Tina; Weiss, Dominik.
A new method for the determination of seawater Pb isotope compositions and concentrations was developed, which combines and optimizes previously published protocols for the separation and isotopic analysis of this element. For isotopic analysis, the procedure involves initial separation of Pb from 1 to 2 L of seawater by co-precipitation with Mg hydroxide and further purification by a two stage anion exchange procedure. The Pb isotope measurements are subsequently carried out by thermal ionization mass spectrometry using a Pb-207-Pb-204 double spike for correction of instrumental mass fractionation. These methods are associated with a total procedural Pb blank of 28 +/- 21 pg(1sd) and typical Pb recoveries of 40-60%. The Pb concentrations are determined by...
Tipo: Text
Palavras-chave: Seawater; Lead isotope; Double spike; Thermal ionization mass spectrometry; GEOTRACES; Inter-calibration.
Ano: 2015
URL: https://archimer.ifremer.fr/doc/00351/46268/46051.pdf

Seawater accelerated ageing of poly(3-hydroxybutyrate-co-3-hydroxyvalerate
Provedor de dados: 5
Autores: Deroine, Morgan; Le Duigou, Antoine; Corre, Yves-marie; Le Gac, Pierre-yves; Davies, Peter; Cesar, Guy; Bruzaud, Stephane.
The aim of this study is to establish a baseline for poly(3-hydroxybutyrate-co-3-hydroxyvalerate) (PHBV) lifetime prediction in a marine environment, by means of mechanical and physico-chemical characterization of specimens immersed in continuously renewed and filtered natural seawater in the laboratory at different temperatures (4, 25 and 40°C). Samples were also aged at sea in Lorient harbour in order to compare laboratory and natural degradation mechanisms and kinetics. Due to its morphology, hydrolysis of PHBV in natural seawater is quite slow, and samples were observed to undergo preferentially an enzymatic surface degradation. Increasing the aging temperature in the laboratory promotes the water uptake and causes hydrolysis. As two degradation...
Tipo: Text
Palavras-chave: Poly(3-hydroxybutyrate-co-3-hydroxyvalerate); Accelerated ageing; Hydrothermal degradation; Seawater.
Ano: 2014
URL: http://archimer.ifremer.fr/doc/00188/29972/28425.pdf

Influence of Sea Water Aging on the Mechanical Behaviour of Acrylic Matrix Composites
Provedor de dados: 5
Autores: Davies, Peter; Le Gac, Pierre-yves; Le Gall, Maelenn.
A new matrix resin was recently introduced for composite materials, based on acrylic resin chemistry allowing standard room temperature infusion techniques to be used to produce recyclable thermoplastic composites. This is a significant advance, particularly for more environmentally-friendly production of large marine structures such as boats. However, for such applications it is essential to demonstrate that composites produced with these resins resist sea water exposure in service. This paper presents results from a wet aging study of unreinforced acrylic and glass and carbon fibre reinforced acrylic composites. It is shown that the acrylic matrix resin is very stable in seawater, showing lower property losses after seawater aging than those of a...
Tipo: Text
Palavras-chave: Acrylic; Thermoplastic; Infusion; Seawater; Immersion.
Ano: 2017
URL: http://archimer.ifremer.fr/doc/00347/45815/45541.pdf

Fatigue resistance of natural rubber in seawater with comparison to air
Provedor de dados: 5
Autores: Ulu, K. Narynbek; Huneau, B.; Le Gac, Pierre-yves; Verron, E.
Fatigue properties of filled natural rubber in seawater environment are investigated by uniaxial fatigue and crack propagation experiments, and the damage is analyzed by scanning electron microscopy. The behavior under relaxing and non-relaxing loading conditions is studied and the results are compared to those obtained in air environment. For relaxing loading conditions, fatigue behavior is the same in both environments. Under non-relaxing conditions at large strain levels, for which the influence of strain-induced crystallization is important, fatigue life is longer in seawater. Such behavior could be explained by increased internal temperatures of specimens tested in air due to lower heat conductivity of air as compared to seawater. Such conclusion is...
Tipo: Text
Palavras-chave: Natural rubber; Fatigue; Environmental effects; Seawater; Strain-induced crystallization.
Ano: 2016
URL: http://archimer.ifremer.fr/doc/00324/43523/43055.pdf

Polychloroprene behaviour in a marine environment: Role of silica fillers
Provedor de dados: 5
Autores: Tchalla, Siwavi Tatiana; Le Gac, Pierre-yves; Maurin, R.; Creac'Hcadec, R.
Polychloroprene rubbers are widely used in marine structures and often filled with silica in order to increase mechanical properties. The presence of silica fillers leads to a complex degradation of the material. This study aims to understand the deeper degradation mechanisms involved when a silica filled polychloroprene is used in sea water. To do so, 4 polychloroprene rubbers filled with different amounts of silica (from 0 to 45 phr) were aged in natural sea water for 6 months at temperatures ranging from 25 to 60 °C. Moreover, a natural rubber with similar formulation was also considered in order to evaluate the role of the chlorine atom in the degradation. . The chemistry and mechanics of the rubber degradation were also studied. In the presence of...
Tipo: Text
Palavras-chave: Polychloroprene; Seawater; Silica filler; Hydrolysis.
Ano: 2017
URL: http://archimer.ifremer.fr/doc/00376/48689/49020.pdf

Fatigue Behaviour of Acrylic Matrix Composites: Influence of Seawater
Provedor de dados: 5
Autores: Davies, Peter; Arhant, Mael.
The recent introduction of liquid acrylic thermoplastic matrix resins which can impregnate fibre reinforcements using traditional infusion moulding offers significant potential for future composite structures in marine applications, such as marine energy devices. However, to date very few results are available to evaluate the long term durability of these composites in a marine environment. This paper describes results from a series of cyclic loading tests on glass and carbon fibre reinforced acrylic composites under both tension and four point flexural loading. Tests were performed before and after aging in natural seawater. The results were compared to results for a glass/epoxy used today in marine structures, and show a lower loss of both static and...
Tipo: Text
Palavras-chave: Acrylic; Fatigue; Immersion; Seawater.
Ano: 2019
URL: https://archimer.ifremer.fr/doc/00444/55596/57249.pdf

Advances in measuring ocean salinity with an optical sensor
Provedor de dados: 5
Autores: Le Menn, Marc; De La Tocnaye, J. L. De Bougrenet; Grosso, P.; Delauney, Laurent; Podeur, Christian; Brault, P.; Guillerme, O.
Absolute salinity measurement of seawater has become a key issue in thermodynamic models of the oceans. One of the most direct ways is to measure the seawater refractive index which is related to density and can therefore be related to the absolute salinity. Recent advances in high resolution position sensitive devices enable us to take advantage of small beam deviation measurements using refractometers. This paper assesses the advantages of such technology with respect to the current state-of-the-art technology. In particular, we present the resolution dependence on refractive index variations and derive the limits of such a solution for designing seawater sensors well suited for coastal and deep-sea applications. Particular attention has been paid to...
Tipo: Text
Palavras-chave: Refractive index; Seawater; Density; Salinity; Refractometer.
Ano: 2011
URL: http://archimer.ifremer.fr/doc/00052/16295/13899.pdf

Evaluation of Basalt Fibre Composites for Marine Applications
Provedor de dados: 5
Autores: Davies, Peter; Verbouwe, W.
Basalt fibres offer potential for use in marine structures, but few data exist to evaluate the influence of seawater immersion on their mechanical behaviour. This paper provides the results from a study in which basalt fibre reinforced epoxy composites were aged in natural seawater at different temperatures. Tests were performed under quasi-static and cyclic loading, first in the as-received state then after saturation in natural seawater. Results are compared to those for an E-glass reinforced composite with the same epoxy matrix. They indicate similar mechanical performance for both materials after seawater saturation.
Tipo: Text
Palavras-chave: Seawater; Aging; Fatigue; Basalt fibre; Epoxy; Unidirectional; Flexure.
Ano: 2018
URL: http://archimer.ifremer.fr/doc/00392/50385/51111.pdf

Kinetics of conditioning layer formation on stainless steel
Provedor de dados: 5
Autores: Compere, Chantal; Bellon Fontaine, M.-n.; Bertrand, P; Costa, D; Marcus, P; Poleunis, C; Pradier, C.m.; Rondot, B; Walls, M.g.
Adhesion of micro-organisms to surfaces in marine environments leads to biofouling. The deleterious effects of biofilm growth in the marine environment are numerous and include : energy losses due to increased fluid frictional resistance or to increased heat transfer resistance, risk of corrosion induced by micro-organisms, loss of optical properties, quality control and safety problems. Antifouling agents are generally used to protect surfaces from being affected by such a biofilm. These agents are toxic and can be persistent, causing harmful environmental and ecological effects. Moreover, the use of biocides and regular cleaning considerably increase the maintenance costs of marine industries. An improved knowledge of the biofilm adhesion mechanisms is...
Tipo: Text
Palavras-chave: Biofilm; Surface characterisation; Carbohydrates; Protein; Seawater; Conditioning layer.
Ano: 2001
URL: http://archimer.ifremer.fr/doc/2001/publication-1701.pdf

Measurement of the isotopic composition of dissolved iron in the open ocean
Provedor de dados: 5
Autores: Lacan, F.; Radic, A.; Jeandel, C.; Poitrasson, F.; Sarthou, Geraldine; Pradoux, C.; Freydier, R.
This work demonstrates for the first time the feasibility of the measurement of the isotopic composition of dissolved iron in seawater for a typical open ocean Fe concentration range (0.1-1 nM). It also presents the first data of this kind. Iron is preconcentrated using a Nitriloacetic Acid Superflow resin and purified using an AG1x4 anion exchange resin. The isotopic ratios are measured with a MC-ICPMS Neptune, coupled with a desolvator (Aridus II), using a Fe-57-Fe-58 double spike mass bias correction. Measurement precision (0.13%, 2SD) allows resolving small iron isotopic composition variations within the water column, in the Atlantic sector of the Southern Ocean (from delta Fe-57 = -0.19 to +0.32 parts per thousand). Isotopically light iron found in...
Tipo: Text
Palavras-chave: MC ICP MS; Chelating resin; Southern ocean; Fractionation; Seawater; Earth; Separation; Accuracy; Pacific; FE(III).
Ano: 2008
URL: https://archimer.ifremer.fr/doc/00202/31374/29781.pdf

Determination of the copper isotope composition of seawater revisited: A case study from the Mediterranean Sea
Provedor de dados: 5
Autores: Baconnais, Isabelle; Rouxel, Olivier; Dulaquais, Gabriel; Boye, Marie.
A new technique for the determination of dissolved copper isotope composition (δ65Cu) of seawater was applied to examine copper sources and internal cycling in the Mediterranean Sea. A succession of chelating resin with nitrilotriacetic acid functional groups and strong base anion exchange resin, together with optimization of the multi-collector inductively coupled plasma mass spectrometry set-up allowed to isolate copper from seawater matrix and to measure the 65Cu/63Cu ratios in seawater with an external precision of 0.06‰ (2 s.d.). This method was first applied for inter-comparison measurements to surface and deep waters sampled at station BATS in the North Atlantic Ocean. Disparities in δ65Cu reported here and in the literature over these samples...
Tipo: Text
Palavras-chave: Copper isotope; Seawater; Mediterranean Sea; Geotraces; Isotope fractionation.
Ano: 2019
URL: https://archimer.ifremer.fr/doc/00457/56880/58742.pdf

Trace element behaviour at cold seeps and the potential export of dissolved iron to the ocean
Provedor de dados: 5
Autores: Lemaitre, Nolwenn; Bayon, Germain; Ondreas, Helene; Caprais, Jean-claude; Freslon, Nicolas; Bollinger, Claire; Rouget, Marie-laure; De Prunele, Alexis; Ruffine, Livio; Olu-le Roy, Karine; Sarthou, Geraldine.
Seawater samples were collected by submersible above methane seeps in the Gulf of Guinea (Regab and Baboon pockmarks) in order to investigate the behaviour of iron (Fe), manganese (Mn) and rare earth elements (REE) during fluid seepage. Our aim was to determine whether cold seeps may represent potential sources of dissolved chemical species to the ocean. Dissolved (&lt;0.45 μm filtered samples) and total dissolvable (unfiltered samples) concentrations were determined over ∼50 m long vertical transects above the seafloor and at various discrete locations within the pockmarks. We show that substantial amounts of Fe and Mn are released into seawater during seepage of methane-rich fluids. Mn is exported almost quantitatively in the dissolved form (more than...
Tipo: Text
Palavras-chave: Iron; Rare earth elements; Cold seeps; Seawater; Organic ligands; Iron-sulfide nanoparticles.
Ano: 2014
URL: http://archimer.ifremer.fr/doc/00211/32190/30704.pdf

Analyse, distribution, production et dégradation d’esters de phtalates (PAEs) en zone côtière méditerranéenne
Provedor de dados: 5
Autores: Paluselli, Andrea.
Phthalic Acid Esters (PAEs) are a group of emerging organic contaminants that have become a serious issue because of their ubiquitous presence on the marine environment worldwide and for the endocrine disrupting effects in animals and humans. However, little is known about their distribution in the Ocean, mainly because of analytical difficulties and the high possibility of ambient sample contamination. Plastic debris in marine environment includes resin pellets, macro- and microplastic fragments, and contains additives such as PAEs that might be released in the aquatic environment in unknown proportion. In our work, we improved an analytical method for the determination of 8 PAEs, at trace levels in marine and fresh waters. In the first part of the...
Tipo: Text
Palavras-chave: Phtalates; DEHP; Eau de mer; Perturbateurs endocriniens; Microplastiques; Microplastics; Endocrine disruptors; Seawater; Phthalates; Dehp.
Ano: 2018
URL: https://archimer.ifremer.fr/doc/00497/60904/64252.pdf

A mid-Holocene transition in the nitrogen dynamics of the western equatorial Pacific: Evidence of a deepening thermocline?
Provedor de dados: 5
Autores: Kienast, M.; Lehmann, M. F.; Timmermann, A.; Galbraith, E.; Bolliet, T.; Holboum, A.; Normandeau, C.; Laj, C.
Sedimentary delta(15)N records from the oligotrophic western equatorial Pacific (WEP) off Mindanao show that late Holocene sedimentary delta(15)N is substantially lower than that of the early Holocene, following a gradual &gt;3 parts per thousand decrease that occurred between 7 and 3 kyrs ago. Analyses of modem day nitrate isotope profiles from the same region indicate the sensitivity of the WEP N pools towards (1) the advection of (15)N-enriched nitrate from the Eastern Equatorial Pacific (EEP) by the North Equatorial Current (NEC) and the Mindanao Current in subsurface waters and, (2) at shallow depths, the input of new and (15)N-depleted nitrate through N, fixation. We suggest that the Holocene decrease in sedimentary delta(15)N reflects a diminished...
Tipo: Text
Palavras-chave: Tropical Pacific; El Nino; Surface temperature; Fresh water; Nitrate; Mindanao; Ocean; Variability; Holocene; Seawater.
Ano: 2008
URL: https://archimer.ifremer.fr/doc/00207/31843/30257.pdf

TRANSMER, un modèle hydrodynamique rapide et précis pour la simulation à moyen et long terme des transferts de radionucléides en Manche et dans le sud de la Mer du Nord
Provedor de dados: 5
Autores: Bailly Du Bois, Pascal; Dumas, Franck.
TRANSMER hydrodynamic model simulates dispersion of dissolved substances in seawater at the scale of the English Channel and the south of the North Sea with a mesh size of one kilometre and a time step of 30 minutes. It has been qualitatively and quantitatively validated by 1400 measurement of 125Sb in seawater. This model evaluates the medium- and long-term consequences of releases of soluble pollutants in the marine ecosystem under normal or accidental conditions, at a very low computation cost (it takes less than one hour to simulate one year).
Tipo: Text
Palavras-chave: English Channel; North Sea; Radionuclide; Concentration; Dispersion; Dissolved substances; Seawater; Hydrodynamic model; Modèle; Sb 125; Dispersion; Mer du Nord; Manche.
Ano: 2004
URL: http://archimer.ifremer.fr/doc/2004/acte-563.pdf

Determination of rare earth elements and other trace elements (Y, Mn, Co, Cr) in seawater using Tm addition and Mg(OH)(2) co-precipitation
Provedor de dados: 5
Autores: Freslon, Nicolas; Bayon, Germain; Birot, Dominique; Bollinger, Claire; Barrat, Jean-alix.
This paper reports on a novel procedure for determining trace element abundances (REE and Y, Cr, Mn, Co) in seawater by inductively coupled plasma sector field mass spectrometry (ICP-SFMS). The procedure uses a combination of pre-concentration using co-precipitation onto magnesium hydroxides and addition of thulium spike. The validity of the method was assessed onto 25 ml volumes of certified reference materials (NASS- and CASS-4) and in house seawater standard. Procedural blanks were determined by applying the same procedure to aliquots of seawater previously depleted in trace elements by successive Mg(OH)(2) co-precipitations, yielding estimated contributions to the studied samples better than 1.1% for all elements, with the exception of Cr (&lt;3.3%)...
Tipo: Text
Palavras-chave: Trace elements; Rare earth elements (REE); Seawater; Mg(OH)(2) co-precipitation; ICP-MS; Thulium.
Ano: 2011
URL: http://archimer.ifremer.fr/doc/00041/15220/15855.pdf

Trace metals assessment in water, sediment, mussel and seagrass species - Validation of the use of Posidonia oceanica as a metal biomonitor
Provedor de dados: 5
Autores: Lafabrie, Céline; Pergent, G; Kantin, Roger; Pergent Martini, C; Gonzalez, Jean-louis.
The accumulation of trace metals (Cd, Co, Cr, Hg, Ni and Pb) was measured in water, sediment, the mussel Mytilus galloprovincialis and the seagrass Posidonia oceanica. Samples were collected in three locations of the north-western Mediterranean (Canari, Livorno and Porto-Torres) which present different levels and sources of human impact. Analyses in the different compartments (water, sediment, M. galloprovincialis and P. oceanica) have allowed to identify Canari as the most Cd, Co, Cr and Ni contaminated site; Livorno as the most Hg contaminated and Porto-Torres as the most Pb contaminated. Furthermore, for the first time, metal concentrations found in P. oceanica have been compared with those found in the water column, in the sediment and in the...
Tipo: Text
Palavras-chave: Mediterranean sea; Marine organisms; Sediment; Seawater; Biomonitoring; Metal contamination.
Ano: 2007
URL: http://archimer.ifremer.fr/doc/2007/publication-3106.pdf

Développement et essais d’un salinomètre optique pour l’océanographie
Provedor de dados: 5
Autores: Le Menn, Monique; Malardé, Damien; David, Arnaud; Brault, Patrice; Grosso, Philippe; De Bougrenet De La Tocnaye, Jean-louis; Le Reste, Serge; Podeur, Christian.
Salinity is the essential parameter for ocean dynamics studies. Its definition and using in the equations used to calculate the thermodynamic properties of seawater, were revised in 2010, opening the possibility of new sensors developments. In this context, NOSS (NKE Optical Salinity Sensor) has emerged as one of the first underwater instrument for in situ refractive index measurement in the past years open up the scope of possibilities to access to density parameter. This achievement is the fruit of the cooperation between several institutions and the fruit of several years of developments and trials. NOSS sensor is designed to be deployed in coastal environment and open-ocean waters up to 2000m, especially on profiling floats of the Argo network.
Tipo: Text
Palavras-chave: Salinity; Density; Ocean; Seawater; Refractive index; Sensor.
Ano: 2016
URL: https://archimer.ifremer.fr/doc/00664/77601/79616.pdf

Analysis of hydrogen and methane in seawater by “Headspace” method: Determination at trace level with an automatic headspace sampler
Provedor de dados: 5
Autores: Donval, Jean-pierre; Guyader, Vivien.
“Headspace” technique is one of the methods for the onboard measurement of hydrogen (H2) and methane (CH4) in deep seawater. Based on the principle of an automatic headspace commercial sampler, a specific device has been developed to automatically inject gas samples from 300 ml syringes (gas phase in equilibrium with seawater). As valves, micro pump, oven and detector are independent, a gas chromatograph is not necessary allowing a reduction of the weight and dimensions of the analytical system. The different steps from seawater sampling to gas injection are described. Accuracy of the method is checked by a comparison with the “purge and trap” technique. The detection limit is estimated to 0.3 nM for hydrogen and 0.1 nM for methane which is close to the...
Tipo: Text
Palavras-chave: Gas; Seawater; Headspace method.
Ano: 2017
URL: http://archimer.ifremer.fr/doc/00354/46523/46287.pdf

Adsorption of norovirus and ostreid herpesvirus type 1 to polymer membranes for the development of passive samplers
Provedor de dados: 5
Autores: Hubert, Francoise; Morga, Benjamin; Renault, Tristan; Le Guyader, Soizick.
Aims  This study was performed to develop passive sampling methodology for the detection of two viruses in seawater in the area of shellfish production, The Norovirus (NoV), a human pathogen implicated in gastroenteritis outbreaks linked to oyster consumption and the ostreid herpesvirus type 1 (OsHV-1) a virus associated with mass mortalities of Pacific oysters. Methods and Results  Commercially membranes were tested for their capacity to adsorb virus: Zetapor, gauze, nylon, low density polyethylene (LDPE) and Polyvinylidene difluoride (PVDF). Laboratory exposures of membranes to contaminated water samples (stool, sewage, seawater) were performed. Our data shown that the amount of NoV GII genome per membrane measured with qRT-PCR increased with the time of...
Tipo: Text
Palavras-chave: Norovirus; OsHV-1; Pacific oysters; Passive samplers; Seawater; Sewage.
Ano: 2017
URL: http://archimer.ifremer.fr/doc/00365/47646/47670.pdf

Influence of Seawater Ageing on Fracture of Carbon Fiber Reinforced Epoxy Composites for Ocean Engineering
Provedor de dados: 5
Autores: Le Guen-geffroy, Antoine; Davies, Peter; Le Gac, Pierre Yves; Habert, Bertrand.
Carbon fiber reinforced composite materials are finding new applications in highly loaded marine structures such as tidal turbine blades and marine propellers. Such applications require long-term damage resistance while being subjected to continuous seawater immersion. However, few data exist on which to base material selection and design. This paper provides a set of results from interlaminar fracture tests on specimens before and after seawater ageing. The focus is on delamination as this is the main failure mechanism for laminated composites under out-of-plane loading. Results show that there are two contributions to changes in fracture toughness during an accelerated wet ageing program: effects due to water and effects due to physical ageing. These are...
Tipo: Text
Palavras-chave: Composite; Delamination; Seawater; Immersion; Ageing.
Ano: 2020
URL: https://archimer.ifremer.fr/doc/00652/76410/77458.pdf

Evidence for intense REE scavenging at cold seeps from the Niger Delta margin
Provedor de dados: 5
Autores: Bayon, Germain; Birot, Dominique; Ruffine, Livio; Caprais, Jean-claude; Ponzevera, Emmanuel; Bollinger, C.; Donval, Jean-pierre; Charlou, Jean-luc; Voisset, Michel; Grimaud, S.
For many trace elements, continental margins are the location of intense exchange processes between sediment and seawater, which control their distribution in the water column, but have yet to be fully understood. In this study, we have investigated the impact of fluid seepage at cold seeps on the marine cycle of neodymium. We determined dissolved and total dissolvable (TD) concentrations for REE and well-established tracers of fluid seepage (CH4, TDFe, TDMn), and Nd isotopic compositions in seawater samples collected above cold seeps and a reference site (i.e. away from any fluid venting area) from the Niger Delta margin. We also analyzed cold seep authigenic phases and various core-top sediment fractions (pore water, detrital component, easily leachable...
Tipo: Text
Palavras-chave: Rare earth elements; Neodymium isotopes; Seawater; Cold seeps; Fe-Mn oxyhydroxides; Benthic fluxes.
Ano: 2011
URL: http://archimer.ifremer.fr/doc/00066/17754/15571.pdf

Estudios sobre factores que afectan la calidad de la merluza fresca
Provedor de dados: 20
Autores: Avdalov, Nelson.
Among other results, it was found that when hake is handied property it maintains good quality levels up to 10 days after catch, irrespective of season. Its total storage life in boxes with ice is approximately two weeks. Although total storage life remained unchanged, it was found that quality levels tended to be significantly higher if overfilling of boxes was avoided, if the fish was gutted immediately after catch, or if hake was stored in containers with seawater.
Tipo: Report
Palavras-chave: Quality control; Fish storage; Seawater; Gutting; Cold storage.
Ano: 1982
URL: http://hdl.handle.net/1834/4903

Efecto de diferentes densidades de siembra en el engorde de tilapia roja  (Oreochromis mossambicus x O. aureus) en jaulas colocadas en la bahía  de Casilda, Cuba
Provedor de dados: 20
Autores: Fraga, I.; Flores, E. R.; Reyes, R.; Llanes, Y.
Con el objetivo de evaluar el efecto sobres el crecimiento y la supervivencia, de diferentes densidades de siembra de tilapia  roja en jaulas de diferentes volúmenes (4, 6 y 16 m3) se desarrollaron tres ciclos de engorde en la bahía de Casilda, provincia  Sancti-Spíritus. La selección del sitio se realizó a partir de una red de cinco estaciones muestreadas en lluvia y seca para  determinar los parámetros físico, químicos, batimétricos y turbidez. Los alevines se adaptaron al agua de mar en tanques de  12 m3, con flujo de agua marina (1.4 - 2.8 L/segundo) durante 24 horas con supervivencia de 96%. Al emplear densidades de  73 y 184 alevines/m3 en jaulas de 6 m3, no se observaron diferencias significativas (p&gt; 0.05) en el crecimiento y  supervivencias...
Tipo: Journal Contribution
Palavras-chave: Food; Seawater; Stock density; Cages; Environmental impact; Yield.
Ano: 2012
URL: http://hdl.handle.net/1834/4334

SALT TOLERANT PLANTS AS A VALUABLE RESOURCE FOR SUSTAINABLE FOOD PRODUCTION IN ARID AND SALINE COASTAL ZONES
Provedor de dados: 37
Autores: HOLGUIN PEÑA,Ramón Jaime; MEDINA HERNÁNDEZ,Diana; GHASEMI,Mojtaba; RUEDA PUENTE,Edgar Omar.
ABSTRACT This review focuses on the potential of halophytes for food, fodder and biofuels production, as well as their impacts on the environment and societies. Moreover, to open new areas in production systems using novel technologies such as halophytes in a desert agriculture. We are faced with the crisis and the shortage of freshwater in arid, semi-arid and desert regions. For this reason, we have to apply sustainable systems for human food, fodder and biofuels. Halophytes are naturally resistant to salt and develop on the coastal coast and arid-saline areas. We present a complete summary of the current situation of human population growth and food demand, a sustainable alternative such as halophilic crops of agro-industrial importance compared with...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Bioprospecting; Halophyte; Seawater.
Ano: 2021
URL: http://www.scielo.org.co/scielo.php?script=sci_arttext&pid=S0120-548X2021000100116

ALLEVIATION OF SALINITY STRESS ON Vicia faba L. PLANTS VIA SEED PRIMING WITH MELATONIN
Provedor de dados: 37
Autores: DAWOOD,Mona Gergis; EL-AWADI,Mohamed E.
Melatonin is an environmentally friendly-molecule with a potent free radical scavenger and antioxidant capacity. Two pot experiments were conducted during two successive winter seasons (2011/2012 and 2012/2013) at the wire-house of the National Research Centre, Dokki, Cairo, Egypt to study the potentiality of melatonin (100 mM and 500 mM) in alleviating the harmful effect of diluted seawater at a relatively low and high concentrations (3.85 dS/m and 7.69 dS/m, respectively) on the performance of faba bean plants. The results revealed that irrigation of faba bean plants with diluted seawater reduced growth parameters (plant height, leaves number/plant, fresh and dry weights of plant), relative water content (RWC), photosynthetic pigments (chlorophylls a, b...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Indole acetic acid; Legumes; Minerals; N-acetyl-5-methoxytryptamine; Protein patterns; Seawater.
Ano: 2015
URL: http://www.scielo.org.co/scielo.php?script=sci_arttext&pid=S0120-548X2015000200022

New bioemulsifiers produced by Candida lipolytica using D-glucose and babassu oil as carbon sources
Provedor de dados: 58
Autores: Vance-Harrop,Mabel H.; Gusmão,Norma B. de; Campos-Takaki,Galba Maria de.
Candida lipolytica IA 1055 produced extracellular biosurfactants with emulsification activity by fermentation using babassu oil and D-glucose as carbon sources. Natural seawater diluted at 50% supplemented with urea, ammonium sulfate, and phosphate was used as economic basal medium. The best results were achieved with the YSW-B2 medium, which contained urea, ammonium sulfate, and babassu oil and with YSW-B3 medium, which contained urea, ammonium sulfate, phosphate, and babassu oil, kept under fed batch fermentation for 60 hours with 5% of babassu oil. For the two media, the maximum specific growth rates were 0.02 h-1 and 0.04 h-1; the generation times were 34.6 h-1 and 17.3 h-1, and the emulsification activities were 0.666 and 0.158 units, respectively....
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Bioemulsifier; Candida lipolytica; Seawater; Babassu oil.
Ano: 2003
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S1517-83822003000200006

Sanitary quality of sands from marine recreational beaches of São Paulo, Brazil
Provedor de dados: 58
Autores: Sato,Maria Inês Zanoli; Di Bari,Marisa; Lamparelli,Claudia Condé; Truzzi,Ana Cristina; Coelho,Maria Cristina L.S.; Hachich,Elayse Maria.
A sanitary evaluation of sand and water from 16 beaches of São Paulo State, Brazil, was undertaken during spring of 1997 and summer of 1998. Ninety six samples each of wet and dry sand and seawater were collected and analysed for fecal indicator bacteria. A parasitological examination and Candida albicans analysis were also performed in sand samples and F-specific bacteriophages were determined in seawater. Statistical analysis of the results demonstrated higher concentrations of fecal coliforms and fecal streptococci in dry sand during summer. Correlation analysis indicated a significant relationship between fecal indicator densities in wet sand and seawater. There was a significant correlation between the densities of fecal coliforms and fecal...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Sand; Seawater; Recreational areas; Fecal indicators; Microbiological criteria.
Ano: 2005
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S1517-83822005000400003

Nutritional and functional characterization of wild and cultivated Sarcocornia neei grown in Chile
Provedor de dados: 118
Autores: Riquelme,Javiera; Olaeta,José Antonio; Gálvez,Lena; Undurraga,Pedro; Fuentealba,Claudia; Osses,Andrea; Orellana,Jaime; Gallardo,José; Pedreschi,Romina.
Sarcocornia neei is a halophyte that grows on the coast of the Valparaiso Region of Chile. Studies related to its nutritional and functional value under wild and cultivated conditions are not available. Thus, in this study, a nutritional (complete proximal, mineral and dietary fiber analysis) and functional characterization (total phenolics, &amp;#946;-carotene, hydrophilic and lipophilic antioxidant activity (HAA and LAA) and ascorbic acid) were performed for wild and cultivated plants. Wild plants displayed higher amounts of compounds involved in stress defense mechanisms such as total phenolics, proteins, dietary fiber and ash. The mineral analysis revealed that Na+ and Cl- are the main ions accumulated in wild and cultivated Sarcocornia neei that are...
Tipo: Journal article
Palavras-chave: Antioxidant; Dietary fiber; Proximal analysis; Seawater; Sustainability.
Ano: 2016
URL: http://www.scielo.cl/scielo.php?script=sci_arttext&pid=S0718-16202016000200011