Data/hora: 16/06/2024 09:37:38

Provedor de dados: | 111
País: | China
Título: | Effect mechanical on rice husking for test two machines
Autores: | Alwan, salih kadhim.
Data: | 2024-03-30
Ano: | 2024
Resumo: | The experiment was conducted to evaluated Effect of husking process on the rice productivity for two cultivars Mashkhab (M-33) and Jasmine (JA). Two types of machines (S-KB40 and Y-ST50) were tested at three ranges of clearance between cylinders of 0.5 mm, 0.7mm and 0.9mm for two rice cultivars of JA and M-33. The experiments were carried out in a factorial experiment under complete randomized design with three replications,&amp;nbsp; the study was of the characteristics following machine productivity, power required and husking efficiency, and the qualitative characteristics for two rice JA and M-33 cultivars included, broken rice ratio and head rice . The results showed that S-KB40 machine is better than Y-ST50 machine in all studied conditions for both two rice JA and M-33 cultivars. The clearance 0.9 was significantly superior to the other two levels of 0.5 and 0.7 mm in all studied condition except the husking efficiency for both two rice JA and M-33 cultivars.
Tipo: | Info:eu-repo/semantics/article
Idioma: | Inglês
Identificador: | http://www.cigrjournal.org/index.php/Ejounral/article/view/8755
Editor: | International Commission of Agricultural and Biosystems Engineering
Relação: | http://www.cigrjournal.org/index.php/Ejounral/article/view/8755/4203
Formato: | application/pdf

Fonte:

Agricultural Engineering International: CIGR Journal; Vol. 26 No. 1 (2024): CIGR Journal

1682-1130

Fonte: | Copyright (c) 2024 Agricultural Engineering International: CIGR Journal