Data/hora: 05/06/2024 15:54:36

Provedor de dados: 	19	
País: 	Japan	
Título: 	3方向応力測定器によるタイヤラグ面接地応力の測定

Measurement of Tire-Lug Contact Stresses by a Three-Dimensional Stress Transducer	
Autores: 	全, 亨奎; 谷口, 哲司; 岸本, 正; 吉田, 慎; 玉利, 達人; JUN, Hyung-gyu; TANIGUCHI, Tetsuji; KISHIMOTO, Tadashi; YOSHIDA, Makoto; TAMARI, Tatsuto.	
Data: 	1997-11	
Ano: 	1997	
Palavras-chave: 	接地応力; 法線方向応力; 接線方向応力; 横方向応力; 農用タイヤ; ラジアルタイヤ; Contact stress; Normal stress; Tangential stress; Lateral stress; Agricultural tractor tire; Radial tire.	
Resumo: 	タイヤの接地面に作用する応力を測定するために, タイヤラグフェースの一点における法線方向応力, 接線方向応力及び横方向応力を同時に測定できる測定器を開発した。本測定器を1本のタイヤラグの3ヶ所すなわちタイヤ踏面中心部, 同側端部ならびにこれらの中間部の3ヶ所に埋め込んで各応力を測定した。測定例としてすべり率20%時の応力分布状態を示し, 最大接地応力値及び発生位置を検討した。 A three-dimensional stress transducer was developed to measure normal，tangential and lateral stresses on the lug face between a tire-lug and soil. Three transducers were mounted on the part of lug - end which is almost the same place of the tire tread center，on the outer edge of lug and a intermediate place of above two places. The stress distributions of three transducers were presented and the relationships between peak stresses and their rotational angles at 20% slippage were discussed.	
Idioma: 	Japonês	
Identificador: 	http://ir.obihiro.ac.jp/dspace/handle/10322/2951	
Editor: 	農業機械学会	
Formato: 	application/pdf	
Fonte: 	農業機械学会