Data/hora: 16/06/2024 09:06:53

Provedor de dados: 	32	
País: 	Mexico	
Título: 	Consecuencias de la agricultura de conservación en la eficiencia del uso de agua bajo condiciones de riego	
Autores: 	Kienle, Fabian.	
Data: 	2012-09-08	
Ano: 	2008	
Palavras-chave: 	Agricultura de conservación; Calidad de suelo; Vertedor de cresta triangular; Riego por surcos; Maestría; Hidrociencias; Conservation agriculture; Soil quality; V-notch weir; Furrow-irrigation.	
Resumo: 	Esta investigación se realizó en un experimento a largo plazo establecido en 1992 para  evaluar el suelo sometido a diferentes prácticas de labranza y manejos de rastrojo del  Centro Internacional de Mejoramiento de Maíz y Trigo (CIMMYT), en la estación  experimental en el Centro de Investigaciones Agrícola del Noroeste (CIANO) en Ciudad  Obregón, Sonora, México, en el invierno 2008. Se evaluaron cinco diferentes sistemas  agrícolas respecto a su eficiencia en el uso de agua (EUA) en el cultivo de trigo, y un  sistema de riego por tubería con compuerta. Los cinco diferentes sistemas incluyeron  camas convencionales (CAC) con incorporación de paja y camas permanentes (CAP)  con cuatro diferentes manejos de paja (paja incorporada, paja quemada, paja removida,  paja parcialmente removida y paja retenida). El tipo de suelo en la estación del CIANO  es arcillo arenoso (Vertisol). El clima se clasifica como subtropical árido. Para evaluar la  EUA se hicieron mediciones en el cultivo, en el suelo y el riego. Se evaluaron el  desarrollo del cultivo mediante un sensor de índice diferencial normalizado de  vegetación y la cobertura por follaje. En el suelo se evaluó la cobertura por rastrojo, la  elasticidad del suelo, el agrietamiento, el tiempo de encharcamiento, la resistencia a la  penetración del suelo y el contenido de humedad del suelo. Para el riego se diseñó un  método para evaluar el riego a nivel de parcela experimental que consistió en la  medición de agua por cama, el agua de entrada, la tasa de avance y la salida del agua.  En las CAP con retención de paja el desarrollo inicial del cultivo fue más tardado en  comparación a CAC, pero en total el primero tenia más tiempo en la actividad  fotosintética. Los sistemas con retención de paja (total o parcial) tienen un tiempo de  encharcamiento mayor que los otros sistemas. La resistencia a la penetración del suelo  fue lo mas alto en CAP con quema de paja. La labranza disminuye la resistencia en la  capa superficial en comparación con las CaP, mientras que las CaP con retención de  paja tuvieron la distribución de la resistencia más uniforme en el perfil. La elasticidad  del suelo fue la mas baja en CaP con quema de paja. La superficie de grietas fue más  alta en CaP con retención de paja que en CaP con quema de paja y CaC. La medición  de la entrada del agua y de la tasa de avance del agua así como la medición de salida  del agua con una adaptación de un vertedor de cresta triangular resultó adecuada para  la evaluación del riego a nivel de parcela experimental. La infiltración del agua del riego  fue mayor en CaP con retención de paja que en CaP con quema de paja y CaC. El  manejo de quemar los residuos es una práctica no recomendable por el efecto  disminuir la calidad del suelo. Los sistemas de manejo agrícolas con retención de paja  total o parcialmente, contribuyen para tener una mayor eficiencia en el uso de agua._______This investigation was realized in a long term trial established in 1992 to evaluate  different tillage and straw management of the International Maize and Wheat  Improvement Center (CIMMYT) in the experimental station of the Northwestern  Agricultural Investigation Centre (Centro de Investigaciones Agrícola del Noroeste,  CIANO) near Ciudad Obregón, in Sonora, Mexico, in 2008. Five different agricultural  systems were evaluated in respect of the water use efficiency (WUE) in wheat under  furrow irrigation. The five systems were conventional beds (CTB) with incorporation of  crop residue and permanent beds (PB) with four residue managements (burning of  straw, straw removal, partial and full straw retention). The soil type at CIANO station is a  coarse sandy clay (Vertisol). The climate is subtropical arid. To evaluate WUE  measurements of crop, soil and irrigation were taken. Of crop development the  Normalized Difference Vegetation Index and crop ground cover were measured. Mulch  ground cover, soil resilience, cracking, time-to-pond, penetration resistance and soli  moisture were measured to evaluate soil quality. To evaluate irrigation a method to  measure irrigation on experimental plot level was developed consisting in the  measurement of inflow, outflow and advance-rate. Irrigation water had a higher advance  rate in systems without straw retention than in PB with straw retention. The infiltration of  water was higher in PB with straw retention than in PB with straw burned and CTB. In  PB with straw retention the initial crop development was delayed in comparison to CTB,  but in total CTB had a longer time of photosynthetic activity. Straw retaining systems  have a higher direct infiltration (time to pond) than other systems. Penetration resistance  was the highest in PB with burning of residue. Tillage decreased the penetration  resistance in the top layer in comparison with PB, while the distribution of penetration  resistance was the most uniform throughout the profile in permanent beds with residue  retention. Soil self-mulching capacity was the lowest in permanent beds with residue  burning. The surface of cracks was higher in PB with residue retention than in PB with  burning of residue and CB. Inflow and advanced measurement as well as outflow  measurement with an adaption of a v-notch weir resulted adapted for irrigation  evaluation at experimental plot level. The irrigation water advanced faster in systems  without mulch cover. The infiltration of irrigation water was higher (but not significantly)  in PB with residue retention than in PB with residue burning and conventional beds. The  system of burning straw is a practice which reduces permeability of the surface soil. The  systems of agricultural managements with total or partly straw retention contribute to a  better water use efficiency.	
Tipo: 	Tesis	
Idioma: 	Espanhol	
Identificador: 	http://hdl.handle.net/10521/1261