Data/hora: 04/06/2024 02:27:32

Provedor de dados: | 42
País: | Brazil
Título: | An experimental study of the partitioning of trace elements between rutile and silicate melt as a function of oxygen fugacity
Autores: | MALLMANN,GUILHERME; FONSECA,RAÚL O.C.; SILVA,ADOLFO B.
Data: | 2014-12-01
Ano: | 2014
Palavras-chave: | Arc magma; HFSE; Partition coefficient; Redox; Rutile.
Resumo: | Subduction zone or arc magmas are known to display a characteristic depletion of High Field Strength Elements (HFSE) relative to other similarly incompatible elements, which can be attributed to the presence of the accessory mineral rutile (TiO2) in the residual slab. Here we show that the partitioning behavior of vanadium between rutile and silicate melt varies from incompatible (∼0.1) to compatible (∼18) as a function of oxygen fugacity. We also confirm that the HFSE are compatible in rutile, with D(Ta)&gt; D(Nb)&gt;&gt; (D(Hf)&gt;/∼ D(Zr), but that the level of compatibility is strongly dependent on melt composition, with partition coefficients increasing about one order of magnitude with increasing melt polymerization (or decreasing basicity). Our partitioning results also indicate that residual rutile may fractionate U from Th due to the contrasting (over 2 orders of magnitude) partitioning between these two elements. We confirm that, in addition to the HFSE, Cr, Cu, Zn and W are compatible in rutile at all oxygen fugacity conditions.
Tipo: | Info:eu-repo/semantics/article
Idioma: | Inglês
Identificador: | http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0001-37652014000401609
Editor: | Academia Brasileira de Ciências
Relação: | 10.1590/0001-3765201420140014
Formato: | text/html
Fonte: | Anais da Academia Brasileira de Ciências  v.86 n.4 2014
Fonte: | info:eu-repo/semantics/openAccess