Data/hora: 03/06/2024 08:17:37

Provedor de dados: | Institutional Archive of Ifreme (ArchiMer)
País: | France
Título: | Description and modeling of polyurethane hydrolysis used as thermal insulation in oil offshore conditions
Autores: | Le Gac, Pierre-yves; Choqueuse, Dominique; Melot, D.
Data: | 2013-12
Ano: | 2013
Palavras-chave: | Polyurethane; Hydrolysis; Accelerated ageing; Sea water; Coating; Offshore.
Resumo: | Polymers are widely used for passive thermal insulation coatings on steel pipe in offshore oil and gas production. In this industry, structures used in deep sea have to be reliable, as they are in service for more than 20 years in a very severe environment: sea water, hydrostatic pressure and temperature gradient. One of the main questions is how to test and predict the lifetime of such structures in the laboratory? This study presents one approach that has been developed to characterize and predict the degradation of polymers used as thermal insulation materials.  This paper is dedicated to polyurethane (polyether based) degradation in sea water at high temperature. Ageing has been performed in natural sea water under hydrostatic pressure at temperatures ranging from 70 to 120 °C on 2 mm thick samples. Water diffusion in the material and hydrolysis have been characterized using mass evolution and tensile tests. Based on these results, a model for the urethane hydrolysis reaction is proposed.
Tipo: | Text
Idioma: | Inglês

Identificador:

http://archimer.ifremer.fr/doc/00160/27132/25330.pdf

DOI:10.1016/j.polymertesting.2013.10.009

Editor: | Elsevier Sci Ltd
Relação: | http://archimer.ifremer.fr/doc/00160/27132/
Formato: | application/pdf
Fonte: | Polymer Testing (0142-9418) (Elsevier Sci Ltd), 2013-12 , Vol. 32 , N. 8 , P. 1588-1593
Fonte: | 2013 Elsevier B.V. All rights reserved.