Data/hora: 05/06/2024 14:33:59

Provedor de dados: | Institutional Archive of Ifreme (ArchiMer)
País: | France
Título: | Elements sur le comportement experimental et numerique de la structure d'un voilier de 7m70 en cours de navigation
Autores: | Baley, C; Cailler, M.
Data: | 1992-12
Ano: | 1992
Palavras-chave: | Finite element method; Navigation; Measurement; Boating; Sailing ships; Mechanical properties; Ship technology; Composite materials; Navigation; Comportement mécanique; Eléments finis; Mesure; Matériau composite; Voilier.
Resumo: | The experimental sailing boat "Mesure Z," has been designed and built on behalf of F.I.N., (the French marine industry association). This research project has been managed in close collaboration with Bureau Veritas, Ifremer and the CEA. The GRP hull is similar to that of a production sailing boat, but it has been designed as a transducer-hull, i.e. a hull sufficiently sensitive to allow measurements (hull strains, acceleration, spar loads, etc), due to its structure and mechanical characteristics. This paper presents different aspects of the experimental boat, the materials and structure of the transducer-hull, and the behaviour of the central and bow regions of the hull during sailing.
Tipo: | Text
Idioma: | Francês
Identificador: | http://archimer.ifremer.fr/doc/1992/acte-1073.pdf
Editor: | Actes de colloques. Ifremer. Brest [ACTES COLLOQ. IFREMER.]. 1992
Relação: | http://archimer.ifremer.fr/doc/00000/1073/
Formato: | application/pdf