Data/hora: 05/06/2024 02:11:54

Provedor de dados: 	5	
País: 	France	
Título: 	The use of high rate algal ponds for the treatment of marine effluent from a recirculating fish rearing system	
Autores: 	Pagand, Pascal; Blancheton, Jean-paul; Lemoalle, J; Casellas, C.	
Data: 	2000-10	
Ano: 	2000	
Palavras-chave: 	Nitrogen; Biofilters; Irradiance; Temperature; Photosynthesis; Growth; Culture; Chlorophyta; Nutrient Removal.	
Resumo: 	A high rate algal pond (HRAP) system was used to treat effluent from a recirculating sea water aquaculture system in southern France. Dicentrarchus labrax L. were farmed at a high density, with effluents containing an average of 10 mg L-1 dissolved inorganic nitrogen (DIN) and 1.3 mg L-1 reactive phosphorus (RP). On a yearly basis, the algal pond removed 59% of the dissolved nitrogen and 56% of the phosphorus input, which was converted into 3.3 kg DW m(-2) algae. Green macroalgae were dominant throughout the year and the algal biomass mirrored the seasonal changes in daily irradiance and temperature. This first year study supports the possibility of treating marine aquaculture wastes using HPAPs, although conditions will have to be found to mitigate the strong influence of climate on the algal community during winter. During the more temperate season, only 150 m(2) of treatment ponds would be necessary to remove the nutrients produced by 1 ton of fish. Treated water was characterized by a high pH, elevated levels of dissolved oxygen (midday value) and low concentrations of nutrients and suspended solids. The absence of toxic phytoplankton meant that the water could be recycled through the farm tanks.	
Tipo: 	Text	
Idioma: 	Inglês	
Identificador: 	http://archimer.ifremer.fr/doc/2000/publication-515.pdf

DOI:10.1046/j.1365-2109.2000.00493.x	
Editor: 	Blackwell science	
Relação: 	http://archimer.ifremer.fr/doc/00000/515/	
Formato: 	application/pdf	
Fonte: 	Aquaculture Research (1355-557X) (Blackwell science), 2000-10 , Vol. 31 , N. 10 , P. 729-736	
Fonte: 	2000 Blackwell Synergy