Data/hora: 16/06/2024 10:42:01

Provedor de dados: 	Institutional Archive of Ifreme (ArchiMer)	
País: 	France	
Título: 	Dynamical modelling of a reactive extrusion process: Focus on residence time distribution in a fully intermeshing co-rotating twin-screw extruder and application to an alginate extraction process	
Autores: 	Baron, Regis; Vauchel, Peggy; Kaas, Raymond; Arhaliass, Abdellah; Legrand, Jack.	
Data: 	2010-05	
Ano: 	2010	
Palavras-chave: 	Alginate; Extraction; Extrusion; Mathematical modelling; Residence time distribution; Simulation; Laminaria digitata.	
Resumo: 	The context of this study is the modelling of reactive extrusion process based on an alginate extraction protocol. Residence Time Distribution (RTD) is one important part to predict the kinetics of reactive compounds. A simple model is proposed to predict RTD in fully intermeshing co-rotating twin-screw extruders without reaction. This model, which can be easily extended to reactive case in a future work, is based on the extension of an axial dispersion model, including control parameters (screw speed and flow rate) and geometrical parameters (screw profile and die design). Simulations were performed for various operating and geometrical conditions so as to illustrate possibilities offered by the proposed model. Validation was conducted for two different extrusion applications, seaweed extrusion and polymer extrusion. This highlighted the model ability to predict RID for various kinds of materials after adjusting only one parameter thanks to a unique experimental RID curve. (C) 2010 Elsevier Ltd. All rights reserved.	
Tipo: 	Text	
Idioma: 	Inglês	
Identificador: 	http://archimer.ifremer.fr/doc/00005/11592/8985.pdf

DOI:10.1016/j.ces.2010.02.019	
Editor: 	Pergamon-elsevier Science Ltd	
Relação: 	http://archimer.ifremer.fr/doc/00005/11592/	
Formato: 	application/pdf	
Fonte: 	Chemical Engineering Science (0009-2509) (Pergamon-elsevier Science Ltd), 2010-05 , Vol. 65 , N. 10 , P. 3313-3321	
Fonte: 	2010 Elsevier Ltd All rights reserved.