Data/hora: 01/06/2024 03:36:21

Provedor de dados: 	Institutional Archive of Ifreme (ArchiMer)	
País: 	France	
Título: 	Modélisation hydrodynamique de la dispersion à court terme dans une mer macrotidale: validation par des mesures à haute résolution de radiotraceurs solubles	
Autores: 	Bailly Du Bois, Pascal; Dumas, Franck.	
Data: 	2004-09	
Ano: 	2004	
Palavras-chave: 	Validation; Tritium; Dispersion; North sea; Hydrodynamic model; Validation; Tritium; Dispersion; Manche; Modèle.	
Resumo: 	DISPRO project aims to validate hydrodynamic models dispersion parameters by field data for the short-term (hours to week) and short distances (100 meters to 30 km). This project is based on a 2D instantaneous currents model with a mesh size of 110 m, coupled with high frequency field data collected in the release plume. At this step of the works, measurements confirm the reliability of the model during six hours following a release. This validation made possible developpement of models with known incertitude to simulate dispersion of dissolved substances in realistic conditions for normal or accidental situations in macrotidal seas.	
Tipo: 	Text	
Idioma: 	Francês	
Identificador: 	http://archimer.ifremer.fr/doc/2004/acte-564.pdf	
Editor: 	VIIIèmes Journées Nationales Génie Civil ¿ Génie Côtier, Compiègne, 7-9 septembre 2004	
Relação: 	http://archimer.ifremer.fr/doc/00000/564/	
Formato: 	application/pdf