Data/hora: 06/06/2024 00:41:52

Provedor de dados: | 5
País: | France
Título: | Modelling mud transport in a macrotidal estuary
Autores: | Le Hir, Pierre; Bassoullet, Philippe; L'Yavanc, Jacky.
Data: | 1988
Ano: | 1988
Palavras-chave: | Dynamique des sédiments cohésifs; Estuaire Morlaix; Tassement des vases; Modèle mathématique; Érosion; Dépôt; Cohesive sediment dynamics; Estuary; Erosion; Deposition; SoiT consolidation; Mathematical modelling.
Resumo: | In order to determine the fate of the fine particles and adsorbed contaminants in·a short macrotidal èstuary, a mathematical modelling system for cohesive suspended mater transport and bottom evolution, including a new consolidation algorithm, is developed. An analysis of successive erosion, transport and deposi~ion processes due to tidal forcing is given and comparisons with field data are provided. A description of mean-term bottom variations has been attempted and is partially validated by differential soundings.
Tipo: | Text
Idioma: | Inglês

Identificador:

https://archimer.ifremer.fr/doc/00682/79379/81909.pdf

https://archimer.ifremer.fr/doc/00682/79379/

Formato: | application/pdf

Fonte:

info:eu-repo/semantics/openAccess

restricted use