Data/hora: 09/06/2024 15:35:42

Provedor de dados: 	5	
País: 	France	
Título: 	Yield stress changes induced by water in polyamide 6: Characterization and modeling	
Autores: 	Le Gac, Pierre-yves; Arhant, Mael; Le Gall, Maelenn; Davies, Peter.	
Data: 	2017-03	
Ano: 	2017	
Palavras-chave: 	Yield stress; Water; Polyamide; Plasticization; Prediction.	
Resumo: 	This paper considers the effect of water content on mechanical properties of polyamide 6 when used in a humid environment. First an experimental section presents the tensile behavior of polyamide with different amounts of water, with and without a through-thickness water gradient. Water profiles are introduced by immersion in sea water at 25 °C. The effect of testing temperature is also investigated in order to consider the influence of macromolecular chain mobility on the mechanical behavior. Then, in a second section, modelling of yield stress is proposed based on physical considerations. This can be used for life time prediction of PA6 in humid environment when plasticization is the main degradation mechanism.	
Tipo: 	Text	
Idioma: 	Inglês	
Identificador: 	http://archimer.ifremer.fr/doc/00371/48208/48321.pdf

DOI:10.1016/j.polymdegradstab.2017.02.003

http://archimer.ifremer.fr/doc/00371/48208/	
Editor: 	Elsevier Sci Ltd	
Formato: 	application/pdf	
Fonte: 	Polymer Degradation And Stability (0141-3910) (Elsevier Sci Ltd), 2017-03 , Vol. 137 , P. 272-280	
Fonte: 	2017 Elsevier Ltd. All rights reserved.

info:eu-repo/semantics/openAccess

restricted use