Data/hora: 04/06/2024 09:26:38

Provedor de dados: | 5
País: | France
Título: | Effect of Coarse Particle Volume Fraction on the Yield Stress of Muddy Sediments from Marennes Oleron Bay
Autores: | Pantet, A.; Robert, Serge; Jarny, S.; Kervella, Stephane.
Data: | 2010
Ano: | 2010
Resumo: | Coastal erosion results from a combination of various factors, both natural and humaninduced, which have different time and space patterns. In addition, uncertainties still remain about the interactions of the forcing agents, as well as on the significance of non-local causes of erosion. We focused about the surface sediments in the Marennes Oleron bay, after a general description of the site that has many various activities. The superficial sediments show a mechanical behavior, mainly depends on the fine fraction for a composition that contains up to 60% of sandy material. Fine sediments fraction has a typical yield stress depending naturally of concentration or water content. This yield could be modified slightly or significantly by adding silt or sand. As a result, the rheological measurement sensitivity allows us to characterize five typical sediments that correlate with solid fraction and fine fraction.
Tipo: | Text
Idioma: | Inglês

Identificador:

http://archimer.ifremer.fr/doc/00035/14608/11927.pdf

DOI:10.1155/2010/245398

Editor: | Hindawi Publishing Corporation
Relação: | http://archimer.ifremer.fr/doc/00035/14608/
Formato: | application/pdf
Fonte: | Advances In Materials Science And Engineering (1687-6822) (Hindawi Publishing Corporation), 2010 , Vol. 2010 , P. 1-6
Fonte: | 2010 A. Pantet et al. This is an open access article distributed under the Creative Commons, Hindawi Publishing