Data/hora: 03/06/2024 01:13:22

Provedor de dados: 	Institutional Archive of Ifreme (ArchiMer)	
País: 	France	
Título: 	Correction and Accuracy of High- and Low-Resolution CTD Data from Animal-Borne Instruments	
Autores: 	Siegelman, Lia; Roquet, Fabien; Mensah, Vigan; Riviere, Pascal; Pauthenet, Etienne; Picard, Baptiste; Guinet, Christophe.	
Data: 	2019-05	
Ano: 	2019	
Palavras-chave: 	Algorithms; Data processing; In situ oceanic observations.	
Resumo: 	Most available CTD Satellite Relay Data Logger (CTD-SRDL) profiles are heavily compressed before satellite transmission. High-resolution profiles recorded at the sampling frequency of 0.5 Hz are, however, available upon physical retrieval of the logger. Between 2014 and 2018, several loggers deployed on elephant seals in the Southern Ocean have been set in continuous recording mode, capturing both the ascent and descent for over 60 profiles per day during several months, opening new horizons for the physical oceanography community. Taking advantage of a new dataset made of seven such loggers, a postprocessing procedure is proposed and validated to improve the quality of all CTD-SRDL data: that is, both high-resolution profiles and compressed low-resolution ones. First, temperature and conductivity are corrected for a thermal mass effect. Then salinity spiking and density inversion are removed by adjusting salinity while leaving temperature unchanged. This method, applied here to more than 50 000 profiles, yields significant and systematic improvements in both temperature and salinity, particularly in regions of rapid temperature variation. The continuous high-resolution dataset is then used to provide updated accuracy estimates of CTD-SRDL data. For high-resolution data, accuracies are estimated to be of +/- 0.02 degrees C for temperature and +/- 0.03 g kg(-1) for salinity. For low-resolution data, transmitted data points have similar accuracies; however, reconstructed temperature profiles have a reduced accuracy associated with the vertical interpolation of +/- 0.04 degrees C and a nearly unchanged salinity accuracy of +/- 0.03 g kg(-1).	
Tipo: 	Text	
Idioma: 	Inglês	
Identificador: 	https://archimer.ifremer.fr/doc/00494/60567/64043.pdf

https://archimer.ifremer.fr/doc/00494/60567/64044.pdf

DOI:10.1175/JTECH-D-18-0170.1

https://archimer.ifremer.fr/doc/00494/60567/	
Editor: 	Amer Meteorological Soc	
Formato: 	application/pdf	
Fonte: 	Journal Of Atmospheric And Oceanic Technology (0739-0572) (Amer Meteorological Soc), 2019-05 , Vol. 36 , N. 5 , P. 745-760	
Fonte: 	info:eu-repo/semantics/openAccess

restricted use