Data/hora: 01/06/2024 06:39:44

Provedor de dados: | Brazilian Journal of Medical and Biological Research
País: | Brazil
Título: | A comparative analysis of preprocessing techniques of cardiac event series for the study of heart rhythm variability using simulated signals
Autores: | Guimarães,H.N.; Santos,R.A.S.
Data: | 1998-03-01
Ano: | 1998
Palavras-chave: | Heart rhythm variability; Heart rate variability; Spectral analysis; Data preprocessing; Integral pulse frequency modulation model.
Resumo: | In the present study, using noise-free simulated signals, we performed a comparative examination of several preprocessing techniques that are used to transform the cardiac event series in a regularly sampled time series, appropriate for spectral analysis of heart rhythm variability (HRV). First, a group of noise-free simulated point event series, which represents a time series of heartbeats, was generated by an integral pulse frequency modulation model. In order to evaluate the performance of the preprocessing methods, the differences between the spectra of the preprocessed simulated signals and the true spectrum (spectrum of the model input modulating signals) were surveyed by visual analysis and by contrasting merit indices. It is desired that estimated spectra match the true spectrum as close as possible, showing a minimum of harmonic components and other artifacts. The merit indices proposed to quantify these mismatches were the leakage rate, defined as a measure of leakage components (located outside some narrow windows centered at frequencies of model input modulating signals) with respect to the whole spectral components, and the numbers of leakage components with amplitudes greater than 1%, 5% and 10% of the total spectral components. Our data, obtained from a noise-free simulation, indicate that the utilization of heart rate values instead of heart period values in the derivation of signals representative of heart rhythm results in more accurate spectra. Furthermore, our data support the efficiency of the widely used preprocessing technique based on the convolution of inverse interval function values with a rectangular window, and suggest the preprocessing technique based on a cubic polynomial interpolation of inverse interval function values and succeeding spectral analysis as another efficient and fast method for the analysis of HRV signals
Tipo: | Info:eu-repo/semantics/article
Idioma: | Inglês
Identificador: | http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-879X1998000300015
Editor: | Associação Brasileira de Divulgação Científica
Relação: | 10.1590/S0100-879X1998000300015
Formato: | text/html
Fonte: | Brazilian Journal of Medical and Biological Research  v.31 n.3 1998
Fonte: | info:eu-repo/semantics/openAccess