Data/hora: 04/06/2024 14:54:32

Provedor de dados: 	70	
País: 	Brazil	
Título: 	Mechanical properties of grain in silos for simulation designs	
Autores: 	Lopes Neto,José P.; Nascimento,José W. B. do; Marques,Jordânio I.; Costa,Carlos A. da.	
Data: 	2016-08-01	
Ano: 	2016	
Palavras-chave: 	Poisson’s coefficient; Compression; Modulus of elasticity; Silos; Simulation.	
Resumo: 	ABSTRACT For the calculation of silos structures it has been used new methods and computational tools that require mechanical properties knowledge that are still unknown for most storable materials, especially grains. In this context, we aimed to determine the mechanical properties of rice and beans grains with moisture contents of 10, 12, and 14% by applying four compressive loads (5, 10, 15 and 20). The determined mechanical properties were Poisson's ratio (ν), Modulus of Elasticity (E), and the dilatancy angle (ψ). The procedure consisted in the application of the load in compression cell, adapted from MOLENDA &amp; STASIAK, aiming to simulate loading and unloading of silos. We observed that the Poisson's ratio calculated for both loading and unloading, presented higher values than the experimental values, with the increase of their moisture content; the experimental elastic modulus presented higher values than the calculated ones, and both increased their values with the increase of their moisture content; the dilatancy angle decreased with the increase of moisture content and compressive loads.	
Tipo: 	Info:eu-repo/semantics/article	
Idioma: 	Inglês	
Identificador: 	http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162016000400573	
Editor: 	Associação Brasileira de Engenharia Agrícola	
Relação: 	10.1590/1809-4430-Eng.Agric.v36n4p573-580/2016	
Formato: 	text/html	
Fonte: 	Engenharia Agrícola  v.36 n.4 2016	
Fonte: 	info:eu-repo/semantics/openAccess