Data/hora: 16/06/2024 06:25:31

Provedor de dados: 	70	
País: 	Brazil	
Título: 	Technical evaluation of artificial ligthing systems for broiler houses	
Autores: 	Pereira,Priscilla A.; Yanagi Junior,Tadayuki; Silva,Joaquim P. da; Lima,Renato R. de; Campos,Alessandro T.; Abreu,Lucas H. P.	
Data: 	2012-12-01	
Ano: 	2012	
Palavras-chave: 	Artificial lighting; Spatial variability; Energy efficiency; Aviculture.	
Resumo: 	The spatial distribution of illuminance and the electric consumption of artificial lighting system is one of the main problems related to broiler production. Therefore, the aim of this study was to evaluate the spatial distribution of luminance level and energy efficiency of different lighting systems for broiler houses. Six types of lamps were tested in two different configurations to find the minimum illuminance of 20 and 5 lux. The tested lamps were incandescent (IL) 100 W, compact fluorescent (CFL) 34 W, mixed (ML) 160 W, sodium vapor (SVL) 70 W, T8 fluorescent tube (T8 FTL) 40 W and T5 fluorescent tube (T5 FTL) 28 W. The first four were evaluated with and without reflective light fixture and the latter two without light fixture. It was observed that the tested system with light fixtures negatively affected the spatial distribution of illuminance inside the house. The systems composed by IL and ML without light fixture led to better results in meeting the minimum illuminance of 20 lux and 5 lux, respectively. T5 FTL presented the lowest energy demand.	
Tipo: 	Info:eu-repo/semantics/article	
Idioma: 	Inglês	
Identificador: 	http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162012000600002	
Editor: 	Associação Brasileira de Engenharia Agrícola	
Relação: 	10.1590/S0100-69162012000600002	
Formato: 	text/html	
Fonte: 	Engenharia Agrícola  v.32 n.6 2012	
Fonte: 	info:eu-repo/semantics/openAccess