Data/hora: 07/06/2024 12:26:08

Provedor de dados: | Engenharia Agrícola
País: | Brazil
Título: | AGRONOMICAL ATTRIBUTES OF SOYBEANS AND SOIL RESISTANCE TO PENETRATION IN NO-TILLAGE AND CHISELED SURFACES
Autores: | Cortez,Jorge W.; Mauad,Munir; Souza,Luiz C. F. de; Rufino,Mauricio V.; Souza,Paulo H. N. de.
Data: | 2017-02-01
Ano: | 2017
Palavras-chave: | Compaction; Soil physics; Chiseling.
Resumo: | ABSTRACT Farming systems may affect soil properties and crop production of components, decreasing yields. This study aimed to assess penetration resistance (PR) and agronomic traits of soybeans under no-tillage (NT) and chiseling (CP). The experiment was carried out in a randomized block with two treatments (tillage and scarification) with 12 repetitions; yet soil penetration resistance (PR) was assessed in a factorial block, considering farming systems and sampling sites (row and interrows). PR was measured with an impact penetrometer, sampling in row and interrows within a 22.5 x 0.1 m2 mesh grid up to 0.60 m depth. The obtained values were higher for NT in the 0.10-0.20 m layer. Great PR values in interrows were only registered within the surface layer. This is because there was no soil mobilization by seeder chisel plow. In chiseled soil, compaction was reduced, however, the first tractor passings were able to compact the soil to a depth of 0.50 m. Therefore, scarification reduced the plant stand and penetration resistance, allowing greater growth and soybean yield.
Tipo: | Info:eu-repo/semantics/article
Idioma: | Inglês
Identificador: | http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162017000100098
Editor: | Associação Brasileira de Engenharia Agrícola
Relação: | 10.1590/1809-4430-eng.agric.v37n1p98-105/2017
Formato: | text/html
Fonte: | Engenharia Agrícola  v.37 n.1 2017
Fonte: | info:eu-repo/semantics/openAccess