Data/hora: 01/06/2024 17:24:34

Provedor de dados: | Engenharia Agrícola
País: | Brazil
Título: | Cassava starch extraction effluent treatment in a one phase tubular horizontal pilot reactor with support medium
Autores: | Kuczman,Osvaldo; Tavares,Maria H. F.; Gomes,Simone D.; Guedes,Luciana P. C.; Grisotti,Geovane.
Data: | 2014-12-01
Ano: | 2014
Palavras-chave: | Biodigester; Biogas; Anaerobic digestion; Cassava; Cassava wastewater.
Resumo: | The cassava starch industries generate a large volume of wastewater effluent that, stabilized in ponds, wastes its biogas energy and pollutes the atmosphere. To contribute with the reversion of this reality, this manipueira treatment research was developed in one phase anaerobic horizontal pilot reactor with support medium in bamboo pieces. The reactor was excavated into the ground and sealed with geomembrane in HDPE, having a volume equal to 33.6 m³ and continuous feeding by gravity. The stability indicators were pH, volatile acidity/total alkalinity ratio and biogas production. The statistical analyses were performed by a completely randomized design, with answers submitted to multivariate analysis. The organical loads in COD were 0.556; 0.670; 0.678 and 0.770 g L-1 and in volatile solids (VS) of 0.659; 0.608; 0.570 and 0.761 g L-1 for the hydraulic retention times (HRT) of 13.0; 11.5; 10.0 and 7.0 days, respectively. The reductions in COD were 88; 80; 88 and 67% and for VS of 76; 77; 65 and 61%. The biogas productions relatively to the consumed COD were 0.368; 0.795; 0.891 and 0.907 Lg-1, for the consumed VS of 0.524; 0.930; 1.757 and 0.952 Lg-1 and volumetric of 0.131; 0.330; 0.430 and 0.374 L L-1 d-1. The reactor remained stable and the bamboo pieces, in visual examination at the end of the experiment, showed to be in good physical conditions.
Tipo: | Info:eu-repo/semantics/other
Idioma: | Inglês
Identificador: | http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162014000600021
Editor: | Associação Brasileira de Engenharia Agrícola
Relação: | 10.1590/S0100-69162014000600021
Formato: | text/html
Fonte: | Engenharia Agrícola  v.34 n.6 2014
Fonte: | info:eu-repo/semantics/openAccess