Data/hora: 03/06/2024 11:00:23

Provedor de dados: | Engenharia Agrícola
País: | Brazil
Título: | HYDROPHOBIC MEMBRANE TECHNOLOGY FOR AMMONIA EXTRACTION FROM WASTEWATERS
Autores: | KUNZ,AIRTON; MUKHTAR,SAQIB.
Data: | 2016-04-01
Ano: | 2016
Palavras-chave: | Ammonia; Separation; Wastewater; Nutrient recovery.
Resumo: | ABSTRACT Total Ammoniacal Nitrogen - TAN (NH3 + NH4+) in wastewaters cause environmental degradation concerns due to their negative impacts on air, soil and water. Several technologies are available for TAN removal from the wastewaters. One emerging technology is the use of hydrophobic membrane as non-destructive NH3 extraction. In this paper the authors discuss the uses of gas permeable membrane (GPM) and its physicochemical characteristics that influence gas mass transfer rate, diffusion and recovery mechanisms of NH3 from liquid sources (e.g. animal wastewater). Several aspects of NH3 extraction from liquid manure and other TAN generation sources using GPM technology as well as its applicability for NH3 mitigation from liquid effluents and possible recovery as a nutrient for plant growth are also discussed in this review.
Tipo: | Info:eu-repo/semantics/article
Idioma: | Inglês
Identificador: | http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162016000200377
Editor: | Associação Brasileira de Engenharia Agrícola
Relação: | 10.1590/1809-4430-Eng.Agric.v36n2p377-386/2016
Formato: | text/html
Fonte: | Engenharia Agrícola  v.36 n.2 2016
Fonte: | info:eu-repo/semantics/openAccess