Data/hora: 09/06/2024 15:57:42

Provedor de dados: 	Engenharia Agrícola	
País: 	Brazil	
Título: 	DEFICIT IRRIGATION OF SUBSURFACE DRIP-IRRIGATED GRAPE TOMATO	
Autores: 	Mendonça,Thaís G.; Silva,Marília B. da; Pires,Regina C. de M.; Souza,Claudinei F.	
Data: 	2020-08-01	
Ano: 	2020	
Palavras-chave: 	TDR; Water resources; Irrigation management; Water content.	
Resumo: 	ABSTRACT Agriculture is one of the segments that most uses water and developments have been made to save irrigation water. Deficit irrigation is a technique that can contribute to production and water saving in agriculture. This study aimed to evaluate the viability of deficit irrigation in tomato production irrigated by subsurface drip in a greenhouse and estimate water saving. The experiment was conducted at the CCA/UFSCar, in Araras, São Paulo, Brazil, with grape tomato cultivation. It consisted of three treatments, 100 % water depth and deficit irrigation (75 and 50 % of water depth), with a randomized block design. Irrigation management was performed using mean soil moisture data collected through TDR probes installed in each treatment. Tomato plants were cultivated for 137 days and conducted vertically with one stem and six bunches. Fruit size, number and mass of fruits per plant, fruit pH and soluble solids were attributes measured and analyzed weekly. The deficit irrigation of 50 % treatment presented lower values in all attributes evaluated and 90.6 % of water saving. The 75 % treatment showed lower value only for pH and fruit diameter and 70.4 % of water saving. Deficit irrigation of 75 % was viable for tomato cultivation in greenhouse and for water saving in crop cycle.	
Tipo: 	Info:eu-repo/semantics/article	
Idioma: 	Inglês	
Identificador: 	http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162020000400453	
Editor: 	Associação Brasileira de Engenharia Agrícola	
Relação: 	10.1590/1809-4430-eng.agric.v40n4p453-461/2020	
Formato: 	text/html	
Fonte: 	Engenharia Agrícola  v.40 n.4 2020	
Fonte: 	info:eu-repo/semantics/openAccess