Data/hora: 11/06/2024 16:25:58

Provedor de dados: 	70	
País: 	Brazil	
Título: 	PERFORMANCE OF AN AGRICULTURAL DIESEL ENGINE USING DIFFERENTS FUELS	
Autores: 	Perin,Gismael F.; Schlosser,José F.; Galon,Leandro; Rodrigues,Fabrício A.; Frantz,Ulisses G.	
Data: 	2017-02-01	
Ano: 	2017	
Palavras-chave: 	Test; Dynamometer; Tractor; Torque; Power.	
Resumo: 	ABSTRACT The use of fuels for agricultural Diesel engines cycle, both of mineral origin (Diesel) or vegetable and animal origin (biodiesel) can significantly alter its performance. Therefore, the aim of this study was to quantify the change in torque, power and consumption of agricultural Diesel engine fuel using minerals and vegetables fuels. It was used a tractor power take-off coupled to a magnetic brake dynamometer (for measuring speed and torque for subsequent calculation of power), and a flow meter (for measuring the hourly fuel consumption and specific fuel consumption calculation). Eleven different fuels (S10 mineral diesel with 5%, 10%, 15%, 20% and 50% biodiesel and mineral diesel S500 with 5%, 10%, 15%, 20% and 50% biodiesel, have been used pure biodiesel B100). The results indicate that the increase of biodiesel in mineral diesel reduces torque and power, increases the specific fuel consumption and practically does not change the hourly consumption. This reduction in torque and power occurs with greater intensity in Diesel S10. Additions of 10% biodiesel in mineral diesel reduces the maximum torque 1.65 Nm (0.6%), the maximum power at 0.33 kW (0.6%) and increases the specific fuel consumption of 3.6 g kWh -1 (1.3%).	
Tipo: 	Info:eu-repo/semantics/article	
Idioma: 	Inglês	
Identificador: 	http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162017000100091	
Editor: 	Associação Brasileira de Engenharia Agrícola	
Relação: 	10.1590/1809-4430-eng.agric.v37n1p91-97/2017	
Formato: 	text/html	
Fonte: 	Engenharia Agrícola  v.37 n.1 2017	
Fonte: 	info:eu-repo/semantics/openAccess