Data/hora: 03/06/2024 06:27:29

Provedor de dados: 	Engenharia Agrícola	
País: 	Brazil	
Título: 	GREEN ROOF: SIMULATION OF ENERGY BALANCE COMPONENTS IN RECIFE, PERNAMBUCO STATE, BRAZIL	
Autores: 	Omar,Aline; Vigoderis,Ricardo; Pandorfi,Héliton; Moura,Geber; Guiselini,Cristiane.	
Data: 	2018-06-01	
Ano: 	2018	
Palavras-chave: 	Radiation balance; Urban climate; Energy fluxes.	
Resumo: 	ABSTRACT Green roof is a technology that consists of the use of soil and vegetation installed in the roof of buildings, being a great solution to combat heat islands. Thus, this study aimed to compare micrometeorological changes and their effect on the energy balance of non-vegetated (slab) and vegetated building roofs by means of a simulation model calculated as a function of the reference evapotranspiration (ETo), determined by the Penman-Monteith method. This research was developed between February 1 and September 30, 2016, in the Charles Darwin Building's Parking Garage, Rio Ave Empreendimentos, Recife, PE, Brazil. For this, a weather station was installed on the external building slab. On the slab, sensible, latent, and soil heat fluxes corresponded to 75, 22, and 3%, respectively, of the energy balance. In the simulated green roof, these fluxes reached values of 6, 87, and 7%, respectively. The simulation model allowed determining the energy balance for the green roof, indicating a lower sensible heat flux (69%) and a higher latent heat flux (55%) when compared to those found in the slab.	
Tipo: 	Info:eu-repo/semantics/article	
Idioma: 	Inglês	
Identificador: 	http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162018000300334	
Editor: 	Associação Brasileira de Engenharia Agrícola	
Relação: 	10.1590/1809-4430-eng.agric.v38n3p334-342/2018	
Formato: 	text/html	
Fonte: 	Engenharia Agrícola  v.38 n.3 2018	
Fonte: 	info:eu-repo/semantics/openAccess