Data/hora: 13/06/2024 08:24:25

Provedor de dados: 	Engenharia Agrícola	
País: 	Brazil	
Título: 	Performance of a diesel engine fueled with a preheated blend of soybean oil and petrodiesel	
Autores: 	Delalibera,Hevandro C.; Campolina,Nilson; Weirich Neto,Pedro H.; Ralisch,Ricardo.	
Data: 	2012-12-01	
Ano: 	2012	
Palavras-chave: 	Electronic injection; Opacity; Lubricant.	
Resumo: 	Brazil is doing a major effort to find alternatives to diesel oil as combustible. Some study lines are oriented to the development of vegetable oils used as fuel, as a source of getting cheaper and have higher energy density than the converted vegetable oils, and less risk of environmental contamination. The aim of this study was to evaluate the performance, the useful life of the lubricant and some components of a Diesel Cycle engine, with an electronic injection system, in a long-term test operating with a preheated blend (65°C) of 50% (v v-1) of soybean oil in petrodiesel. There was a reduction of the useful life of the injectors which presented failure because of high wear with 264 hours of operation and showed an increase in emissions of particulate matter (opacity) which may be assigned to the failures occurred in the injection system. An increase in the useful life of the lubricant, when compared with the literature was also observed. The electronic injection system may favor the burning of the tested fuel. The test was interrupted with 264 hours because of failures in the injection system.	
Tipo: 	Info:eu-repo/semantics/article	
Idioma: 	Inglês	
Identificador: 	http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162012000600007	
Editor: 	Associação Brasileira de Engenharia Agrícola	
Relação: 	10.1590/S0100-69162012000600007	
Formato: 	text/html	
Fonte: 	Engenharia Agrícola  v.32 n.6 2012	
Fonte: 	info:eu-repo/semantics/openAccess