Data/hora: 16/06/2024 04:21:43

Provedor de dados: 	70	
País: 	Brazil	
Título: 	EFFECT OF AERATION AND RECIRCULATION IN THE REMOVAL OF NITROGEN AND CHEMICAL OXYGEN DEMAND FROM SANITARY SEWAGE IN A STRUCTURED BED REACTOR	
Autores: 	Leick,Sheilla A.; Oliveira,João G B. De; Tavares,Karoline A.; Lopes,Deize D.; Barana,Ana C.	
Data: 	2017-12-01	
Ano: 	2017	
Palavras-chave: 	Bioreactor; Wastewater; Denitrification; Nitrification; SND (Simultaneous Nitrification and Denitrification).	
Resumo: 	ABSTRACT This study aimed to evaluate a structured bed reactor with intermittent aeration in the simultaneous removal of Chemical Oxygen Demand (COD) and Total Nitrogen (TN) from sanitary sewage. The reactor was operated for 339 days with a Hydraulic Retention Time (HRT) of 12 hours, temperature of 30 ± 1°C and continuous feeding. Nine trials were carried out in which three different effluent recirculation flow (Qr), 3, 2 and 1 time the incoming flow, were evaluated in three different aeration times, of 1h, 2h, and 3h, in 3 hour cycles. The results showed that different recirculation flows and aeration times did not influence the removal of COD, which reached 89%±12. It was observed that the efficiency of TN removal was higher in the tests with higher COD/TKN ratio, between 7.2 and 7.8, reaching TN effluent values of 17 mg.L-1, being 5 mg.L-1 of N-NH4+, 2 mg.L-1 of N-NO2 and 10 mg.L-1 of N-NO3-. It was verified that it is possible to remove the COD and nitrogen from sanitary sewage in a structured bed reactor with intermittent aeration.	
Tipo: 	Info:eu-repo/semantics/article	
Idioma: 	Inglês	
Identificador: 	http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162017000601236	
Editor: 	Associação Brasileira de Engenharia Agrícola	
Relação: 	10.1590/1809-4430-eng.agric.v37n6p1236-1243/2017	
Formato: 	text/html	
Fonte: 	Engenharia Agrícola  v.37 n.6 2017	
Fonte: 	info:eu-repo/semantics/openAccess