Data/hora: 13/06/2024 09:59:34

Provedor de dados: 	70	
País: 	Brazil	
Título: 	Influence of distance, geometry and number of control stations on quality of local geodetic networks for the purpose of georeferencing of rural properties	
Autores: 	Rosalen,David Luciano.	
Data: 	2014-04-01	
Ano: 	2014	
Palavras-chave: 	GNSS baseline Law 10; 267/2001.	
Resumo: 	The implementation of local geodetic networks for georeferencing of rural properties has become a requirement after publication of the Georeferencing Technical Standard by INCRA. According to this standard, the maximum distance of baselines to GNSS L1 receivers is of 20 km. Besides the length of the baseline, the geometry and the number of geodetic control stations are other factors to be considered in the implementation of geodetic networks. Thus, this research aimed to examine the influence of baseline lengths higher than the regulated limit of 20 km, the geometry and the number of control stations on quality of local geodetic networks for georeferencing, and also to demonstrate the importance of using specific tests to evaluate the solution of ambiguities and on the quality of the adjustment. The results indicated that the increasing number of control stations has improved the quality of the network, the geometry has not influenced on the quality and the baseline length has influenced on the quality; however, lengths higher than 20 km has not interrupted the implementation, with GPS L1 receiver, of the local geodetic network for the purpose of georeferencing. Also, the use of different statistical tests, both for the evaluation of the resolution of ambiguities and for the adjustment, have enabled greater clearness in analyzing the results, which allow that unsuitable observations may be eliminated.	
Tipo: 	Info:eu-repo/semantics/article	
Idioma: 	Inglês	
Identificador: 	http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162014000200012	
Editor: 	Associação Brasileira de Engenharia Agrícola	
Relação: 	10.1590/S0100-69162014000200012	
Formato: 	text/html	
Fonte: 	Engenharia Agrícola  v.34 n.2 2014	
Fonte: 	info:eu-repo/semantics/openAccess