Data/hora: 09/06/2024 17:46:59

Provedor de dados: | 90
País: | Brazil
Título: | Rheological Parameters as Affected by Water Tension in Subtropical Soils
Autores: | Pértile,Patricia; Reichert,José Miguel; Gubiani,Paulo Ivonir; Holthusen,Dörthe; Costa,André da.
Data: | 2016-01-01
Ano: | 2016
Palavras-chave: | Soil mechanics; Rheometry; Cohesion; Water content; Capillary forces.
Resumo: | ABSTRACT Rheological parameters have been used to study the interaction between particles and the structural strength of soils subjected to mechanical stresses, in which soil composition and water content most strongly affect soil resistance to deformation. Our objective was to evaluate the effect of water tension on rheological parameters of soils with different mineralogical, physical, and chemical composition. Surface and subsurface horizons of four Oxisols, two Ultisols, one Alfisol, and one Vertisol were physically and chemically characterized; their rheological parameters were obtained from amplitude sweep tests under oscillatory shear on disturbed soil samples that were saturated and subjected to water tension of 1, 3, 6, and 10 kPa. In these samples, the rheological parameters linear viscoelastic deformation limit (γL), maximum shear stress (τmax), and integral z were determined. By simple regression analysis of the rheological parameters as a function of soil water tension, we observed increased mechanical strength with increasing water tension up to at least 6 kPa, primarily due to increased capillary forces in the soil. However, increased elasticity assessed by γL was not as expressive as the increase in structural rigidity assessed by τmax and integral z. Elastic deformation of the soil (γL) increases with the increase in the number of bonds among particles, which depend on the clay, total carbon, expansive clay mineral, and cation contents; however, maximum shear resistance (τmax) and structural stiffness (integral z) mainly increase with clay, kaolinite, and oxide content by increasing the strength of interparticle bonds. A decrease in mechanical strength occurs for water tension of 10 kPa (the lowest water content evaluated) in sandy horizons or in horizons with a high proportion of resistant microaggregates (pseudosand), when associated with low bulk density, due to fewer points of contact between soil particles and therefore lower capillary force.
Tipo: | Info:eu-repo/semantics/article
Idioma: | Inglês
Identificador: | http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-06832016000100411
Editor: | Sociedade Brasileira de Ciência do Solo
Relação: | 10.1590/18069657rbcs20150286
Formato: | text/html
Fonte: | Revista Brasileira de Ciência do Solo  v.40 2016
Fonte: | info:eu-repo/semantics/openAccess