Data/hora: 10/06/2024 06:38:54

Provedor de dados: 	96	
País: 	Brazil	
Título: 	Kinetics of transit and degradation of the fiber from guinea grass silages enriched with waste from soybean pre-cleaning	
Autores: 	Fialho,Filipe Ton; Villela,Severino Delmar Junqueira; Leonel,Fernando de Paula; Tamy,Wagner Pessanha; Araujo,Raphael Pavesi; Machado,Henrique Valentim Nunes.	
Data: 	2015-06-01	
Ano: 	2015	
Palavras-chave: 	By-product; Mathematical models; Mean retention time; True digestibility.	
Resumo: 	The objective was to study the kinetics of transit and degradation of the fiber from guinea grass and the waste from soybean pre-cleaning (WSPC), ensiled with different proportions of mass (0, 100, 150, and 200 g WSPC/kg total mass). Four crossbred (Gyr × Holstein), fistulated cattle with an average body mass of 400±50 kg were organized in a 4 × 4 Latin square experimental design. The fiber utilized in the study of the transit kinetics was stained with chromium mordant, whereas the in situ technique was adopted for the degradation kinetics. The level of inclusion of WSPC only affected the true digestibility and the mean retention time. The addition of waste from soybean pre-cleaning to the silage of guinea grass is beneficial, in terms of kinetics of digestion and passage, at up to levels close to 100 g/kg, because after this quantity the fiber digestion and passage in and through the reticulo-rumen are impaired and there may be alterations in the ruminal environment that will affect the use of silage by animals.	
Tipo: 	Info:eu-repo/semantics/article	
Idioma: 	Inglês	
Identificador: 	http://www.scielo.br/scielo.php?script=sci_arttext&pid=S1516-35982015000600201	
Editor: 	Sociedade Brasileira de Zootecnia	
Relação: 	10.1590/S1806-92902015000600001	
Formato: 	text/html	
Fonte: 	Revista Brasileira de Zootecnia  v.44 n.6 2015	
Fonte: 	info:eu-repo/semantics/openAccess