Consulta: creatorFacets:"Addezio,Francesco Di"
Registros recuperados: 1
Data/hora: 06/06/2024 00:42:57

Sucrose hydrolysis by invertase using a membrane reactor: effect of membrane cut-off on enzyme performance
Provedor de dados: Brazilian Journal of Pharmaceutical Sciences
Autores: Addezio,Francesco Di; Yoriyaz,Ester Junko; Cantarella,Maria; Vitolo,Michele.
Sucrose hydrolysis by invertase [EC.3.2.1.26] produces inverted sugar syrup, an ingredient mainly used in the food industry. To properly catalyze hydrolysis, the enzyme should be reused after this reaction. It is advisable to maintain constant activity over a considerable period. Thus, sucrose hydrolysis was performed in a membrane bioreactor - a continuously stirred tank reactor coupled with an ultrafiltration membrane (UFM) which provides good diffusion and high activity per unit volume. Molecular weight cut-off for soluble invertase UFMs was up to 100kDa. This study focused on the role of UFM invertase cut-off as it is the main element in the process. We demonstrated that both the cut-off and chemical nature of the UFM affected specific invertase...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Invertase; Membrane Reactor; Sucrose/hydrolysis.
Ano: 2014
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S1984-82502014000200257