Consulta: creatorFacets:"Almeida,Ronaldo de"
Registros recuperados: 6
Data/hora: 01/06/2024 01:33:00

Desempenho de um aquecedor solar de água em Manaus
Provedor de dados: 36
Autores: Harwood,John Harry; Almeida,Ronaldo de.
Resumo Um aquecedor solar de água comercial para fins domésticos foi testado em Manaus tanto no verão quanto no inverno. O desempenho foi medido em função da radiação incidente, observando-se a temperatura da água no reservatório e na entrada e na saída do coletor. A velocidade de termossifonagem foi medida através de uma injeção de tinta em tubulação transparente. A eficiência variou durante o dia. O valor máximo observado foi do 58% e valores de 37% são mostrados nos dados analisados em detalhe. O ângulo de inclinação (de 4 até 25°) não teve influência significativa no desempenho dos coletores. Agua quente (150 l) acima de 45°C seria obtida em pelo menos 93% dos dias do ano.
Tipo: Info:eu-repo/semantics/article
Ano: 1981
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0044-59671981000200019

A description of mercury in fishes from the Madeira River Basin, Amazon, Brazil
Provedor de dados: 36
Autores: Bastos,Wanderley Rodrigues; Rebelo,Mauro de Freitas; Fonseca,Márlon de Freitas; Almeida,Ronaldo de; Malm,Olaf.
Over the last 20 years several projects carried on the Madeira River basin in the Amazon produced a great amount data on total Hg concentration in different fish species. In this paper we discuss temporal trends in Hg contamination and its relation to body weight in some of those fishes, showing that even within similar groups, such as carnivorous and non-migratory fish, the interspecies variability in Hg accumulation is considerable.
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Fish; Mercury; Biomagnification; Madeira River; Amazon.
Ano: 2008
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0044-59672008000300006

Flood pulse and spatial dynamics of mercury in sediments in Puruzinho lake, Brazilian Amazon
Provedor de dados: 36
Autores: Almeida,Ronaldo de; Bernardi,José Vicente Elias; Oliveira,Ronaldo Cavalcante; Carvalho,Dario Pires de; Manzatto,Angelo Gilberto; Lacerda,Luiz Drude de; Bastos,Wanderley Rodrigues.
The study was conducted in Puruzinho lake (Humaitá, AM) considering seasonal periods of rainy and dry in way to elucidate the flood pulse importance in the deposition, remobilization and distributions of mercury and organic matter in bottom sediments in the Madeira River Basin (Brazilian Amazon). Bottom sediments and soils samples were analyzed for total mercury and organic matter. Mercury concentrations obtained in bottom sediment were 32.20-146.40 ng g-1 and organic matter values were 3.5 - 18.0%. The main region for accumulation of mercury and organic matter was in the central and deepest lake area In the rainy season there was a greater distribution of Hg and organic matter, mainly controlled by means of income of the Madeira river water during...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Organic matter; Indicator kriging; Madeira river; Seasonality.
Ano: 2014
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0044-59672014000100010

Bomba acionada por um rotor Savonius submerso
Provedor de dados: 36
Autores: Harwood,John H.; Almeida,Ronaldo de.
Resumo A construção de uma bomba de água acionada por correntezas de rios mediante um rotor Savonius submerso está descrita em detalhe. O desenho da bomba é muito simples, de maneira que a construção pode ser feita por qualquer pessoa usando ferramentas manuais. O custo de materiais para fazer uma bomba é de US$ 70,00. Há uma leve variação no desempenho de bombas deste tipo devida à construção artesanal. Contudo uma bomba desenvolvendo potência máxima instalada num local com uma correnteza de 0,6 m.seg.-1 (2,2 km/h) jogou 2100 litros de água por dia a uma altura de 28 m e uma outra bomba instalada num local com uma correnteza de 1.1 m.seg.-1 (4,0 km/ h) jogou 3100 litros de água à mesma altura. Com pressões menores a vazão aumentou até a faixa de 3500 até...
Tipo: Info:eu-repo/semantics/article
Ano: 1982
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0044-59671982000300639

Hidreletricidade do rio Solimões usando um "cata-água"
Provedor de dados: 36
Autores: Harwood,John Harry; Almeida,Ronaldo de.
Summary Eletricity was generated by the current of the Amazon river (rio Solimões) using an apparatus ressembling an underwater windmill. The machine, a free-floating structure ancored to the river-bed, comprised a twelve-bladed, fantype turbine of 2m. diametre held submerged beneath two floates, facing the current. A bicycle chain around the circumference of the turbine transmitted the rotation via multiplying gears to a car alternator. In a current of 0,6 m.s.-1 the power generated was 40 W representing an overall eficiency of 12%. The experiment demonstrates the feasability of generating power from river currents without using dams or waterfalls. The technology is considered highly appropriate to the Amazonian region where a rural eletricity grid is...
Ano: 1981
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0044-59671981000300659

Distribuição espectral e coeficientes de transmissão da radiação solar para condições de céu limpo em Manaus
Provedor de dados: 36
Autores: Almeida,Ronaldo de; Salati,Eneas; Nova,Nilson Augusto Villa.
Resumo Medidas de radiação solar global e direta utilizando-se os filtros OG-530, RG-630 e RG-695 foram realizadas em Manaus-INPA. Os equipamentos disponíveis para estas medidas foram um piranômetro espectral e um pireliômetro de incidência normal da Eppley. Os sinais foram registrados com o auxílio de um potenciógrafo LEEDS e NORTHRUP modelo SPEEDOMAX-W. As medidas foram realizadas em dois dias claros. Com os dados obtidos foi possível estimar a variação horária do coeficiente de transmissão atmosférica correspondente a cada uma das faixas espectrais. Os autores apresentam uma distribuição horária dos fluxos de radiação solar global direta e difusa.
Ano: 1979
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0044-59671979000300279