Consulta: creatorFacets:"Aouji, Oualid"
Registros recuperados: 1
Data/hora: 09/06/2024 11:28:04

A new device to follow temporal variations of oxygen demand in deltaic sediments: the LSCE benthic station
Provedor de dados: Institutional Archive of Ifreme (ArchiMer)
Autores: Toussaint, Flora; Rabouille, Christophe; Cathalot, Cecile; Bombled, Bruno; Abchiche, Abdel; Aouji, Oualid; Buchholtz, Gilles; Clemencon, Aurelien; Geyskens, Nicolas; Repecaud, Michel; Pairaud, Ivane; Verney, Romaric; Tisnerat-laborde, Nadine.
A new benthic station equipped with oxygen microelectrodes and environmental sensors was developed by Laboratoire des Sciences du Climat et de L’Environnement (LSCE) and Division Technique of the Institut National des Sciences de L’Univers (DT-INSU) to perform in situ time series monitoring of sediment oxygen demand, linked to the mineralization of organic matter. The time series typically cover periods of 2-3 months, with a base frequency of 1 set of oxygen profiles per day. The profiling head assessed the lateral heterogeneity of the sediment oxygen demand at the beginning of the time series over a 0.8-m long rectangle to discriminate spatial and temporal variability. A continuous recalibration is performed using a moored oxygen optode anchored to the...
Tipo: Text
Ano: 2014
URL: http://archimer.ifremer.fr/doc/00230/34126/32597.pdf