Consulta: creatorFacets:"Araújo,Jairton F."
Registros recuperados: 1
Data/hora: 13/06/2024 02:12:28

CALIBRATION OF THE THERMAL DISSIPATION PROBE FOR ATEMOYA: (Annona squamosa x A. cherimola)
Provedor de dados: Engenharia Agrícola
Autores: Santos,Irai M. S.; Vellame,Lucas M.; Araújo,Jairton F.; Marinho,Lígia B.
ABSTRACT When determining plant transpiration (TR) using the thermal dissipation probe method, it is necessary to calibrate the sap flow (SF) estimation equation for each species under study, and thus obtain reliable information about the water demand of crops. This study aims to calibrate the equation used to determine SF using the thermal dissipation probe for atemoya cultivation. The experiment was conducted in the experimental field of the Universidade do Estado da Bahia, Juazeiro, Northeast Brazil. Atemoya plants in the initial phase of development were transplanted into 21.5-l pots arranged on weighing platforms that acted as lysimeters. The SF was determined by the thermal dissipation probe method using 1-cm-long probes. The angular coefficient of...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Annonaceous; Sap flow; Lysimeter; Granier method.
Ano: 2020
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162020000400545