Consulta: creatorFacets:"Bacchi,Osny Oliveira Santos"
Registros recuperados: 19
Data/hora: 01/06/2024 17:13:19

Calibração de um equipamento de TDR para medida de umidade de solos
Provedor de dados: 86
Autores: Tommaselli,José Tadeu Garcia; Bacchi,Osny Oliveira Santos.
Este estudo visou à obtenção das curvas de calibração de um equipamento de TDR (Time Domain Reflectometry) em cinco solos da região de Piracicaba, SP, e testou a adequação da calibração interna do equipamento e das curvas genéricas de calibração. As curvas ajustadas, em cada solo separadamente, apresentaram coeficientes de determinação (R²) da ordem de 0,99, e a curva ajustada para o conjunto de dados dos cinco solos apresentou R² = 0,976. A análise de erros-padrão de estimativa mostrou que as curvas genéricas não se prestam às aplicações mais sensíveis, tais como na determinação absoluta do conteúdo de água do solo. Os testes de comparação entre as curvas ajustadas, a curva genérica e a curva embutida no equipamento mostraram que a primeira é superior às...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Propriedades dielétricas; Conteúdo de água do solo; Instrumento de medição.
Ano: 2001
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-204X2001000900008

Mudanças na estrutura do solo avaliada com uso de tomografia computadorizada
Provedor de dados: 86
Autores: Pires,Luiz Fernando; Bacchi,Osny Oliveira Santos.
O objetivo deste trabalho foi avaliar, em escala milimétrica, a modificação da densidade e da porosidade de amostras deformadas de solo submetidas a ciclos de umedecimento e secamento (U-S), por meio da tomografia computadorizada de raios gama. Amostras com 98,1 cm³ foram preparadas procedendo ao peneiramento do solo em malha de 2 mm e acondicionamento de forma homogênea em tubos de PVC. As amostras de solo foram submetidas a um, dois e três ciclos de U-S. As amostras controle não foram submetidas a nenhum ciclo de U-S. Após a aplicação dos ciclos de U-S, a porosidade das amostras diminuiu e as camadas de solo se adensaram. Os dados de tomografia computadorizada permitiram análise contínua da densidade do solo e de sua porosidade, em camadas milimétricas...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Análise de imagens; Atenuação de raios gama; Ciclos de umedecimento e secamento; Densidade do solo; Porosidade do solo.
Ano: 2010
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-204X2010000400007

Fertilizer 15N balance in a coffee cropping system: a case study in Brazil
Provedor de dados: 90
Autores: Fenilli,Tatiele Anete Bergamo; Reichardt,Klaus; Favarin,José Laércio; Bacchi,Osny Oliveira Santos; Silva,Adriana Lúcia; Timm,Luis Carlos.
Knowledge about the fate of fertilizer nitrogen in agricultural systems is essential for the improvement of management practices in order to maximize nitrogen (N) recovery by the crop and reduce N losses from the system to a minimum. This study involves fertilizer management practices using the 15N isotope label applied in a single rate to determine the fertilizer-N balance in a particular soil-coffee-atmosphere system and to deepen the understanding of N plant dynamics. Five replicates consisting of plots of about 120 plants each were randomly defined within a 0.2 ha coffee plantation planted in 2001, in Piracicaba, SP, Brazil. Nine plants of each plot were separated in sub-plots for the 15N balance studies and treated with N rates of 280 and 350 kg ha-1...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Coffee crop; Nitrogen uptake; N dynamics; 15N tracer studies; Stable isotope.
Ano: 2008
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-06832008000400010

Avaliação do uso de resíduos de construção e demolição reciclados como corretivo da acidez do solo
Provedor de dados: 90
Autores: Lasso,Paulo Renato Orlandi; Vaz,Carlos Manoel Pedro; Bernardi,Alberto Carlos de Campos; Oliveira,Cauê Ribeiro de; Bacchi,Osny Oliveira Santos.
A geração e o armazenamento de resíduos de construção civil e demolição (RCD) constituem-se em um problema ambiental, pois representam mais de 50 % do total de resíduos sólidos gerados nos médios e grandes centros urbanos. Porém, como o calcário é uma das principais matérias-primas utilizadas na fabricação do cimento e da cal hidratada e, consequentemente, de concretos, argamassas e reboques, a reciclagem desses materiais pode fornecer, em princípio, um subproduto com potencial para correção da acidez dos solos. Este estudo teve o objetivo de avaliar a utilização de resíduos de construção e demolição reciclados como corretivos de acidez do solo. Utilizaram-se RCD-R provenientes de concretos, argamassas e reboques (material cinza), que foram caracterizados...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Reciclagem; Calcário; Cimento; Cal; Agricultura.
Ano: 2013
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-06832013000600022

Method to estimate soil macroporosity and microporosity based on sand content and bulk density
Provedor de dados: 90
Autores: Stolf,Rubismar; Thurler,Álvaro de Mendonça; Bacchi,Osny Oliveira Santos; Reichardt,Klaus.
Macroporosity is often used in the determination of soil compaction. Reduced macroporosity can lead to poor drainage, low root aeration and soil degradation. The aim of this study was to develop and test different models to estimate macro and microporosity efficiently, using multiple regression. Ten soils were selected within a large range of textures: sand (Sa) 0.07-0.84; silt 0.03-0.24; clay 0.13-0.78 kg kg-1 and subjected to three compaction levels (three bulk densities, BD). Two models with similar accuracy were selected, with a mean error of about 0.02 m³ m-3 (2 %). The model y = a + b.BD + c.Sa, named model 2, was selected for its simplicity to estimate Macro (Ma), Micro (Mi) or total porosity (TP): Ma = 0.693 - 0.465 BD + 0.212 Sa; Mi = 0.337 +...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Degree of compaction; Modeling; Macropore; Texture; Maximum bulk density; Relative bulk density.
Ano: 2011
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-06832011000200014

A software to calculate soil hydraulic conductivity in internal drainage experiments (SHC, Version 2.00)
Provedor de dados: 90
Autores: Dourado Neto,Durval; Reichardt,Klaus; Silva,Adriana Lúcia da; Bacchi,Osny Oliveira Santos; Timm,Luis Carlos; Oliveira,Júlio César Martins; Nielsen,Donald R.
A software for the calculation of unsaturated soil hydraulic conductivity K(theta) is presented for commonly used methods found in the literature, based on field experiments in which a soil profile is submitted to water infiltration followed by internal drainage. The software is available at: dourado@esalq.usp.br.
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Internal drainage; Soil water content; Water infiltration.
Ano: 2007
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-06832007000500037

Soil hydraulic conductivily measurement on a sloping field
Provedor de dados: 91
Autores: Timm,Luís Carlos; Oliveira,Julio Cesar Martins de; Tominaga,Tânia Toyomi; Cássaro,Fábio Augusto Meira; Reichardt,Klaus; Bacchi,Osny Oliveira Santos.
A field methodology is presented for the measurement of the soil hydraulic conductivity in a sloping field, minimizing the leveling soil movement before water pounding and redistribution. The assurance of vertical flow only is performed through soil water potential isolines. The hydraulic conductivity was determined by the instantaneous profile method. Results for the nine neutron probe access tubes indicate that one single K(theta) relation is sufficient to represent the experimental site.
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Hydraulic conductivity; Slope; Neutron probe.
Ano: 2000
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S1415-43662000000300027

Growth, development, and fertilizer-15N recovery by the coffee plant
Provedor de dados: 63
Autores: Fenilli,Tatiele Anete Bergamo; Reichardt,Klaus; Dourado-Neto,Durval; Trivelin,Paulo César Ocheuze; Favarin,José Laercio; Costa,Flávio Murilo Pereira da; Bacchi,Osny Oliveira Santos.
The relationship between growth and fertilizer nitrogen recovery by perenial crops such as coffee is poorly understood and improved understanding of such relations is important for the establishment of rational crop management practices. In order to characterize the growth of a typical coffee crop in Brazil and quantify the recovery of 15N labeled ammonium sulfate, and improve information for fertilizer management practices this study presents results for two consecutive cropping years, fertilized with 280 and 350 kg ha-1 of N, respectively, applied in four splittings, using five replicates. Shoot dry matter accumulation was evaluated every 60 days, separating plants into branches, leaves and fruits. Labeled sub-plots were used to evaluate N-total and 15N...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Coffea arabica L.; Stable isotope; Nitrogen; Dry matter accumulation; 15N.
Ano: 2007
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0103-90162007000500012

Distribuição do sistema radicular de uma cultura de aveia forrageira
Provedor de dados: 63
Autores: Fante Jr.,Lorival; Reichardt,Klaus; Jorge,Lucio André de Castro; Bacchi,Osny Oliveira Santos.
Avaliou-se a distribuição das raízes de uma aveia forrageira através da aplicação dos métodos do anel volumétrico, da placa com pregos, do trado e do auxiliado por processamento de imagens. A aveia forrageira foi cultivada em latossolo vermelho-escuro, sob dois tratamentos distintos em função da manutenção da capacidade de água disponível no solo (CAD): tratamento 1 - 50% da CAD; tratamento 2 - 80% da CAD. Foram realizadas 3 amostragens, aos 25, 60 e 115 dias após a emergência. As raízes da aveia forrageira concentraram-se nas camadas iniciais do solo, cerca de 90% entre 0 a 20 cm. Os resultados encontrados para a quantificação das raízes variaram com o tratamento, a metodologia e a época de amostragem. Verificou-se a existência de correlações entre os...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Aveia forrageira; Sistema radicular; Processamento de imagem; Água do solo.
Ano: 1999
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0103-90161999000500010

State-space approach for the analysis of soil water content and temperature in a sugarcane crop
Provedor de dados: 63
Autores: Dourado-Neto,Durval; Timm,Luís Carlos; Oliveira,Julio Cesar Martins de; Reichardt,Klaus; Bacchi,Osny Oliveira Santos; Tominaga,Tania Toyomi; Cássaro,Fabio Augusto Meira.
The state-space approach is used to describe surface soil water content and temperature behaviour, in a field experiment in which sugarcane is submitted to different management practices. The treatments consisted of harvest trash mulching, bare soil, and burned trash, all three in a ratoon crop, after first cane harvest. One transect of 84 points was sampled, meter by meter, covering all treatments and borders. The state-space approach is described in detail and the results show that soil water contents measured along the transect could successfully be estimated from water content and temperature observations made at the first neighbour.
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Soil water; Soil temperature; State-space; Transect.
Ano: 1999
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0103-90161999000500025

Software to model soil water retention curves (SWRC, version 2.00)
Provedor de dados: 63
Autores: Dourado-Neto,Durval; Nielsen,Donald R.; Hopmans,Jan W.; Reichardt,Klaus; Bacchi,Osny Oliveira Santos.
A software for the adjustment of soil water retention curves (SWRC) is presented, using twelve models found in the literature.
Tipo: Info:eu-repo/semantics/report
Palavras-chave: Soil matric potential; Soil water content; Retention.
Ano: 2000
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0103-90162000000100031

Variability of water balance components in a coffee crop in Brazil
Provedor de dados: 63
Autores: Silva,Adriana Lúcia da; Roveratti,Renato; Reichardt,Klaus; Bacchi,Osny Oliveira Santos; Timm,Luis Carlos; Bruno,Isabeli Pereira; Oliveira,Julio César Martins; Dourado Neto,Durval.
Establishing field water balances is difficult and costly, the variability of their components being the major problem to obtain reliable results. This component variability is presented herein for a coffee crop grown in the Southern Hemisphere, on a tropical soil with 10% slope. It was observed that: rainfall has to be measured with an appropriate number of replicates; irrigation can introduce great variability into calculations; evapotranspiration, calculated as a remainder of the water balance equation, has exceedingly high coefficients of variation; the soil water storage component is the major contributor in error propagation calculations to estimate evapotranspiration; and that runoff can be satisfactorily controlled on the 10% slope through crop...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Component variability; Rainfall; Evapotranspiration; Soil water storage.
Ano: 2006
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0103-90162006000200001

EXACT EQUATIONS FOR SOIL PARTICLE-SIZE ANALYSIS BY GAMMA-RAY ATTENUATION
Provedor de dados: 63
Autores: Elias,Elimoel Abraão; Bacchi,Osny Oliveira Santos; Reichardt,Klaus.
Soil particle-size analysis by gamma-ray attenuation was first suggested in 1992 and improved in 1997 by diminishing the measurement time and adapting it for automation. It is here demonstrated that when the mass attenuation coefficient &lt;FONT FACE="Symbol"&gt;m&lt;/font&gt;w and the density Dw are replaced by &lt;FONT FACE="Symbol"&gt;m&lt;/font&gt;s and Ds (where the subscripts w and s stand for water and solution) in the approximate equations used to estimate the concentration of suspended particles, they become exact. The demonstration is based by treating the dispersant and water solution as one single medium, instead of treating them as two media. In this way, six variables are reduced to only three. Physical considerations suggest that the...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Granulometry; Soil mechanical analysis; Soil texture; Gamma attenuation.
Ano: 1999
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0103-90161999000100014

Random and systematic spatial variability of 137Cs inventories at reference sites in South-Central Brazil
Provedor de dados: 63
Autores: Correchel,Vladia; Bacchi,Osny Oliveira Santos; Reichardt,Klaus; De Maria,Isabella Clerici.
The precision of the 137Cs fallout redistribution technique for the evaluation of soil erosion rates is strongly dependent on the quality of an average inventory taken at a representative reference site. The knowledge of the sources and of the degree of variation of the 137Cs fallout spatial distribution plays an important role on its use. Four reference sites were selected in the South-Central region of Brazil which were characterized in terms of soil chemical, physical and mineralogical aspects as well as the spatial variability of 137Cs inventories. Some important differences in the patterns of 137Cs depth distribution in the soil profiles of the different sites were found. They are probably associated to chemical, physical, mineralogical and biological...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Cesium-137; Spatial distribution; Radioisotope; Sediment; Radioactive tracer.
Ano: 2005
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0103-90162005000200013

Soil spatial variability and the estimation of the irrigation water depth
Provedor de dados: 63
Autores: Reichardt,Klaus; Silva,José Carlos de Araújo; Bassoi,Luis Henrique; Timm,Luís Carlos; Oliveira,Julio Cesar Martins de; Bacchi,Osny Oliveira Santos; Pilotto,João Eduardo.
The effects of soil water spatial variability previous to irrigation and of the field capacity on the estimation of irrigation water depth are evaluated. The experiment consisted of a common bean (Phaseolus vulgaris L.) crop established on a Kandiudalfic Eutrudox of Piracicaba, SP, Brazil, irrigated by central pivot, in which soil water contents were evaluated with a depth neutron gauge, in a grid of 20x4 points with lag of 0.5 m. In a given situation, the 80 calculated irrigation water depths presented a coefficient of variation of 29.3%, with an average water value of 18 mm, maximum of 41mm and minimum of 9 mm. It is concluded that the only practical way of irrigation is the use of an average water depth, due to the inherent variability of the soil, and...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Irrigation water depth; Field capacity; Spatial variability.
Ano: 2001
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0103-90162001000300017

Interação solo-planta avaliada por modelagem estatística de espaço de estados
Provedor de dados: 63
Autores: Timm,Luis Carlos; Fante Jr.,Lorival; Barbosa,Emanuel Pimentel; Reichardt,Klaus; Bacchi,Osny Oliveira Santos.
Para estudar a interação solo-planta utilizou-se um modelo de espaço de estados (regressão dinâmica) comparativamente à um modelo de regressão estática, em versão convencional e em versão sequencial. Para tal, foram utilizados dados experimentais de densidade do solo, macroporosidade, microporosidade e porosidade total de um solo Latossolo Vermelho Escuro, além da densidade radicular por comprimento de raiz por unidade de volume, de uma cultura de aveia forrageira. Das variáveis explanatórias estudadas, a porosidade total apresentou correlação bastante significativa com a densidade radicular, considerada como a variável resposta do estudo. Um modelo de regressão estática representado na forma de espaço de estados com estimação seqüencial forneceu um...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Variabilidade espacial; Regressão dinâmica; Regressão estática; Estimação seqüencial.
Ano: 2000
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0103-90162000000400025

Comparison between climatological and field water balances for a coffee crop
Provedor de dados: 63
Autores: Bruno,Isabeli Pereira; Silva,Adriana Lúcia da; Reichardt,Klaus; Dourado-Neto,Durval; Bacchi,Osny Oliveira Santos; Volpe,Clóvis Alberto.
The use of climatological water balances in substitution to complete water balances directly measured in the field allows a more practical crop management, since the climatological water balances are based on data monitored as a routine. This study makes a comparison between these methods in terms of estimatives of evapotranspiration, soil water storage, soil available water, runoff losses, and drainage below root zone, during a two year period, taking as an example a coffee crop of the variety Catuaí, three to five years old. Climatological water balances based on the estimation of the evapotranspiration through the methods of Thornthwaite and Penman-Monteith, can reasonably substitute field measured balances, however underestimating the above mentioned...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Evapotranspiration; Soil water storage; Available water; Water deficit; Water excess.
Ano: 2007
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0103-90162007000300001

Field spatial and temporal patterns of soil water content and bulk density changes
Provedor de dados: 63
Autores: Timm,Luís Carlos; Pires,Luiz Fernando; Roveratti,Renato; Arthur,Robson Clayton Jacques; Reichardt,Klaus; Oliveira,Júlio Cesar Martins de; Bacchi,Osny Oliveira Santos.
Soil water content (theta) and bulk density (rhos) greatly influence important soil and plant processes, such as water movement, soil compaction, soil aeration, and plant root system development. Spatial and temporal variability of theta and rhos during different periods of the year and different phases of crops are of fundamental interest. This work involves the characterization of spatial and temporal patterns of theta and rhos during different climatic periods of year, aiming to verify whether there are significant temporal changes in rhos at the soil surface layer when submitted to wetting and drying cycles. The field experiment was carried out in a coffee plantation, Rhodic Kandiudalf soil, clayey texture. Using a neutron/gamma surface probe, theta...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Neutron/gamma surface probe; Wetting/drying cycles; Spatial and temporal variability.
Ano: 2006
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0103-90162006000100009

Estimativa de fluxos de água em solos não saturados
Provedor de dados: 53
Autores: Reichardt,Klaus; Bacchi,Osny Oliveira Santos; Villagra,Maria Mercedes.
Com dados obtidos em perfis de terra roxa estruturada do município de Piracicaba (SP), é mostrada a dificuldade da estimativa de fluxos de água no solo, utilizando o modelo de Darcy-Buckingham. O experimento trata do estabelecimento de balanços hídricos em 25 parcelas de 5 x 5 m, alinhadas ao longo de uma transeção de 125 m. O componente drenagem profunda do balanço hídrico é estimado mediante medidas de umidade do solo (teta, cm³/cm³), feitas com sonda de nêutrons, e de potencial total da água do solo H (cm H2O) obtidas com tensiômetros. O trabalho mostra a grande dificuldade da estimativa de fluxos de drenagem q (mm/dia), a qual está relacionada: (1) à exponencialidade da relação entre a condutividade hidráulica do solo k (mm/dia) e a umidade do solo ou...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Condutividade hidráulica do solo; Equação de Darcy.
Ano: 1993
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0006-87051993000100010