Consulta: creatorFacets:"Bombled, Bruno"
Registros recuperados: 2
Data/hora: 09/06/2024 10:47:55

Etude pilote des apports en contaminants par la Seine : niveaux de contamination, variations saisonnières et flux d'éléments traces a poses en 1990 et 1991
Provedor de dados: Institutional Archive of Ifreme (ArchiMer)
Autores: Bombled, Bruno; Cossa, Daniel.
Le présent rapport constitue une première présentation des résultats de l'Etude pilote des apports en contaminants par la Seine. Il est consacré aux métaux et à l'arsenic et traite de leurs niveaux de concentration, de leurs variations saisonnières et des flux à l'estuaire. Il comporte des fiches-annexes qui contiennent les méthodes de prélèvement, de filtration et de dosage ainsi que des résumés des résultats. A partir des conclusions, des recommandations sont faites quant aux méthodes à privilégier pour tirer les meilleurs enseignements du suivi des contaminants métalliques et de l'arsenic à la limite amont de l'estuaire de la Seine. Les données contenues dans ce rapport ont été produites par la Cellule de lutte contre la pollution (Service de navigation...
Tipo: Text
Ano: 1992
URL: http://archimer.ifremer.fr/doc/00131/24272/22270.pdf

A new device to follow temporal variations of oxygen demand in deltaic sediments: the LSCE benthic station
Provedor de dados: Institutional Archive of Ifreme (ArchiMer)
Autores: Toussaint, Flora; Rabouille, Christophe; Cathalot, Cecile; Bombled, Bruno; Abchiche, Abdel; Aouji, Oualid; Buchholtz, Gilles; Clemencon, Aurelien; Geyskens, Nicolas; Repecaud, Michel; Pairaud, Ivane; Verney, Romaric; Tisnerat-laborde, Nadine.
A new benthic station equipped with oxygen microelectrodes and environmental sensors was developed by Laboratoire des Sciences du Climat et de L’Environnement (LSCE) and Division Technique of the Institut National des Sciences de L’Univers (DT-INSU) to perform in situ time series monitoring of sediment oxygen demand, linked to the mineralization of organic matter. The time series typically cover periods of 2-3 months, with a base frequency of 1 set of oxygen profiles per day. The profiling head assessed the lateral heterogeneity of the sediment oxygen demand at the beginning of the time series over a 0.8-m long rectangle to discriminate spatial and temporal variability. A continuous recalibration is performed using a moored oxygen optode anchored to the...
Tipo: Text
Ano: 2014
URL: http://archimer.ifremer.fr/doc/00230/34126/32597.pdf