Consulta: creatorFacets:"COSTA,CLAUDIO"
Registros recuperados: 1
Data/hora: 16/06/2024 06:54:08

Accuracy of linear measurements performed with two imaging software in cone-beam computed tomography scans of dry human mandibles
Provedor de dados: 42
Autores: SILVA,ALESSANDRO A.L.S.; FRANCO,ADEMIR; FERNANDES,ÂNGELA; COSTA,CLAUDIO; BARBOSA,JORGE S.; WESTPHALEN,FERNANDO H.
ABSTRACT The present study aimed to assess the accuracy of linear measurements performed with two software packages in multislice (MSCT) and cone beam (CBCT) computed tomography (CT) images. The sample consisted of 10 human mandibles marked standardly 8 times with metallic orthodontic wires. The mandibles underwent both MSCT and CBCT scanning and were measured linearly and digitally with two software packages, namely Studio 3.1® (Anne Solutions®, SP, Brazil) (ST) and Implant Viewer 2.817® (Anne Solutions®, SP, Brazil) (IV). The linear measurements were the mandibular height (MH) and width (MW), and the distance from the alveolar ridge to the mandibular canal (AC). To validate the measurements, the mandibles were sectioned in the marked regions and measured...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Computed tomography; Dental implant; Morphology; Radiology.
Ano: 2017
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0001-37652017000602865