Consulta: creatorFacets:"Cuq, Veronique"
Registros recuperados: 3
Data/hora: 01/06/2024 02:49:22

Bilan des tempêtes de l’hiver 2013-2014 sur la dynamique de recul du trait de côte en Bretagne
Provedor de dados: Institutional Archive of Ifreme (ArchiMer)
Autores: Blaise, Emmanuel; Suanez, Serge; Stephan, Pierre; Fichaut, Bernard; David, Laurence; Cuq, Veronique; Autret, Ronan; Houron, Julien; Rouan, Mathias; Floc'H, France; Ardhuin, Fabrice; Cancouet, Romain; Davidson, Robert; Costa, Stephane; Delacourt, Christophe.
Between December 2013 and March 2014, a cluster of about 12 storm events hit the coast of Brittany with an exceptional frequency. It was in February that these storm events were the most frequent and particularly virulent. The significant wave heights measured off Finistere reached respectively 12.3 m and 12.4 m during Petra and Ulla storms on February 5 and 14. However, analysis of hydrodynamic conditions shows that only three episodes promoted extreme morphogenetic conditions because they were combined with high spring tide level. The first one occurred on January 1 to 4, it was followed by events from February 1 to 3, and March 2-3. During these three extreme events observed tide levels were above highest astronomical tide level (HAT). Maximum surge...
Tipo: Text
Palavras-chave: Tempête; Érosion; Trait de côte; Marée de vive-eau; Bretagne; Surcote; Storm; High spring tide; Surge; Erosion; Shoreline; Brittany.
Ano: 2015
URL: http://archimer.ifremer.fr/doc/00310/42171/43029.pdf

Adequacy of pseudo-direct georeferencing of terrestrial laser scanning data for coastal landscape surveying against indirect georeferencing
Provedor de dados: Institutional Archive of Ifreme (ArchiMer)
Autores: Jaud, Marion; Letortu, Pauline; Augereau, Emmanuel; Le Dantec, Nicolas; Beauverger, Mickael; Cuq, Veronique; Prunier, Christophe; Le Bivic, Rejanne; Delacourt, Christophe.
The georeferencing process is crucial to the accuracy of terrestrial laser scanner (TLS) data, in particular in the context of diachronic studies relying on multi-temporal surveys. The use of Ground Control Points in the georeferencing process can however be complex when confronted with the practical constraints of coastal surveying. A simple and quick alternative method called "pseudo-direct georeferencing" is proposed in the present paper. This method involves internal inclinometers to measure roll and pitch angles and a centimetric GPS to measure the position of the TLS center and the position of one backsight target. When assessing the transformational uncertainty by using a set of independent ground validation points for both classical indirect and...
Tipo: Text
Palavras-chave: Terrestrial laser scanning; Coastal monitoring; Direct georeferencing; Indirect georeferencing; Multi-temporal surveys; Geomorphological evolution.
Ano: 2017
URL: https://archimer.ifremer.fr/doc/00638/75050/75683.pdf

Diachronic UAV Photogrammetry of a Sandy Beach in Brittany (France) for a Long-Term Coastal Observatory
Provedor de dados: Institutional Archive of Ifreme (ArchiMer)
Autores: Jaud, Marion; Delacourt, Christophe; Le Dantec, Nicolas; Allemand, Pascal; Ammann, Jerome; Grandjean, Philippe; Nouaille, Henri; Prunier, Christophe; Cuq, Veronique; Augereau, Emmanuel; Cocquempot, Lucie; Floc'H, France.
In the dual context of coastal hazard intensification and the growing number of stakes exposed to these hazards, coastal observatories are in demand to provide a structured framework dedicated to long-term monitoring. This article describes the drone-based photogrammetry monitoring performed since 2006 on Porsmilin Beach (Brittany, France) in the framework of the DYNALIT (Littoral and Coastline Dynamics) observatory, focusing on data quality and the consistency of long-term time series under the influence of multiple technological evolutions: Unmanned Aerial Vehicles (UAV) platforms with the arrival of electric multirotor drones, processing tools with the development of structure-from-motion (SfM) photogrammetry, and operational modes of survey. A study...
Tipo: Text
Palavras-chave: UAV; SfM photogrammetry; Coastal observatory; Beach monitoring.
Ano: 2019
URL: https://archimer.ifremer.fr/doc/00637/74927/76116.pdf