Consulta: creatorFacets:"Gomes,Benedito M."
Registros recuperados: 12
Data/hora: 09/06/2024 16:49:15

STREAMFLOW REGIONALIZATION IN PIQUIRI RIVER BASIN
Provedor de dados: 70
Autores: Araujo,Fernanda C.; Mello,Eloy L. de; Gollin,Gisele M.; Quadros,Luciana E. de; Gomes,Benedito M.
ABSTRACT The objective of this study was to regionalize 7-day 10-year low flows, long-term annual mean, and 90% and 95% permanence flows from Piquiri (PR) river basin. The following regionalization methods were adopted: Traditional, Linear interpolation, Chaves, Modified linear interpolation, and Modified Chaves. The equations obtained by the Traditional method, adding main river length or drainage density as independent variables, significantly improved R2 equations value. Streamflow forecasting by Linear Interpolation and Chaves methods were as good as those provided by the Traditional Method, thus, these methods could be applied to Piquiri River basin, especially when drainage area is the only available spatial information.
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Water availability; Water resources management; Average streamflow; Low flows; Flows permanence.
Ano: 2018
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162018000100022

Selection of microorganisms producer of lipase for fat removal from biodiesel purification water
Provedor de dados: 70
Autores: Rocha,Dayane C. da; Gomes,Benedito M.; D.Gomes,Simone; Sene,Luciane; Zenatti,Dilcemara C.
The objective this study has been the selection of lipase productor microorganism, for removal of oils and grease, in the pre-treatment of biodiesel wastewater washing. For this, analyses of the physicist-chemistries characteristics had been made with the wastewater of the biodiesel washing, and then it had been isolated and chosen, by means of determinations of the lipase activity. Following, it was made a test of fat biodegradation, in the conditions: pH (5.95), temperature (35 ºC), rotation (180 rpm) and ammonium sulfate as nitrogen source (3 g L-1) and establishing as variable the two microorganism preselected and the time (24; 48; 72; 96 and 120 h). The biodiesel purification wastewater had presented high potential of environmental impact, presenting...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Enzymatic degradation; Fatty effluent; Lipolytical activity.
Ano: 2013
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162013000200012

Turbidimetry as an alternative method to determine the rating curve of suspended sediments
Provedor de dados: 70
Autores: Poletto,Kayla; Sampaio,Silvio C.; Queiroz,Manoel M. F. de; Gomes,Benedito M.; Soncela,Rosimaldo.
Understanding hydrosedimental behavior of a watershed is essential for properly managing and using its hydric resources. The objective of this study was to verify the feasibility of the alternative procedure for the indirect determination of the sediment key curve using a turbidimeter. The research was carried out on the São Francisco Falso River, which is situated in the west of the state of Paraná on the left bank of ITAIPU reservoir. The direct method was applied using a DH-48 sediment suspended sampler. The indirect method consisted of the use of a linigraph and a turbidimeter. Based on the results obtained, it was concluded that the indirect method using a turbidimeter showed to be fully feasible, since it gave a power function-type mathematical model...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Watershed; Hydrosedimentalogy; Agriculture.
Ano: 2011
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162011000300019

Variação espacial e temporal dos fatores limnológicos em riachos da microbacia do rio São Francisco Verdadeiro
Provedor de dados: 70
Autores: Oliveira,Luciano C. de; Gomes,Benedito M.; Baumgartner,Gilmar; Sebastien,Nyamien Y.
Com objetivo de caracterizar espacial e temporalmente os riachos da microbacia do rio São Francisco Verdadeiro, Marechal Cândido Rondon - PR, em função de fatores limnológicos, foram estabelecidas seis estações de coleta em três riachos (Curvado, Ajuricaba e Arroio Fundo), sendo uma estação na foz e outra na nascente. As coletas de água foram obtidas entre junho de 2005 e maio de 2006, totalizando 72 amostras. Foram analisadas as seguintes variáveis: temperatura, pH, condutividade elétrica, oxigênio dissolvido, turbidez, material em suspensão, fósforo total dissolvido, ortofosfato, nitrogênio total e nitrogênio amoniacal. De acordo com a análise de variância, houve baixa variabilidade entre as estações de coleta, porém a variação temporal demonstrou a...
Tipo: Info:eu-repo/semantics/report
Palavras-chave: Variáveis físicas e químicas; Limnologia; Material alóctone.
Ano: 2008
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162008000400017

Kinetic behavior of nitrification in the post-treatment of poultry wastewater in a sequential batch reactor
Provedor de dados: 70
Autores: Mees,Juliana B. R.; Gomes,Simone D.; Vilas Boas,Márcio A.; Gomes,Benedito M.; Passig,Fernando H.
A sequential batch reactor with suspended biomass and useful volume of 5 L was used in the removal of nutrients and organic matter in workbench scale under optimal conditions obtained by central composite rotational design (CCRD), with cycle time (CT) of 16 h (10.15 h, aerobic phase, and 4.35 h, anoxic phase) and carbon: nitrogen ratio (COD/NO2--N+NO3--N) equal to 6. Complete cycles (20), nitrification followed by denitrification, were evaluated to investigate the kinetic behavior of degradation of organic (COD) and nitrogenated (NH4+-N, NO2--N and NO3--N) matter present in the effluent from a bird slaughterhouse and industrial processing facility, as well as to evaluate the stability of the reactor using Shewhart control charts of individual measures. The...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Nitrifying activity; Kinetic constants; Nutrient removal; Quality control; Processing capacity.
Ano: 2011
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162011000500013

Application of response surface methodology to study the biological removal of nitrogen from effluent of cattle slaughterhouse in a sequencing batch reactor
Provedor de dados: 70
Autores: Lima,Adriana N. de; Gomes,Benedito M.; Gomes,Simone D.; Carvalho,Karina Q. de; Christ,Divair.
The aim of this study was to evaluate the efficiency of a sequencing batch reactor (SBR) on biological removal of nitrogen from cattle slaughterhouse wastewater by nitrification/denitrification processes. The effects of initial concentration of ammoniacal nitrogen were investigated at 100; 150 and 200 mg L-1 and air flow rate at 0.125; 0.375 and 0.625 L min¹ Lreactor-1 on the nitrogen compounds removal, by a Central Composite Rotational Design (CCRD) configuration. There were variations from 9.2 to 94.9%, 4.0 to 19.6% and 20.8 to 92.0% in the conversion of ammoniacal nitrogen to nitrate and nitrite concentration and removal of total nitrogen, respectively. The increase of air flow rate and decrease of the initial concentration of ammoniacal nitrogen...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Nitrification; Denitrification; Central composite rotational design.
Ano: 2014
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162014000200017

COMPARISON OF METHODS FOR ESTIMATING REFERENCE EVAPOTRANSPIRATION: AN APPROACH TO THE MANAGEMENT OF WATER RESOURCES WITHIN AN EXPERIMENTAL BASIN IN THE BRAZILIAN CERRADO
Provedor de dados: 70
Autores: Gotardo,Jackeline T.; Rodrigues,Lineu N.; Gomes,Benedito M.
ABSTRACT This study aimed to compare methods for estimating reference evapotranspiration using an experimental basin in the Brazilian Cerrado, for water management purposes. For that, we estimated daily reference evapotranspiration over a certain period (time series between 1982 and 2012) through different empirical methods. These methods consisted of Blaney-Criddle (BC), Hargreaves &amp; Samani (HS), ASCE Penman-Monteith (ASCE- PM), Penman (1948/1963) (PO), Priestley-Taylor (PT), which were all compared to the standard Penman-Monteith FAO-56 (PM-FAO56). Based on statistics, ASCE- PM, P and BC methods should be recommended for cerrado areas, either in rainy or dry seasons. After these, the PT also stood out. Among the less complex methods, based on...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Evapotranspiration; Methods; Penman-Monteith FAO-56.
Ano: 2016
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162016000601016

Anaerobic co-digestion of crude glycerin and starch industry effluent
Provedor de dados: 70
Autores: Larsen,Andrea C.; Gomes,Benedito M.; Gomes,Simone D.; Zenatti,Dilcemara C.; Torres,Douglas G. B.
The Brazil's Biodiesel Production and Use Program introduces biodiesel in the Brazilian energy matrix, bringing along the perspective of a growth of the glycerin offer, co-product generated in the proportion of 10 kg for each 100 L of biodiesel. The aim of this study was to evaluate the addition of crude glycerin in the anaerobic digestion of cassava starch industry effluent (cassava wastewater), in a horizontal semi-continuous flow reactor of one phase in laboratory scale. It was used a reactor with a 8.77 L of useful volume, a medium support for corrugated conduit of polyvinyl chloride (PVC), temperature of 261 ºC, fed with cassava wastewater and glycerin, with hydraulic detention times of 4 and 5 days and increasing volumetric organic load of 3.05;...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Cassava wastewater; Biodiesel; Biogas; Glycerol.
Ano: 2013
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-69162013000200013

Características químicas de solo cultivado com soja e irrigado com água residuária da suinocultura
Provedor de dados: 91
Autores: Caovilla,Franciele A.; Sampaio,Silvio C.; Smanhotto,Adriana; Nóbrega,Lúcia H. P.; Queiroz,Manoel M. F. de; Gomes,Benedito M.
Neste trabalho se avaliou a distribuição "in situ" de fósforo (P), matéria orgânica (MO), potássio (K), cálcio (Ca), magnésio (Mg), capacidade de troca catiônica (T), alumínio (Al), soma de bases (S), saturação por bases (V) e do pH, em um solo cultivado com soja irrigada com água residuária proveniente da suinocultura (ARS), com níveis de concentração de 0, 25, 50 e 75%. Constituiu-se um esquema fatorial a partir dos quatros níveis de concentração da ARS, das profundidades de 20, 40 e 60 cm com cinco repetições. Os resultados encontrados demonstraram diferenças significativas apenas para P, K e T no perfil do solo. Para todas as características na profundidade de 60 cm, os respectivos níveis de concentração estiveram bastante próximos aos níveis iniciais,...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Poluição; Lixiviação; Meio ambiente.
Ano: 2010
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S1415-43662010000700002

Tratamento de efluente de refinaria de óleo de soja por sistema de flotação por ar dissolvido
Provedor de dados: 91
Autores: Cecchet,Juliana; Gomes,Benedito M.; Costanzi,Ricardo N.; Gomes,Simone D.
Propôs-se, neste trabalho, avaliar o desempenho de coagulantes combinados a três tipos de polieletrólitos (aniônico, catiônico e não iônico), através de Flotação por Ar Dissolvido (FAD), no tratamento de efluentes de refinaria de óleo de soja. O experimento, conduzido em escala de laboratório, ensejou não apenas encontrar, pelos diagramas de coagulação, a melhor faixa de pH e a melhor concentração de coagulante mas, também, as dosagens e os tipos de floculante, culminando em sua dosagem ótima. Para tanto, parâmetros, como tempo e gradiente de mistura rápida (1 min / 150 s-1), tempo e gradiente de mistura lenta (10 min / 40 s-1 - 5 min / 20 s-1), pressão na câmara de saturação (450 kPa) e velocidade ascensional (1,67 cm min-1) foram usados para a fase da...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Coagulação; Floculação; FAD; Polieletrólito.
Ano: 2010
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S1415-43662010000100011

Uso de manipueira no desenvolvimento vegetativo do milho em ambiente protegido
Provedor de dados: 91
Autores: Saraiva,Fernanda Z.; Sampaio,Silvio C.; Silvestre,Marciane G.; Queiroz,Manoel M. F. de; Nóbrega,Lúcia H. P.; Gomes,Benedito M.
Avaliaram-se efeitos da água residuária de fecularia tratada por sistema de lagoas, na cultura do milho. A irrigação com água residuária propiciou aumento de todos os parâmetros químicos do solo, proporcional aos respectivos tratamentos como segue: L1E (efluente da lagoa de decantação), L1ED (efluente da lagoa de decantação diluído em 50%), L2E (efluente da primeira lagoa anaeróbia), L2ED (efluente da primeira lagoa anaeróbia diluído em 50%), L3E (efluente da segunda lagoa anaeróbia), L3ED (efluente da segunda lagoa anaeróbia diluído em 50%) e T (testemunha sem adubação, irrigação com água) exceto para o tratamento TA (testemunha com adubação 85 kg ha-1 K2O; 60 kg ha-1 N; 100 kg ha-1 P2O5 e irrigação com água) que também mostrou altos teores dos elementos...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Água residuária; Fecularia; Reúso; Zea mays L.
Ano: 2007
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S1415-43662007000100004

Equação de Hazen-Williams corrigida para água residuária proveniente da suinocultura
Provedor de dados: 91
Autores: Sampaio,Silvio C.; Cilene,Kátia; Boas,Márcio A. Vilas; Queiroz,Manoel M. F. de; Gomes,Benedito M.; Fazolo,Ajadir.
O objetivo do trabalho foi avaliar a perda de carga em tubulações comerciais de aço zincado, ferro galvanizado e PVC, com diferentes diâmetros, com o intuito de determinar fatores de correção para a equação de Hazen-Williams em função da concentração de sólidos totais, em águas residuárias oriundas da suinocultura. Os resultados mostraram que a perda de carga possui comportamento linear em função da concentração de sólidos totais da água residuária proveniente da suinocultura; as perdas de carga determinadas a partir dos fatores de correção parcial e global, apresentaram superestimativa e subestimativa média de 0,7 e 13%, respectivamente.
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Reúso de água; Irrigação; Hidráulica.
Ano: 2007
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S1415-43662007000100001