Consulta: creatorFacets:"Leão,Tairone Paiva"
Registros recuperados: 10
Data/hora: 10/06/2024 00:54:38

Estimativa da capacidade de suporte de carga do solo a partir da avaliação da resistência à penetração
Provedor de dados: 90
Autores: Lima,Claudia Liane Rodrigues de; Silva,Alvaro Pires da; Imhoff,Silvia; Leão,Tairone Paiva.
A pressão de preconsolidação, apesar das dificuldades inerentes à sua obtenção, representa uma medida útil do estado mecânico do solo para o seu uso, manejo e planejamento de sistemas de mecanização. A estimativa da pressão de preconsolidação, a partir de propriedades do solo facilmente mensuráveis, é, portanto, uma alternativa que pode ser utilizada para contornar as dificuldades. Os objetivos deste trabalho foram: (a) quantificar a pressão de preconsolidação e a resistência do solo à penetração, em laboratório e em campo, para um Latossolo Vermelho-Amarelo, sob pomar de laranja, e (b) estabelecer a relação entre ambos os indicadores físicos. A amostragem e as avaliações foram realizadas em oito dias consecutivos, acompanhando o secamento natural do solo....
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Pomar de laranja; Pressão de preconsolidação; Latossolo Vermelho-Amarelo.
Ano: 2006
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-06832006000200003

Tráfego de máquinas agrícolas e alterações de bioporos em área sob pomar de laranja
Provedor de dados: 90
Autores: Lima,Herdjania Veras de; Lima,Cláudia Liane Rodrigues de; Leão,Tairone Paiva; Cooper,Miguel; Silva,Alvaro Pires da; Romero,Ricardo Espíndola.
O estudo micromorfológico permite observar detalhadamente todas as modificações causadas na estrutura e no espaço poroso do solo, impostas pelo cultivo e pelo tráfego de máquinas agrícolas. Este trabalho testou a hipótese de que a compactação causada pelo tráfego de máquinas influi, diferencialmente, na forma e na distribuição das classes de poros, os quais podem ser utilizados como indicadores da qualidade do solo. O objetivo deste trabalho foi avaliar e quantificar, por meio de estudos micromorfológicos, as modificações na porosidade oriunda da atividade biológica (bioporos) em um Latossolo Vermelho-Amarelo sob pomar de laranja submetido ao tráfego de máquinas. Amostras indeformadas foram coletadas na superfície (0-12 cm) de uma área sob pomar de...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Latossolo Vermelho-Amarelo; Micromorfologia; Compactação do solo; Distribuição do espaço poroso.
Ano: 2005
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-06832005000500003

Determinação da permeabilidade ao ar em amostras indeformadas de solo pelo método da pressão decrescente
Provedor de dados: 90
Autores: Silva,Álvaro Pires da; Leão,Tairone Paiva; Tormena,Cássio Antonio; Gonçalves,Antonio Carlos Andrade.
A permeabilidade do solo ao ar (Ka) determina o fluxo convectivo de gases na matriz do solo e a troca de gases na interface do sistema solo-atmosfera, influenciando diretamente a qualidade do ambiente físico para o crescimento de plantas e a taxa de ocorrência de processos dependentes da concentração de gases no solo. A Ka pode ser estimada por um método simplificado baseado em uma modificação da lei de Darcy para fluxo de gases no solo em pressão decrescente. Os objetivos deste trabalho foram modificar e aprimorar um permeâmetro para quantificar, em laboratório, a permeabilidade de amostras indeformadas de solos ao ar utilizando o método da pressão decrescente. Foram utilizados dois sistemas de aquisição de dados: um sistema eletrônico automatizado...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Aeração; Densidade do solo; Umidade do solo; Funcionalidade do solo; Processos do solo.
Ano: 2009
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-06832009000600003

Organic matter quality and dynamics in tropical soils amended with sugar industry residue
Provedor de dados: 90
Autores: Busato,Jader Galba; Leão,Tairone Paiva; Baldotto,Marihus Altoé; Canellas,Luciano Pasqualoto.
Soil organic matter depletion caused by agricultural management systems have been identified as a critical problem in most tropical soils. The application of organic residues from agro-industrial activities can ameliorate this problem by increasing soil organic matter quality and quantity. Humic substances play an important role in soil conservation but the dynamics of their transformations is still poorly understood. This study evaluated the effect of compost application to two contrasting tropical soils (Inceptisol and Oxisol) for two years. Soil samples were incubated with compost consisting of sugarcane filter cake, a residue from the sugar industry, at 0, 40, 80, and 120 Mg ha-1. Filter cake compost changed the humic matter dynamics in both content...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Humic substances; Soil electrical charges; Stable carbon; Filter cake.
Ano: 2012
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-06832012000400012

Numerical modeling of the effect of variation of boundary conditions on vadose zone hydraulic properties
Provedor de dados: 90
Autores: Leão,Tairone Paiva; Gentry,Randall.
An accurate estimation of hydraulic fluxes in the vadose zone is essential for the prediction of water, nutrient and contaminant transport in natural systems. The objective of this study was to simulate the effect of variation of boundary conditions on the estimation of hydraulic properties (i.e. water content, effective unsaturated hydraulic conductivity and hydraulic flux) in a one-dimensional unsaturated flow model domain. Unsaturated one-dimensional vertical water flow was simulated in a pure phase clay loam profile and in clay loam interlayered with silt loam distributed according to the third iteration of the Cantor Bar fractal object Simulations were performed using the numerical model Hydrus 1D. The upper and lower pressure heads were varied around...
Tipo: Info:eu-repo/semantics/report
Palavras-chave: Numerical model; Hydrus 1D; Uncertainty; Boundary conditions; Hydraulic conductivity; Soil physics.
Ano: 2011
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-06832011000100025

Modeling water movement in horizontal columns using fractal theory
Provedor de dados: 90
Autores: Leão,Tairone Paiva; Perfect,Edmund.
Fractal mathematics has been used to characterize water and solute transport in porous media and also to characterize and simulate porous media properties. The objective of this study was to evaluate the correlation between the soil infiltration parameters sorptivity (S) and time exponent (n) and the parameters dimension (D) and the Hurst exponent (H). For this purpose, ten horizontal columns with pure (either clay or loam) and heterogeneous porous media (clay and loam distributed in layers in the column) were simulated following the distribution of a deterministic Cantor Bar with fractal dimension H" 0.63. Horizontal water infiltration experiments were then simulated using Hydrus 2D software. The sorptivity (S) and time exponent (n) parameters of the...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Numerical modeling; Hydrus 2D; Fractal model; Cantor bar; Sorptivity; Soil physics.
Ano: 2010
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-06832010000400042

Análise de formulações NPK fiscalizadas pelo mapa, de 2008 a 2010
Provedor de dados: 90
Autores: Sena,Mariana Coelho de; Leão,Tairone Paiva; von Borries,George Freitas; Turnes,Osiris.
O Brasil ocupa o quarto lugar mundial em consumo de fertilizantes; dentre esses, destaca-se o fertilizante mineral misto como o mais consumido no País. Depois da atualização da legislação brasileira de fertilizantes em 2004, muitos produtores desses insumos afirmam que houve aumento excessivo no rigor da legislação em relação à fiscalização dos teores de nutrientes neles contidos. Dentro desse contexto, os objetivos deste trabalho foram aplicar técnicas de análise estatística exploratória e descritiva e de regressão logística aos dados de análises fiscais de fertilizantes realizadas pelo Ministério da Agricultura, Pecuária e Abastecimento (MAPA), nos anos de 2008 a 2010, buscando indicadores da contribuição das fontes de variação referentes aos fatores...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Fertilizante mineral misto; Regressão logística; Legislação.
Ano: 2014
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-06832014000400017

A simplified Excel® algorithm for estimating the least limiting water range of soils
Provedor de dados: 63
Autores: Leão,Tairone Paiva; Silva,Alvaro Pires da.
The least limiting water range (LLWR) of soils has been employed as a methodological approach for evaluation of soil physical quality in different agricultural systems, including forestry, grasslands and major crops. However, the absence of a simplified methodology for the quantification of LLWR has hampered the popularization of its use among researchers and soil managers. Taking this into account this work has the objective of proposing and describing a simplified algorithm developed in Excel® software for quantification of the LLWR, including the calculation of the critical bulk density, at which the LLWR becomes zero. Despite the simplicity of the procedures and numerical techniques of optimization used, the nonlinear regression produced reliable...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Nonlinear regression; Spreadsheet software; Optimization; Soil physics; Soil quality.
Ano: 2004
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0103-90162004000600013

Water retention and penetration resistance equations for the least limiting water range
Provedor de dados: 63
Autores: Leão,Tairone Paiva.
ABSTRACT: The least limiting water range is a soil physical quality indicator, which is useful to predict the optimum water range for plant growth in a given soil and to study the effects of soil use and management over this optimum water range by integrating the effects of available water, penetration resistance and air filled porosity. This study tested six equations to fit water retention and penetration resistance surface responses used to determine the least limiting water range and present a simple algorithm written in the open source software R for fitting, calculation and visualization of the least limiting water range. Five soils from Brazil and Canada, under different use and management conditions were used to test the functions. The results show...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Nonlinear regression; Soil physical quality.
Ano: 2019
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0103-90162019001200172

A statistical basis for selecting parameters for the evaluation of soil penetration resistance
Provedor de dados: 63
Autores: Leão,Tairone Paiva; Silva,Álvaro Pires da.
Measurements of soil penetration resistance (SR) have been frequently used for the evaluation of soil structural quality for plant growth. However, different data analysis approaches have been used, without a previous evaluation of their statistical quality. In this study we tested the hypothesis that the mean is the parameter with best statistical properties to evaluate alterations in soil penetration resistance in response to soil use and management, as compared to other SR statistical parameters. Undisturbed (5 × 5 cm) soil cores were collected from three sampling sites with different degrees of compaction: an undisturbed site under native scierophylous forest (NC); a site under short-duration grazing with post-grazing residue maintained at 2.0 to 2.5...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: LSD; Probit analysis; Means comparison test; Soil physical quality assessment.
Ano: 2006
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0103-90162006000600007