Consulta: creatorFacets:"Linke, P"
Registros recuperados: 1
Data/hora: 02/06/2024 00:45:14

Intercalibration of benthic flux chambers II. Hydrodynamic characterization and flux comparisons of 14 different designs
Provedor de dados: 5
Autores: Tengberg, Anders; Hall, P; Andersson, U; Linden, B; Styrenius, O; Boland, G; De Bovee, F; Carlsson, B; Ceradini, S; Devol, A; Duineveld, G; Friemann, J; Glud, R; Khripounoff, Alexis; Leather, J; Linke, P; Lund Hansen, L; Rowe, G; Santschi, P; De Wilde, P; Witte, U.
We have compared 14 different sediment incubation chambers, most of them were used on bottom landers. Measurements of mixing time, pressure gradients at the bottom and Diffusive Boundary Layer thickness (DBL) were used to describe the hydrodynamic properties of the chambers and sediment-water solute fluxes of silicate (34 replicates) and oxygen (23 replicates) during three subsequently repeated incubation experiments on a homogenized, macrofauna-free sediment. The silicate fluxes ranged from 0.24 to 1.01 mmol m(-2) day(-1) and the oxygen fluxes from 9.3 to 22.6 mmol m(-2) day(-1). There was no statistically significant correlation between measured fluxes and the chamber design or between measured fluxes and hydrodynamic settings suggesting that type of...
Tipo: Text
Palavras-chave: Comparative flux incubations; Hydrodynamic properties; Calibration; Benthic chambers.
Ano: 2005
URL: http://archimer.ifremer.fr/doc/2005/publication-750.pdf