Consulta: creatorFacets:"Magalhães,Paulo Sérgio Graziano"
Registros recuperados: 7
Data/hora: 13/06/2024 23:31:19

Correlation of physical and chemical attributes of soil with sugarcane yield
Provedor de dados: 86
Autores: Cerri,Domingos Guilherme Pellegrino; Magalhães,Paulo Sérgio Graziano.
The objective of this work was to evaluate the correlation between sugarcane yield and some physical and chemical attributes of soil. For this, a 42‑ha test area in Araras, SP, Brazil, was used. Soil properties were determined from samples collected at the beginning of the 2003/2004 harvest season, using a regular 100x100 m grid. Yield assessment was done with a yield monitor (Simprocana). Correlation analyses were performed between sugarcane yield and the following soil properties: pH, pH CaCl2, N, C, cone index, clay content, soil organic matter, P, K, Ca, Mg, H+AL, cation exchange capacity, and base saturation. Correlation coefficients were respectively ‑0.05, ‑0.29, 0.33, 0.41, ‑0.27, 0.22, 0.44, ‑0.24, trace, ‑0.06, 0.01, 0.32, 0.14, and 0.04....
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Saccharum officinarum; Precision agriculture; Soil sampling; Spatial variation; Variation structure.
Ano: 2012
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0100-204X2012000400018

Computational system for geostatistical analysis
Provedor de dados: 63
Autores: Vendrusculo,Laurimar Gonçalves; Magalhães,Paulo Sérgio Graziano; Vieira,Sidney Rosa; Carvalho,José Ruy Porto de.
Geostatistics identifies the spatial structure of variables representing several phenomena and its use is becoming more intense in agricultural activities. This paper describes a computer program, based on Windows Interfaces (Borland Delphi), which performs spatial analyses of datasets through geostatistic tools: Classical statistical calculations, average, cross- and directional semivariograms, simple kriging estimates and jackknifing calculations. A published dataset of soil Carbon and Nitrogen was used to validate the system. The system was useful for the geostatistical analysis process, for the manipulation of the computational routines in a MS-DOS environment. The Windows development approach allowed the user to model the semivariogram graphically...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Spatial variability; Semivariogram; Software.
Ano: 2004
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0103-90162004000100017

Precision production environments for sugarcane fields
Provedor de dados: 63
Autores: Sanches,Guilherme Martineli; Paula,Maria Thereza Nonato de; Magalhães,Paulo Sérgio Graziano; Duft,Daniel Garbellini; Vitti,André César; Kolln,Oriel Tiago; Borges,Bernardo Melo Montes Nogueira; Franco,Henrique Coutinho Junqueira.
ABSTRACT: Sugarcane (saccharum spp.) in Brazil is managed on the basis of “production environments”. These “production environments” are used for many purposes, such as variety allocation, application of fertilizers and definition of the planting and harvesting periods. A quality classification is essential to ensure high economic returns. However, the classification is carried out by few and, most of the time, non-representative soil samples, showing unreal local conditions of soil spatial variability and resulting in classifications that are imprecise. One of the important tools in the precision agriculture technological package is the apparent electrical conductivity (ECa) sensors that can quickly map soil spatial variability with high-resolution and at...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Proximal soil sensors; Site-specific soil management; Soil apparent electrical conductivity; Precision agriculture technologies.
Ano: 2019
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0103-90162019000100010

How much sugarcane trash should be left on the soil?
Provedor de dados: 63
Autores: Cantarella,Heitor; Cerri,Carlos Eduardo Pellegrino; Carvalho,João Luís Nunes; Magalhães,Paulo Sérgio Graziano.
Tipo: Info:eu-repo/semantics/other
Ano: 2013
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0103-90162013000500001

Assessment of sugarcane trash for agronomic and energy purposes in Brazil
Provedor de dados: 63
Autores: Franco,Henrique Coutinho Junqueira; Pimenta,Maria Teresa Borges; Carvalho,João Luís Nunes; Magalhães,Paulo Sérgio Graziano; Rossell,Carlos Eduardo Vaz; Braunbeck,Oscar Antonio; Vitti,André Cesar; Kölln,Oriel Tiago; Rossi Neto,João.
Due to new possibilities for using sugarcane (Saccharum spp.) trash for electricity generation, and the production of 2nd generation ethanol and others chemicals, the interest for its recovery has increased. However, the question of how much trash can be removed from sugarcane field still needs to be clarified. This study evaluated the amount of dry matter, nutrients content, structural compounds and efficiency of the enzymatic hydrolysis of the hydrothermal pretreated materials for tops and dry leaves in samples from sugarcane varieties. Tops and dry leaves present differences in nutrients content and moisture. Therefore, the amount of trash to be collected should not be simply based on percentages, but also should take into account the different...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Saccharum spp.; Enzymatic hydrolysis; Sugarcane crop residues.
Ano: 2013
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0103-90162013000500004

Desempenho operacional de um arado de discos
Provedor de dados: 53
Autores: Mello,Roberto da Cunha; Magalhães,Paulo Sérgio Graziano.
Desenvolveu-se este trabalho com o objetivo de avaliar o desempenho de um arado de três discos, reversível, e estabelecer uma relação em função da velocidade de deslocamento e do ângulo de ataque horizontal dos discos, caracterizados pela resistência específica e pelo consumo de combustível por volume de solo mobilizado. Os resultados mostraram que a resistência específica do solo não diferiu significativamente nem com a velocidade de deslocamento nem com o ângulo de ataque horizontal dos discos. O consumo de combustível variou com a velocidade, mas não em relação ao ângulo de ataque horizontal dos discos. Os valores da resistência específica variaram na faixa de 6,37 a 7,22 N/cm², em média, enquanto o consumo de combustível por volume de solo mobilizado...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Arado; Ensaio de desempenho; Resistência específica do solo.
Ano: 1995
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0006-87051995000200024

Análise dos atributos do solo e da produtividade da cultura de cana-de-açúcar com o uso da geoestatística e árvore de decisão
Provedor de dados: 65
Autores: Souza,Zigomar Menezes de; Cerri,Domingos Guilherme Pellegrino; Colet,Marcelo José; Rodrigues,Luiz Henrique Antunes; Magalhães,Paulo Sérgio Graziano; Mandoni,Rafael Junqueira Araújo.
Um dos desafios da agricultura de precisão é oferecer subsídios para a definição de unidades de manejo para posteriores intervenções. Portanto, o objetivo deste trabalho foi avaliar os atributos químicos do solo e a produtividade da cultura de cana-de-açúcar por meio da geoestatística e mineração de dados pela indução da árvore de decisão. A produtividade da cana-de-açúcar foi mapeada em uma área de aproximadamente 23ha, utilizando-se o critério de célula, por meio de um monitor de produtividade que permitiu a elaboração de um mapa digital que representa a superfície de produção para a área em estudo. Para determinar os atributos de um Argissolo Vermelho-Amarelo, foram coletadas as amostras no início da safra 2006/2007, utilizando-se uma grade regular de...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Agricultura de precisão; Variabilidade espacial; Mineração de dados; Monitor de produtividade.
Ano: 2010
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S0103-84782010000400015