Consulta: creatorFacets:"Mantai,Rubia D."
Registros recuperados: 8
Data/hora: 02/06/2024 05:36:24

Nitrogen efficiency in oat yield through the biopolymer hydrogel
Provedor de dados: Revista Brasileira de Engenharia Agrícola e Ambiental
Autores: Scremin,Osmar B.; Silva,José A. G. da; Mamann,Ângela T. W. de; Mantai,Rubia D.; Brezolin,Ana P.; Marolli,Anderson.
ABSTRACT The retainers of water in the soil can favor nitrogen (N) use efficiency in oat yield. The aim of the study was to determine if the conditions of use of the biopolymer hydrogel increase the fertilizer-N use efficiency in oat yield in succession systems of high and low residual-N release. In each succession system (soybean/oat, corn/oat), two experiments were conducted in 2014 and 2015, one to quantify biomass yield and the other to estimate grain yield and lodging. The design was randomized blocks with four replicates in a 4 x 4 factorial scheme for hydrogel doses (0, 30, 60 and 120 kg ha-1), added in the furrow with the seed, and N fertilizer doses (0, 30, 60 and 120 kg ha-1) applied in the fourth-expanded-leaf stage. The use of hydrogel...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Avena sativa L.; Biodegradable; C/N ratio; Lodging; Biomass.
Ano: 2017
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S1415-43662017000600379

A eficiência na produção de biomassa e grãos de aveia pelo uso do nitrogênio
Provedor de dados: Revista Brasileira de Engenharia Agrícola e Ambiental
Autores: Mantai,Rubia D.; Silva,José A. G. da; Sausen,Airam T. Z. R.; Costa,Juliane S. P.; Fernandes,Sandra B. V.; Ubessi,Cassiane.
A produção de biomassa e grãos de aveia depende diretamente das formas de fornecimento de nitrogênio (N). Propôs-se, com este estudo, determinar a eficiência de aproveitamento de N-fertilizante na elaboração de biomassa e grãos de aveia em distintos sistemas de cultivo e estimar a máxima eficiência técnica e econômica de produtividade de grãos na identificação de cultivares mais eficientes no uso do N. O estudo foi conduzido nos anos de 2011 e 2012, em delineamento experimental de blocos casualizados com quatro repetições em esquema fatorial 4 x 2 para Doses de Nitrogênio (0, 30, 60 e 120 kg ha-1) e Cultivares de Aveia (Barbarasul e Brisasul) no sistema soja/aveia e milho/aveia. Há tendência de crescimento na taxa de biomassa em aveia com o incremento das...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Avena sativa L.; Ureia; Razão C/N; Eficiência técnica e econômica.
Ano: 2015
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S1415-43662015000400343

Single and split nitrogen dose in wheat yield indicators
Provedor de dados: Revista Brasileira de Engenharia Agrícola e Ambiental
Autores: Costa,Juliane S. P.; Mantai,Rubia D.; Silva,José A. G. da; Scremin,Osmar B.; Arenhardt,Emilio G.; Lima,Andressa R. C. de.
ABSTRACT Single or split nitrogen (N) supply can maximize the expression of wheat yield indicators. The objective of the study was to evaluate the greater N use efficiency on wheat yield indicators by the single and split N supply under favorable and unfavorable year conditions to the crop in succession system of high and reduced residual N release. The study was conducted in 2014 and 2015, in a randomized complete block design with four replicates in a 4 x 3 factorial, for N-fertilizer doses (0, 30, 60, 120 kg ha-1) and supply forms [full dose (100%) in the phenological stage V3 (third expanded leaf); split dose (70 and 30%) in the phenological stages V3/V6 (third and sixth expanded leaves, respectively) and; split dose (70 and 30%) in the phenological...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Triticum aestivum; Urea; Residual N; Temperature; Rainfall.
Ano: 2018
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S1415-43662018000100016

Nitrogen efficiency in wheat yield through the biopolymer hydrogel
Provedor de dados: Revista Brasileira de Engenharia Agrícola e Ambiental
Autores: Mamann,Ângela T. W De; Silva,José A. G. da; Scremin,Osmar B.; Mantai,Rubia D.; Scremin,Ari H.; Dornelles,Eldair F.
ABSTRACT Nitrogen use efficiency in wheat biomass and grain yields can be favored by the biopolymer hydrogel. The objective of the study was to analyze the use of the biopolymer hydrogel applied to the seed in the optimization of fertilizer-N on wheat biomass and grain yields, under different conditions of agricultural year and succession systems of high and reduced release of residual-N. In the study, two experiments were conducted, with different farming systems, soybean/wheat and maize/wheat, one to quantify the biomass yield rate and the other to determine grain yield. The experiments were conducted in the years 2014 and 2015, in a randomized block design with four replicates in a 4 x 4 factorial scheme, corresponding to hydrogel doses (0, 30, 60 and...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Triticum aestivum; Simulation; Farming systems; Water stress.
Ano: 2017
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S1415-43662017001000697

Biomass and grain yield of oats by growth regulator
Provedor de dados: Revista Brasileira de Engenharia Agrícola e Ambiental
Autores: Marolli,Anderson; Silva,José A. G. da; Romitti,Marcos V.; Mantai,Rubia D.; Hawerroth,Maraisa C.; Scremin,Osmar B.
ABSTRACT The use of growth regulator in oats can reduce plant lodging with reflections in biomass and grain yield. The objective of the study was to determine the feasibility and efficiency of using Trinexapac-Ethyl regulator in the growth of white oat under different conditions of N-fertilizer and years favorable and unfavorable for cultivation. In this study, two experiments were conducted in the years 2011, 2012 and 2013, one for quantifying biomass production rate and the other for the determination of grain yield and lodging. The experimental design was randomized blocks with four replicates, in a 4 x 3 factorial scheme, for growth regulator doses (0, 200, 400 and 600 mL ha-1) and nitrogen doses (30, 90 and 150 kg ha-1), respectively. There is a...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Avena sativa; Trinexapac-ethyl; Lodging; Nitrogen; Regression.
Ano: 2017
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S1415-43662017000300163

Oat yield through panicle components and growth regulator
Provedor de dados: Revista Brasileira de Engenharia Agrícola e Ambiental
Autores: Marolli,Anderson; Silva,José A. G. da; Mantai,Rubia D.; Brezolin,Ana P.; Gzergorczick,Maria E.; Lambrecht,Darlei M.
ABSTRACT The growth regulator modifies the expression of lodging and panicle components in oat plants, with reflexes in yield. The objective of this study was to define the optimal dose of growth regulator in oat for a maximum lodging of 5%. In addition, this study aimed to identify potential variables of the panicle to compose the multiple linear regression model and the simulation of grain yield in conditions of use of the regulator under low, high and very high fertilization with nitrogen. The study was conducted in 2011, 2012 and 2013 in a randomized block design with four replicates in a 4 x 3 factorial scheme, for growth regulator doses (0, 200, 400 and 600 mL ha-1) and N-fertilizer doses (30, 90 and 150 kg ha-1), respectively. The growth regulator...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Avena sativa; Nitrogen; Trinexapac-ethyl; Multiple linear regression.
Ano: 2017
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S1415-43662017000400261

Simulation of oat development cycle by photoperiod and temperature
Provedor de dados: Revista Brasileira de Engenharia Agrícola e Ambiental
Autores: Mantai,Rubia D.; Silva,José A. G. da; Marolli,Anderson; Mamann,Ângela T. W. de; Sawicki,Sandro; Krüger,Cleusa A. M. B.
ABSTRACT The simulation of oat development cycle can be used in the planning of agricultural practices. The aim of the study was to simulate and validate the duration of oat development cycle by photoperiod, temperature and coefficients of development of wheat for use in the WE-Streck model, considering different doses of N-fertilizer and systems of succession of high and low C/N ratio. The study was conducted in 2015 in a randomized block design with four replicates in a 4 x 2 factorial scheme, corresponding to N rates (0, 30, 60 and 120 kg ha-1) and oat cultivars (Barbarasul and Brisasul), respectively, in the soybean/oat and maize/oat systems. The duration of the stages from emergence to anthesis and from anthesis to maturation of oats was simulated in...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Avena sativat; Succession system; Nitrogen; WE-Streck model.
Ano: 2017
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S1415-43662017000100003

Nitrogen efficiency in oats on grain yield with stability
Provedor de dados: Revista Brasileira de Engenharia Agrícola e Ambiental
Autores: Silva,José A. G. da; Goi Neto,Constantino J.; Fernandes,Sandra B. V.; Mantai,Rubia D.; Scremin,Osmar B.; Pretto,Rafael.
ABSTRACT Nitrogen (N) is the nutrient most absorbed by the oat crop. Unfavorable climate conditions decrease its efficiency, generating instability and reduction in yield. The objective of this study was to improve N use efficiency in oat grain yield by the economic value of the product and of the input and by models that scale the stability, considering systems of succession of high and reduced residual-N release in favorable and unfavorable years for cultivation. The study was conducted in the years 2013, 2014 and 2015 in two systems of succession (soybean/oat, maize/oat) in randomized blocks with eight replicates, using the N-fertilizer doses of 0, 30, 60 and 120 kg ha-1. The N-fertilizer dose for maximum economic efficiency in oats should be considered...
Tipo: Info:eu-repo/semantics/article
Palavras-chave: Avena Sativa; C/N; Predictability; Biometric models; Optimization.
Ano: 2016
URL: http://www.scielo.br/scielo.php?script=sci_arttext&pid=S1415-43662016001201095